(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 16)
    (no_connects 0)
    (area 143.724999 100.224999 155.275001 112.775001)
    (thickness 1.6)
    (drawings 56)
    (tracks 21)
    (zones 0)
    (modules 18)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.153)
    (user_trace_width 0.28)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.37)
    (user_trace_width 0.4)
    (user_trace_width 0.46)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.153)
    (segment_width 0.1)
    (edge_width 0.05)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.75 0.4)
    (user_via 0.84 0.49)
    (user_via 0.95 0.5)
    (uvia_size 0.45)
    (uvia_drill 0.3)
    (uvias_allowed yes)
    (uvia_min_size 0.45)
    (uvia_min_drill 0.3)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/Denise/Desktop/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P1-Pad1)")
  (net 3 "Net-(P10-Pad1)")
  (net 4 "Net-(P11-Pad1)")
  (net 5 "Net-(P12-Pad1)")
  (net 6 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.153)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.45)
    (uvia_drill 0.3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P12-Pad1)")
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A81DF9E)
    (at 149 106.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.5) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(P10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A81DF96)
    (at 149 109)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2A0)
    (at 149 111.5)
    (attr virtual)
    (fp_text reference GND1 (at 0 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E304)
    (at 152.5 109)
    (attr virtual)
    (fp_text reference P1 (at 1.5 -2.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(P1-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E363)
    (at 152.5 106.5)
    (attr virtual)
    (fp_text reference P2 (at -0.5 -0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(P10-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E31D)
    (at 152.5 104)
    (attr virtual)
    (fp_text reference P3 (at 1.5 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(P11-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E34C)
    (at 152.5 101.5)
    (attr virtual)
    (fp_text reference P4 (at -0.5 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(P12-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2DA)
    (at 145.5 101.5)
    (attr virtual)
    (fp_text reference P5 (at 0 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 6 +5V))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2D6)
    (at 145.5 104)
    (attr virtual)
    (fp_text reference P6 (at -0.5 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 6 +5V))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2DF)
    (at 145.5 106.5)
    (attr virtual)
    (fp_text reference P7 (at -0.5 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 6 +5V))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2E3)
    (at 145.5 109)
    (attr virtual)
    (fp_text reference P8 (at -0.5 -0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 6 +5V))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E35D)
    (at 154 109)
    (attr virtual)
    (fp_text reference P9 (at 0.5 -0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(P1-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E356)
    (at 154 106.5)
    (attr virtual)
    (fp_text reference P10 (at -0.5 0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(P10-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E346)
    (at 154 104)
    (attr virtual)
    (fp_text reference P11 (at 0.5 -0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(P11-Pad1)"))
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E339)
    (at 154 101.5)
    (attr virtual)
    (fp_text reference P12 (at 0.5 -0.5) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(P12-Pad1)"))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A81DF80)
    (at 149 104)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 0 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.75) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(P11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5A81DF90)
    (at 149 101.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 8.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(P12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cmon:1.4_0.9_S (layer F.Cu) (tedit 5A81E2E9)
    (at 145.5 111.5)
    (attr virtual)
    (fp_text reference VCC1 (at -0.5 0.5 90) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -0.5) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Paste *.Mask)
      (net 6 +5V))
  )
  (gr_text MCU (at 154 111.25) (layer F.SilkS))
  (gr_text SW4 (at 149.25 101.5) (layer F.SilkS))
  (gr_text SW3 (at 149.25 104) (layer F.SilkS))
  (gr_text SW2 (at 149.25 106.5) (layer F.SilkS))
  (gr_text SW1 (at 149.25 109) (layer F.SilkS))
  (gr_text GND (at 151 111.5) (layer F.SilkS))
  (gr_text 5V (at 147 111.75) (layer F.SilkS))
  (gr_text "LimitSW\nv0.1" (at 152.5 111.25) (layer B.SilkS))
  (gr_line (start 155.25 112.75) (end 155.25 100.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.75 112.75) (end 155.25 112.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.75 100.25) (end 143.75 112.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 146.5 100.25) (end 143.75 100.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.25 100.25) (end 146.5 100.25) (angle 90) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 146.5 110.5) (xy 146.5 112) (xy 146.5 112.5) (xy 144 112.5) (xy 144 100.5)
        (xy 146.5 100.5)
      )
    )
  )
  (zone (net 2) (net_name "Net-(P1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 155 110) (xy 151.5 110) (xy 151.5 108) (xy 155 108)
      )
    )
  )
  (zone (net 3) (net_name "Net-(P10-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 155 107.5) (xy 151.5 107.5) (xy 151.5 105.5) (xy 155 105.5)
      )
    )
  )
  (zone (net 4) (net_name "Net-(P11-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 155 105) (xy 151.5 105) (xy 151.5 103) (xy 155 103)
      )
    )
  )
  (zone (net 5) (net_name "Net-(P12-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 155 102.5) (xy 151.5 102.5) (xy 151.5 100.5) (xy 155 100.5)
      )
    )
  )
)
