(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 50)
    (no_connects 1)
    (area 125.649999 80.049999 147.750001 97.150001)
    (thickness 1.6)
    (drawings 11)
    (tracks 87)
    (zones 0)
    (modules 23)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.17)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GNDREF)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(Q1-Pad3)")
  (net 7 "Net-(Q1-Pad2)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(R2-Pad1)")
  (net 10 "Net-(R3-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(Q1-Pad1)")
  (net 14 "Net-(C5-Pad2)")
  (net 15 "Net-(C7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDREF)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R6-Pad2)")
  )
  (module "Custom Parts:SOD-123W" (layer F.Cu) (tedit 5A6CE79A)
    (at 146 85.4 270)
    (fp_text reference D1 (at 0 1.9 270) (layer F.SilkS))
    (fp_text value D_RECT (at 0 -1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1.55 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.55 0 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
  )
  (module "Custom Parts:Wurth_WE-FB_10.18x13.36mm" (layer F.Cu) (tedit 5A91E72C)
    (at 140 91.5 180)
    (fp_text reference T1 (at 0 0 180) (layer F.SilkS))
    (fp_text value Wurth_Transformer_10.16x13.36mm (at 0 -6.1 180) (layer F.Fab))
    (pad 1 smd rect (at -5.83 2.5 180) (size 2.08 1.17) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at -5.83 0 180) (size 2.08 1.17) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.83 -2.5 180) (size 2.08 1.17) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 4 smd rect (at 5.83 -2.5 180) (size 2.08 1.17) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 6 smd rect (at 5.83 2.5 180) (size 2.08 1.17) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 5 smd rect (at 5.83 0 180) (size 1.1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 131.8 93.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value R_GATE (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-12-1EP_3x4mm_Pitch0.65mm (layer F.Cu) (tedit 57AFAE52)
    (at 130.3 90.6)
    (descr "MSE Package; 12-Lead Plastic MSOP, Exposed Die Pad; (see Linear Technology 05081666_G_MSE12.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.05) (layer F.SilkS))
    (fp_text value LTC3759 (at 0 3.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.105 -1.625) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at -2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at -2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 6 smd rect (at -2.105 1.625) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 7 smd rect (at 2.105 1.625) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad3)"))
    (pad 8 smd rect (at 2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 9 smd rect (at 2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (pad 10 smd rect (at 2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 11 smd rect (at 2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 12 smd rect (at 2.105 -1.625) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 13 smd rect (at 0.4125 1.06875) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.4125 0.35625) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.4125 -0.35625) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at 0.4125 -1.06875) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.4125 1.06875) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.4125 0.35625) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.4125 -0.35625) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (pad 13 smd rect (at -0.4125 -1.06875) (size 0.825 0.7125) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-12-1EP_3x4mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 127 86.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value R_FB (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 129.2 93.8)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value R_SENSE (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 127 88.55 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value R_BIAS (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 129 87.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45) (layer F.SilkS))
    (fp_text value R_VC (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 127 93.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R_FREQ (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 129.1 85.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value C_VC (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 132.4 87.45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value C (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 127 91 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value C_SS (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Custom Parts:EPC2016C" (layer F.Cu) (tedit 5A8E6323)
    (at 131.8 95.6 270)
    (fp_text reference Q1 (at 0 1.8 270) (layer F.SilkS))
    (fp_text value Q_SWITCH (at 0 -1.7 270) (layer F.Fab))
    (pad 3 smd oval (at 0 0 270) (size 0.18 1.362) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad3)") (solder_paste_margin -0.05))
    (pad 1 smd oval (at 0.4 0 270) (size 0.18 1.362) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)") (solder_paste_margin -0.05))
    (pad 3 smd oval (at 0.8 0 270) (size 0.18 1.362) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad3)") (solder_paste_margin -0.05))
    (pad 1 smd oval (at -0.4 0 270) (size 0.18 1.362) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)") (solder_paste_margin -0.05))
    (pad 3 smd oval (at -0.8 0.401 270) (size 0.18 0.56) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q1-Pad3)") (solder_paste_margin -0.05))
    (pad 2 smd oval (at -0.8 -0.401 270) (size 0.18 0.56) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q1-Pad2)") (solder_paste_margin -0.05))
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 131.9 84.95)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.25) (layer F.SilkS))
    (fp_text value C (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_2220 (layer F.Cu) (tedit 58AA8565)
    (at 137.7 83.1)
    (descr "Capacitor SMD 2220, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C5 (at 0 -3.5) (layer F.SilkS))
    (fp_text value C_OUT (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0 -3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.8 0) (size 1 5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 2.8 0) (size 1 5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812 (layer F.Cu) (tedit 58AA850E)
    (at 143 83.35 90)
    (descr "Capacitor SMD 1812, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C6 (at 0 -2.75 90) (layer F.SilkS))
    (fp_text value C_OUT (at 0 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.3 0 90) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 2.3 0 90) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 134.2 90.35)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5) (layer F.SilkS))
    (fp_text value C_BP (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 131.9 81.8 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C8 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value C (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDREF))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 56C360B9)
    (at 126.9 95.9)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J3 (at 0 -2) (layer F.SilkS))
    (fp_text value GND (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 56C360B9)
    (at 146.5 95.9)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J4 (at 0 -2) (layer F.SilkS))
    (fp_text value GND (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GNDREF))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 56C360B9)
    (at 146.5 81.3)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J5 (at 0 -2) (layer F.SilkS))
    (fp_text value VOUT (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C5-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 56C360B9)
    (at 126.9 81.3)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J1 (at 0 -2) (layer F.SilkS))
    (fp_text value VIN (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 56C360B9)
    (at 126.9 83.3)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference J2 (at 0 -2) (layer F.SilkS))
    (fp_text value EN (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (gr_text "LT3759 Rev.B" (at 136.6 87.4) (layer B.SilkS))
  (gr_text 0x7D.com (at 136.7 89.8) (layer B.SilkS))
  (gr_text VOUT (at 145.5 81.35) (layer B.SilkS))
  (gr_text GND (at 145.5 95.95 360) (layer B.SilkS))
  (gr_text EN (at 127.9 83.35) (layer B.SilkS))
  (gr_text GND (at 127.9 95.95) (layer B.SilkS))
  (gr_text VIN (at 127.9 81.35) (layer B.SilkS))
  (gr_line (start 125.7 97.1) (end 147.7 97.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7 80.1) (end 125.7 80.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7 97.1) (end 147.7 80.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.7 80.1) (end 125.7 97.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 125.7 80.1) (xy 125.7 97.1) (xy 147.7 97.1) (xy 147.7 80.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.5 86.3) (xy 144.5 86.3) (xy 144.5 96.7) (xy 135.5 96.7)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 131.9 90.5) (xy 133.05 90.5) (xy 133.05 89.775) (xy 135.5 89.775) (xy 135.5 85.6)
        (xy 135.5 83.05) (xy 132.9 83.05) (xy 132.9 80.55) (xy 132.3 80.55) (xy 126.15 80.55)
        (xy 126.15 82.05) (xy 128.1 82.05) (xy 128.1 83.1) (xy 131.1 83.1) (xy 131.1 83.4)
        (xy 131.1 86.5) (xy 132.4 86.5) (xy 132.4 88.7) (xy 131.9 88.7) (xy 131.9 89)
        (xy 131.9 89.3) (xy 131.9 89.4)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 139.8 85.8) (xy 141.2 85.8) (xy 141.2 82.9) (xy 144.7 82.9) (xy 144.7 88.3)
        (xy 147 88.3) (xy 147 89.7) (xy 144.5 89.7) (xy 144.5 95.15) (xy 147.25 95.15)
        (xy 147.25 96.65) (xy 144.2 96.65) (xy 144.2 86.3) (xy 135.7 86.3) (xy 135.7 85.6)
        (xy 134.4 85.6) (xy 134.4 83.05) (xy 132.9 83.05) (xy 132.9 80.55) (xy 139.8 80.55)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 140 85.6) (xy 141 85.6) (xy 141 82.7) (xy 141.5 82.7) (xy 144.5 82.7)
        (xy 145.1 82.7) (xy 145.1 84.7) (xy 147.25 84.7) (xy 147.25 84.2) (xy 147.25 80.75)
        (xy 147.25 80.55) (xy 140.15 80.55) (xy 140 80.55)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 129.9 83.6) (xy 131.3 83.6) (xy 131.3 86.5) (xy 132.4 86.5) (xy 132.4 88.55)
        (xy 131.7 88.55) (xy 131.7 92.35) (xy 129.75 92.35) (xy 129.75 92.9) (xy 129.75 96.65)
        (xy 129.1 96.65) (xy 126.15 96.65) (xy 126.15 93.25) (xy 126.6 93.25) (xy 127.35 93.25)
        (xy 127.65 93.25) (xy 127.65 92.75) (xy 127.65 92.45) (xy 127.65 92.35) (xy 127.65 92.15)
        (xy 126.55 92.15) (xy 126.55 91.35) (xy 127.55 91.35) (xy 128.9 91.35) (xy 128.9 91)
        (xy 128.9 89.5) (xy 128.9 88.25) (xy 130.05 88.25) (xy 130.05 87.1) (xy 129.7 87.1)
        (xy 129.7 85.7) (xy 128.1 85.7) (xy 128.1 85.25) (xy 128.1 83.6) (xy 129.5 83.6)
      )
    )
  )
  (zone (net 6) (net_name "Net-(Q1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 132.9 92.45) (xy 132 92.45) (xy 132 92.9) (xy 130.5 92.9) (xy 130.5 94.5)
        (xy 130.5 94.7) (xy 131.7 94.7) (xy 131.7 95.5) (xy 132.5 95.5) (xy 132.5 96.5)
        (xy 129.8 96.5) (xy 129.8 94.45) (xy 129.8 92.95) (xy 129.8 92.4) (xy 131.6 92.4)
        (xy 131.6 92) (xy 132.9 92)
      )
    )
  )
  (zone (net 7) (net_name "Net-(Q1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 130.8 93.15) (xy 130.8 94.9) (xy 132.5 94.9) (xy 132.5 93.15)
      )
    )
  )
  (zone (net 11) (net_name "Net-(R6-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 131.9 91.35) (xy 131.9 91.85) (xy 132.85 91.85) (xy 132.85 92.6) (xy 132.2 92.6)
        (xy 132.2 94.15) (xy 132.9 94.15) (xy 132.9 93.15) (xy 133.4 93.15) (xy 133.4 91.35)
      )
    )
  )
  (zone (net 15) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 131.9 91.15) (xy 133.9 91.15) (xy 133.9 89.95) (xy 133.05 89.95) (xy 131.9 89.95)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 134.5 89.95) (xy 134.5 92.1) (xy 133.7 92.1) (xy 133.7 92.7) (xy 135.525 92.7)
        (xy 135.525 89.95)
      )
    )
  )
  (zone (net 12) (net_name "Net-(D1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 144.8 94.6) (xy 147.7 94.6) (xy 147.7 86.2) (xy 145.2 86.2) (xy 145.2 87.7)
        (xy 147.1 87.7) (xy 147.1 93.1) (xy 144.8 93.1)
      )
    )
  )
  (zone (net 10) (net_name "Net-(R3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 128.7 89.85) (xy 127.35 89.85) (xy 127.35 89.65) (xy 125.95 89.65) (xy 125.95 86.75)
        (xy 127.45 86.75) (xy 127.45 87.25) (xy 126.35 87.25) (xy 126.35 89.05) (xy 128.7 89.05)
      )
    )
  )
  (zone (net 3) (net_name "Net-(C3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 130 88.05) (xy 128.7 88.05) (xy 128.7 85.9) (xy 129.5 85.9) (xy 129.5 87.15)
        (xy 130 87.15)
      )
    )
  )
  (zone (net 9) (net_name "Net-(R2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 128.7 89.2) (xy 127.75 89.2) (xy 127.75 87.15) (xy 128.7 87.15)
      )
    )
  )
  (zone (net 1) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 126.55 87.5) (xy 126.55 88.85) (xy 127.45 88.85) (xy 127.45 87.5)
      )
    )
  )
  (zone (net 4) (net_name "Net-(C4-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 128.7 90.05) (xy 128.7 90.5) (xy 127.45 90.5) (xy 127.45 90.65) (xy 126.55 90.65)
        (xy 126.55 89.85) (xy 127.45 89.85) (xy 127.45 90.05)
      )
    )
  )
  (zone (net 8) (net_name "Net-(R1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 127.45 92.95) (xy 125.95 92.95) (xy 125.95 90.85) (xy 127.6 90.85) (xy 127.6 90.7)
        (xy 128.7 90.7) (xy 128.7 91.15) (xy 127.65 91.15) (xy 126.35 91.15) (xy 126.35 92.45)
        (xy 127.45 92.45)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 126.55 85.75) (xy 127.45 85.75) (xy 127.45 84.4) (xy 126.55 84.4)
      )
    )
  )
  (zone (net 13) (net_name "Net-(Q1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.06))
    (polygon
      (pts
        (xy 133.1 93.4) (xy 133.1 95.1) (xy 131.1 95.1) (xy 131.1 96.5) (xy 135.25 96.5)
        (xy 135.25 93.4)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 131.9 89.2) (xy 132.85 89.2) (xy 132.85 88.75) (xy 132.5 88.75) (xy 132.5 86.4)
        (xy 131.35 86.4) (xy 131.35 83.275) (xy 127.5 83.275) (xy 127.5 83.475) (xy 131.15 83.475)
        (xy 131.15 86.6) (xy 132.3 86.6) (xy 132.3 88.75) (xy 131.9 88.75)
      )
    )
  )
)
