(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 18)
    (no_connects 0)
    (area 102.794999 88.824999 185.495001 109.295001)
    (thickness 1.6)
    (drawings 9)
    (tracks 73)
    (zones 0)
    (modules 12)
    (nets 13)
  )
  (page USLetter)
  (title_block
    (title "Incubator Breakout Board")
    (date 2017-11-29)
    (rev 1)
    (company "Urban Coop Company / Andy Vaselaar")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Servo_Data)
  (net 2 /DHT22_Data)
  (net 3 /Relay_4)
  (net 4 /Relay_3)
  (net 5 /Relay_2)
  (net 6 /Relay_1)
  (net 7 "Net-(P2-Pad4)")
  (net 8 "Net-(P2-Pad5)")
  (net 9 DGND)
  (net 10 +5V)
  (net 11 +3.3V)
  (net 12 "Net-(P6-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3.3V)
    (add_net +5V)
    (add_net /DHT22_Data)
    (add_net /Relay_1)
    (add_net /Relay_2)
    (add_net /Relay_3)
    (add_net /Relay_4)
    (add_net /Servo_Data)
    (add_net DGND)
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P6-Pad3)")
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A1EC892)
    (at 175.26 95.25 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P1 (at 5 -3.5 180) (layer F.SilkS))
    (fp_text value "RPI 31-39" (at 5 4.5 180) (layer F.SilkS))
    (fp_text user %R (at 5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 /DHT22_Data))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Servo_Data))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Relay_4))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Relay_3))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B05B-XH-A_05x2.50mm_Straight (layer F.Cu) (tedit 5A1ED454)
    (at 157.48 95.25 180)
    (descr "JST XH series connector, B05B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P2 (at 5 -3.5 180) (layer F.SilkS))
    (fp_text value "RPI 32-40" (at 5 4.5 180) (layer F.SilkS))
    (fp_text user %R (at 5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Relay_2))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Relay_1))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad5)"))
    (model Connectors_JST.3dshapes/JST_XH_B05B-XH-A_05x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5A1ED47A)
    (at 124.46 106.68 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.86 90) (layer F.SilkS))
    (fp_text value 1k (at 2.54 1.86 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 /DHT22_Data))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1EC2CE)
    (at 181.61 92.71)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1EC2DB)
    (at 181.61 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1EC2BA)
    (at 106.68 92.71)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1EC2C0)
    (at 106.68 105.41)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A1ED474)
    (at 121.92 95.25 180)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P7 (at 1.25 -3.5 180) (layer F.SilkS))
    (fp_text value "5V INPUT" (at 1.25 4.5 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 9 DGND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight (layer F.Cu) (tedit 5A1ED5F7)
    (at 138.43 95.25 180)
    (descr "JST XH series connector, B03B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P3 (at 2.5 -3.5 180) (layer F.SilkS))
    (fp_text value "RPI POWER" (at 2.5 4.5 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (model Connectors_JST.3dshapes/JST_XH_B03B-XH-A_03x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B06B-XH-A_06x2.50mm_Straight (layer F.Cu) (tedit 5A1ED5EA)
    (at 146.05 104.14)
    (descr "JST XH series connector, B06B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P4 (at 6.25 -3.5) (layer F.SilkS))
    (fp_text value RELAY (at 6.25 4.5) (layer F.SilkS))
    (fp_text user %R (at 6.25 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Relay_1))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Relay_2))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Relay_3))
    (pad 5 thru_hole circle (at 10 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Relay_4))
    (pad 6 thru_hole circle (at 12.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (model Connectors_JST.3dshapes/JST_XH_B06B-XH-A_06x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight (layer F.Cu) (tedit 5A1ED5E3)
    (at 166.37 104.14)
    (descr "JST XH series connector, B03B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P5 (at 2.5 -3.5) (layer F.SilkS))
    (fp_text value SERVO (at 2.5 4.5) (layer F.SilkS))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Servo_Data))
    (model Connectors_JST.3dshapes/JST_XH_B03B-XH-A_03x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B04B-XH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A1ED5F1)
    (at 130.81 104.14)
    (descr "JST XH series connector, B04B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P6 (at 3.75 -3.5) (layer F.SilkS))
    (fp_text value DHT22 (at 3.75 4.5) (layer F.SilkS))
    (fp_text user %R (at 3.75 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 /DHT22_Data))
    (pad 3 thru_hole circle (at 5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P6-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 9 DGND))
    (model Connectors_JST.3dshapes/JST_XH_B04B-XH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Incubator\nBreakout\nv1.0" (at 114.3 102.87) (layer F.SilkS))
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "20.320 mm" (at 193.12 99.06 270) (layer Dwgs.User))
    (feature1 (pts (xy 185.42 109.22) (xy 194.47 109.22)))
    (feature2 (pts (xy 185.42 88.9) (xy 194.47 88.9)))
    (crossbar (pts (xy 191.77 88.9) (xy 191.77 109.22)))
    (arrow1a (pts (xy 191.77 109.22) (xy 191.183579 108.093496)))
    (arrow1b (pts (xy 191.77 109.22) (xy 192.356421 108.093496)))
    (arrow2a (pts (xy 191.77 88.9) (xy 191.183579 90.026504)))
    (arrow2b (pts (xy 191.77 88.9) (xy 192.356421 90.026504)))
  )
  (dimension 82.55 (width 0.3) (layer Dwgs.User)
    (gr_text "82.550 mm" (at 144.145 81.2) (layer Dwgs.User))
    (feature1 (pts (xy 185.42 88.9) (xy 185.42 79.85)))
    (feature2 (pts (xy 102.87 88.9) (xy 102.87 79.85)))
    (crossbar (pts (xy 102.87 82.55) (xy 185.42 82.55)))
    (arrow1a (pts (xy 185.42 82.55) (xy 184.293496 83.136421)))
    (arrow1b (pts (xy 185.42 82.55) (xy 184.293496 81.963579)))
    (arrow2a (pts (xy 102.87 82.55) (xy 103.996504 83.136421)))
    (arrow2b (pts (xy 102.87 82.55) (xy 103.996504 81.963579)))
  )
  (gr_line (start 185.42 88.9) (end 153.67 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.42 109.22) (end 185.42 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 109.22) (end 185.42 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 88.9) (end 102.87 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 109.22) (end 153.67 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.87 88.9) (end 102.87 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 9) (net_name DGND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 184.15 107.95) (xy 104.14 107.95) (xy 104.14 90.17) (xy 184.15 90.17)
      )
    )
  )
)
