(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 59)
    (tracks 206)
    (zones 0)
    (modules 30)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2.54)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerber"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(D4-Pad2)")
  (net 7 "Net-(D5-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(J4-Pad4)")
  (net 12 "Net-(J4-Pad2)")
  (net 13 "Net-(K1-Pad4)")
  (net 14 "Net-(Q1-Pad2)")
  (net 15 "Net-(R1-Pad2)")
  (net 16 "Net-(R2-Pad1)")
  (net 17 "Net-(R3-Pad2)")
  (net 18 "Net-(U2-Pad9)")
  (net 19 "Net-(U2-Pad10)")
  (net 20 "Net-(U2-Pad11)")
  (net 21 "Net-(U2-Pad12)")
  (net 22 "Net-(U2-Pad13)")
  (net 23 "Net-(U2-Pad14)")
  (net 24 "Net-(U2-Pad15)")
  (net 25 "Net-(U2-Pad16)")
  (net 26 "Net-(U2-Pad3)")
  (net 27 "Net-(U2-Pad4)")
  (net 28 "Net-(U2-Pad5)")
  (net 29 "Net-(U2-Pad8)")
  (net 30 "Net-(U4-Pad9)")
  (net 31 "Net-(U4-Pad1)")
  (net 32 "Net-(J2-Pad2)")
  (net 33 "Net-(U2-Pad7)")
  (net 34 "Net-(U4-Pad6)")
  (net 35 +3V3)
  (net 36 GND)
  (net 37 Tx)
  (net 38 D0)
  (net 39 D4)
  (net 40 D8)
  (net 41 D5)
  (net 42 D7)
  (net 43 D6)
  (net 44 Rx)
  (net 45 A0)
  (net 46 D3)
  (net 47 D2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net A0)
    (add_net D0)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad9)")
    (add_net Rx)
    (add_net Tx)
  )
  (module Module:D1_mini_board (layer F.Cu) (tedit 5C64DED3)
    (at 146.05 177.8 270)
    (fp_text reference U4 (at 0 12.7 270) (layer F.SilkS) hide)
    (fp_text value WeMos_mini (at 1.27 -19.05 270) (layer F.Fab))
    (pad 9 thru_hole circle (at 11.43 -10.16 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U4-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 -7.62 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 A0))
    (pad 11 thru_hole circle (at 11.43 -5.08 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 D0))
    (pad 12 thru_hole circle (at 11.43 -2.54 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 D5))
    (pad 13 thru_hole circle (at 11.43 0 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 D6))
    (pad 14 thru_hole circle (at 11.43 2.54 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 D7))
    (pad 15 thru_hole circle (at 11.43 5.08 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 D8))
    (pad 16 thru_hole circle (at 11.43 7.62 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 +3V3))
    (pad 1 thru_hole circle (at -11.43 7.62 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -11.43 5.08 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (pad 3 thru_hole circle (at -11.43 2.54 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 D4))
    (pad 4 thru_hole circle (at -11.43 0 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 D3))
    (pad 5 thru_hole circle (at -11.43 -2.54 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 D2))
    (pad 6 thru_hole circle (at -11.43 -5.08 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -11.43 -7.62 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 Rx))
    (pad 8 thru_hole circle (at -11.43 -10.16 270) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 Tx))
  )
  (module Buzzer_Beeper:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5C64DEB5)
    (at 137.16 177.165)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value Buzzer (at 3.8 7.4) (layer F.Fab))
    (fp_text user %R (at 3.8 -4) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54) (layer F.SilkS))
    (fp_text user + (at -0.01 -2.54) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.6 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 D0))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5D0FE066)
    (at 128.905 170.815)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D4 (at 0 -3.5) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5D0FDF9F)
    (at 128.905 164.465)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D5 (at 0 -3.5) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D5-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad2)"))
    (pad 3 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C64DFC5)
    (at 147.955 163.83 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Female (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 Tx))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 Rx))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:Hackspace_logo_10mm (layer F.Cu) (tedit 0)
    (at 140.335 90.17)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5C64DFBF)
    (at 138.43 160.02 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Female (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 -180) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 D8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 D5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 D7))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 D6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C64DEF3)
    (at 128.27 159.385 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:D1_mini_board (layer F.Cu) (tedit 5C64DE55)
    (at 147.955 90.805 90)
    (fp_text reference U2 (at -2.54 13.97 180) (layer F.SilkS) hide)
    (fp_text value WeMos_mini (at 1.27 -19.05 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 11.43 -10.16 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U2-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 -7.62 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 11.43 -5.08 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 -2.54 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 11.43 0 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U2-Pad13)"))
    (pad 14 thru_hole circle (at 11.43 2.54 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 11.43 5.08 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad15)"))
    (pad 16 thru_hole circle (at 11.43 7.62 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad16)"))
    (pad 1 thru_hole circle (at -11.43 7.62 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at -11.43 5.08 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at -11.43 2.54 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 0 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at -11.43 -2.54 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at -11.43 -5.08 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(R1-Pad2)"))
    (pad 7 thru_hole circle (at -11.43 -7.62 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at -11.43 -10.16 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad8)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C64DE0F)
    (at 132.715 99.06)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 154.305 90.17)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C64DDF1)
    (at 157.48 97.155 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_A-405_P12.70mm_Horizontal (layer F.Cu) (tedit 5C64DDC4)
    (at 150.495 113.665)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 6.35 0) (layer F.SilkS))
    (fp_text value 1N4007 (at 6.35 2.47) (layer F.Fab))
    (fp_text user K (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text user K (at 0 -1.9) (layer F.Fab))
    (fp_text user %R (at 6.74 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 12.7 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 128.27 143.51)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 166.37 97.79)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 128.27 97.79)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 166.37 143.51)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C64DE14)
    (at 132.715 95.885)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 5C64DDDA)
    (at 160.655 108.585)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 3.81 -2.54) (layer F.SilkS))
    (fp_text value S8050 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 5C64DDA0)
    (at 156.845 118.745 270)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K1 (at 17.145 -0.127) (layer F.SilkS))
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6 270) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025 270) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 4 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(K1-Pad4)"))
    (pad 3 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 1.95 6.05) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:HLK-PM01 (layer F.Cu) (tedit 5C64DD87)
    (at 136.525 121.285 90)
    (fp_text reference U1 (at 0 1 90) (layer F.SilkS))
    (fp_text value HLK-PM05 (at 0 -1 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.7 -2.5 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at -14.7 2.5 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 14.7 -7.7 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad1)"))
    (pad 4 thru_hole circle (at 14.7 7.7 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad1)"))
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 5C64DDD0)
    (at 156.845 108.585 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-3_P5.08mm (layer F.Cu) (tedit 5C64E77F)
    (at 144.145 145.415 180)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference J1 (at 5.05 -4.65 180) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x03 (at 5.08 5.08 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-3_P5.08mm (layer F.Cu) (tedit 5C64E786)
    (at 160.655 145.415 180)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference J2 (at 5.05 -4.65 180) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x03 (at 5.08 5.08 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Panelization:mouse-bite-2.54mm-slot (layer F.Cu) (tedit 551DB929)
    (at 131.7625 154.305)
    (fp_text reference mouse-bite-2.54mm-slot (at 0 -2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 2.1) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Panelization:mouse-bite-2.54mm-slot (layer F.Cu) (tedit 551DB929)
    (at 163.5125 154.305)
    (fp_text reference mouse-bite-2.54mm-slot (at 0 -2) (layer F.SilkS) hide)
    (fp_text value VAL** (at 0 2.1) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.8 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.8 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -1.1) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 5C64DE5B)
    (at 132.08 92.71 90)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 1.27 90) (layer F.SilkS))
    (fp_text value PC817 (at 3.81 4.87 90) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Rotary_Encoder:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm (layer F.Cu) (tedit 5C64DF03)
    (at 154.305 173.355)
    (descr "Alps rotary encoder, EC12E... with switch, vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
    (tags "rotary encoder")
    (fp_text reference SW1 (at 3.81 -0.635) (layer F.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 7.5 10.4) (layer F.Fab))
    (fp_text user %R (at 11.1 6.3) (layer F.Fab))
    (pad A thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 47 D2))
    (pad C thru_hole circle (at 0 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad B thru_hole circle (at 0 5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 46 D3))
    (pad MP thru_hole rect (at 7.5 -3.1) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
    (pad MP thru_hole rect (at 7.5 8.1) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
    (pad S2 thru_hole circle (at 14.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 45 A0))
    (pad S1 thru_hole circle (at 14.5 5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5D0FD812)
    (at 156.845 184.15 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37 180) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.37 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 A0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5D0FE06F)
    (at 128.905 177.8)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at 0 -3.175) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 +3V3))
    (pad 2 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 4 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 39 D4))
    (pad 3 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 166.37 184.785) (end 166.37 187.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 190.5) (end 163.83 190.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.91 180.975) (end 168.91 182.245) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.91 184.785) (end 168.91 182.245) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.82091 187.952655) (end 130.82091 190.492655) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.74091 180.967655) (end 124.47091 180.967655) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.74091 184.777655) (end 125.74091 182.237655) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.28091 187.952655) (end 128.28091 184.777655) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 163.83 187.96) (end 163.83 190.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.35909 80.652345) (end 166.35909 83.827345) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 163.81909 80.652345) (end 163.81909 78.112345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.89909 83.827345) (end 168.89909 86.367345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.81 80.645) (end 130.81 78.105) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.73 83.82) (end 125.73 86.36) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Teesside Hackspace\nTool Access Control\nv1.3" (at 147.32 84.455) (layer F.SilkS))
  (gr_arc (start 133.985 154.305) (end 133.985 153.035) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.54 154.305) (end 129.54 155.575) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.54 154.305) (end 130.81 154.305) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 133.985 154.305) (end 132.715 154.305) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.29 154.305) (end 161.29 155.575) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.29 154.305) (end 162.56 154.305) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.735 154.305) (end 164.465 154.305) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.735 154.305) (end 165.735 153.035) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 155.575) (end 128.27 155.575) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 153.035) (end 129.54 153.035) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.985 155.575) (end 161.29 155.575) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 153.035) (end 133.985 153.035) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 155.575) (end 165.735 155.575) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.37 159.385) (end 170.18 159.385) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 159.385) (end 128.27 155.575) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 180.975) (end 170.18 159.385) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 159.385) (end 124.46 180.975) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 124.46) (end 154.305 124.46) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.305 116.84) (end 159.385 116.84) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 159.385 116.84) (end 159.385 124.46) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 159.385 124.46) (end 167.005 124.46) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.305 124.46) (end 154.305 116.84) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160.655 123.19) (end 167.005 123.19) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160.655 115.57) (end 160.655 123.19) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.035 115.57) (end 160.655 115.57) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.035 123.19) (end 153.035 115.57) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139.7 123.19) (end 153.035 123.19) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 139.7 123.825) (end 139.7 123.19) (angle -180) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 167.005 123.825) (end 167.005 124.46) (angle -180) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 165.735 153.035) (end 166.37 153.035) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.73 87.63) (end 125.73 86.36) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.18 149.225) (end 170.18 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 87.63) (end 124.46 149.225) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 78.105) (end 130.81 78.105) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 83.82) (end 128.27 80.645) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 166.37 149.225) (end 166.37 153.035) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 149.225) (end 124.46 149.225) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.89909 87.637345) (end 170.16909 87.637345) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text N (at 160.655 150.495) (layer F.SilkS))
  (gr_text E (at 150.495 150.495) (layer F.SilkS))
  (gr_text E (at 144.145 150.495) (layer F.SilkS))
  (gr_text N (at 133.985 150.495) (layer F.SilkS))
  (gr_text L (at 155.575 150.495) (layer F.SilkS))
  (gr_text L (at 139.065 150.495) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.194 118.872) (xy 158.496 118.872) (xy 158.496 127) (xy 156.21 129.286) (xy 146.558 129.286)
        (xy 140.462 135.382) (xy 140.462 146.05) (xy 137.414 146.304) (xy 137.414 134.239) (xy 145.542 125.984)
        (xy 155.194 125.984)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.225 133.35) (xy 149.225 135.89) (xy 149.352 136.398) (xy 153.924 140.97) (xy 153.924 146.05)
        (xy 156.972 146.05) (xy 156.972 139.7) (xy 152.4 134.874) (xy 152.4 133.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.145 144.145) (xy 151.13 144.145) (xy 151.13 146.685) (xy 144.145 146.685)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.004 144.78) (xy 162.052 144.78) (xy 162.052 151.13) (xy 160.782 152.146) (xy 134.747 152.146)
        (xy 132.334 149.86) (xy 132.334 135.89) (xy 135.636 135.89) (xy 135.636 148.844) (xy 159.004 148.844)
      )
    )
  )
  (zone (net 36) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 155.575) (xy 170.18 155.575) (xy 170.18 190.5) (xy 124.46 190.5)
      )
    )
  )
  (zone (net 36) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 155.575) (xy 170.18 155.575) (xy 170.18 190.5) (xy 124.46 190.5)
      )
    )
  )
)
