(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 86)
    (no_connects 3)
    (area 156.389999 90.089999 171.410001 105.110001)
    (thickness 0.8)
    (drawings 44)
    (tracks 437)
    (zones 0)
    (modules 38)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.1524)
    (zone_clearance 0.15)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.02)
    (edge_width 0.02)
    (via_size 0.4)
    (via_drill 0.254)
    (via_min_size 0.36)
    (via_min_drill 0.254)
    (user_via 0.36 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.3 1.3)
    (pad_drill 1.3)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (grid_origin 158.1 103.1)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(C10-Pad1)")
  (net 5 "Net-(C12-Pad1)")
  (net 6 /D+)
  (net 7 /D-)
  (net 8 "Net-(R3-Pad1)")
  (net 9 CS_MPU)
  (net 10 "Net-(U2-Pad5)")
  (net 11 "Net-(U2-Pad6)")
  (net 12 INT_MPU)
  (net 13 SCLK_MPU)
  (net 14 AD0_MPU)
  (net 15 SDI_MPU)
  (net 16 /Boot)
  (net 17 /S4)
  (net 18 /S3)
  (net 19 /S2)
  (net 20 /S1)
  (net 21 /SBUS)
  (net 22 /Vbat)
  (net 23 "Net-(J10-Pad1)")
  (net 24 "Net-(D1-Pad1)")
  (net 25 "Net-(D1-Pad2)")
  (net 26 "Net-(U2-Pad2)")
  (net 27 "Net-(U2-Pad4)")
  (net 28 "Net-(U2-Pad11)")
  (net 29 "Net-(U2-Pad12)")
  (net 30 "Net-(U2-Pad18)")
  (net 31 "Net-(U2-Pad19)")
  (net 32 "Net-(U2-Pad20)")
  (net 33 "Net-(U2-Pad21)")
  (net 34 "Net-(U2-Pad22)")
  (net 35 "Net-(U2-Pad25)")
  (net 36 "Net-(U2-Pad26)")
  (net 37 "Net-(U2-Pad27)")
  (net 38 "Net-(U2-Pad28)")
  (net 39 "Net-(U2-Pad30)")
  (net 40 "Net-(U2-Pad31)")
  (net 41 "Net-(U2-Pad34)")
  (net 42 "Net-(U2-Pad37)")
  (net 43 "Net-(U2-Pad39)")
  (net 44 "Net-(U2-Pad45)")
  (net 45 "Net-(U2-Pad46)")
  (net 46 "Net-(U3-Pad6)")
  (net 47 "Net-(U3-Pad5)")
  (net 48 "Net-(U3-Pad2)")
  (net 49 "Net-(U3-Pad4)")
  (net 50 "Net-(U3-Pad3)")
  (net 51 "Net-(U3-Pad16)")
  (net 52 "Net-(U3-Pad15)")
  (net 53 "Net-(U3-Pad17)")
  (net 54 "Net-(U3-Pad14)")
  (net 55 "Net-(U3-Pad21)")
  (net 56 "Net-(U3-Pad20)")
  (net 57 "Net-(U3-Pad19)")
  (net 58 "Net-(U3-Pad7)")
  (net 59 "Net-(U3-Pad11)")
  (net 60 "Net-(U3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.16)
    (via_dia 0.4)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Boot)
    (add_net /D+)
    (add_net /D-)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /S4)
    (add_net /SBUS)
    (add_net /Vbat)
    (add_net AD0_MPU)
    (add_net CS_MPU)
    (add_net INT_MPU)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad34)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad45)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net SCLK_MPU)
    (add_net SDI_MPU)
  )
  (net_class BATT ""
    (clearance 0.16)
    (trace_width 0.22)
    (via_dia 0.4)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
  )
  (net_class GND ""
    (clearance 0.16)
    (trace_width 0.22)
    (via_dia 0.4)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class VCC ""
    (clearance 0.16)
    (trace_width 0.22)
    (via_dia 0.4)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (module KiCadCustomLibs:MPU-6000 (layer F.Cu) (tedit 59E9C3B2)
    (at 163.14 97.62)
    (fp_text reference U3 (at 0.2 3.4) (layer F.SilkS) hide)
    (fp_text value ICM20689 (at -0.1 -3.4) (layer F.Fab) hide)
    (pad 6 smd rect (at -2 1.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U3-Pad6)"))
    (pad 1 smd rect (at -2 -1.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-Pad1)"))
    (pad 5 smd rect (at -2 0.75 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad5)"))
    (pad 2 smd rect (at -2 -0.75 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U3-Pad2)"))
    (pad 4 smd rect (at -2 0.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -2 -0.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U3-Pad3)"))
    (pad 16 smd rect (at 2 -0.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U3-Pad16)"))
    (pad 15 smd rect (at 2 0.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad15)"))
    (pad 17 smd rect (at 2 -0.75 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U3-Pad17)"))
    (pad 14 smd rect (at 2 0.75 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U3-Pad14)"))
    (pad 18 smd rect (at 2 -1.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2 1.25 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 21 smd rect (at 0.25 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U3-Pad21)"))
    (pad 22 smd rect (at -0.25 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 CS_MPU))
    (pad 20 smd rect (at 0.75 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad20)"))
    (pad 23 smd rect (at -0.75 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 SCLK_MPU))
    (pad 19 smd rect (at 1.25 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad19)"))
    (pad 24 smd rect (at -1.25 -2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 SDI_MPU))
    (pad 7 smd rect (at -1.25 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-Pad7)"))
    (pad 12 smd rect (at 1.25 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 INT_MPU))
    (pad 8 smd rect (at -0.75 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 11 smd rect (at 0.75 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U3-Pad11)"))
    (pad 9 smd rect (at -0.25 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 AD0_MPU))
    (pad 10 smd rect (at 0.25 2) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (model Housings_DFN_QFN.3dshapes/QFN-24_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer B.Cu) (tedit 59B00697)
    (at 163.72 97.64 270)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 6 270) (layer B.SilkS) hide)
    (fp_text value STM32F303CCTx (at 0 -6 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -4.35 2.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -4.35 2.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -4.35 1.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D1-Pad1)"))
    (pad 4 smd rect (at -4.35 1.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -4.35 0.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -4.35 0.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -4.35 -0.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 8 smd rect (at -4.35 -0.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -4.35 -1.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 10 smd rect (at -4.35 -1.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 /Vbat))
    (pad 11 smd rect (at -4.35 -2.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -4.35 -2.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 12 INT_MPU))
    (pad 14 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 CS_MPU))
    (pad 15 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 SCLK_MPU))
    (pad 16 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 14 AD0_MPU))
    (pad 17 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 SDI_MPU))
    (pad 18 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 25 smd rect (at 4.35 -2.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U2-Pad25)"))
    (pad 26 smd rect (at 4.35 -2.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 4.35 -1.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 4.35 -1.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at 4.35 -0.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J10-Pad1)"))
    (pad 30 smd rect (at 4.35 -0.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U2-Pad30)"))
    (pad 31 smd rect (at 4.35 0.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U2-Pad31)"))
    (pad 32 smd rect (at 4.35 0.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /D-))
    (pad 33 smd rect (at 4.35 1.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /D+))
    (pad 34 smd rect (at 4.35 1.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U2-Pad34)"))
    (pad 35 smd rect (at 4.35 2.25 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 4.35 2.75 270) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 37 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U2-Pad37)"))
    (pad 38 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 /SBUS))
    (pad 39 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U2-Pad39)"))
    (pad 40 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /S4))
    (pad 41 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /S3))
    (pad 42 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /S2))
    (pad 43 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 /S1))
    (pad 44 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /Boot))
    (pad 45 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U2-Pad45)"))
    (pad 46 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U2-Pad46)"))
    (pad 47 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0402 (layer F.Cu) (tedit 59F08634)
    (at 161.28 92.48)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.4) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.61 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.61 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59EDA237)
    (at 160.12 100.54 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 300mA (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EA098A)
    (at 169.9 103.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EA098A)
    (at 169.9 91.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module MountingHole_1.1mm_M1 (layer F.Cu) (tedit 59EA098A)
    (at 157.9 91.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 59EA09AE)
    (at 157.9 103.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:Boot_Pin (layer F.Cu) (tedit 59E9EC0C)
    (at 158.7 94.45)
    (fp_text reference J1 (at 0.5 1.5) (layer F.SilkS) hide)
    (fp_text value Boot1 (at 0.1 -1.3) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
  )
  (module UDFN-4_1x1mm_Pitch0.65mm (layer F.Cu) (tedit 59E9E2C7)
    (at 166.62 98.44 90)
    (descr UDFN-4_1x1mm_Pitch0.65mm)
    (tags UDFN-4_1x1mm_Pitch0.65mm)
    (attr smd)
    (fp_text reference U1 (at 0.45 -2.16 90) (layer F.SilkS) hide)
    (fp_text value MIC550X-DFN (at 0.47 2.34 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.34 -0.5) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0 -0.17 45) (size 0.24 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.17 0 45) (size 0.24 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.17 0 45) (size 0.24 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.34 0.5 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd trapezoid (at 0.44 0.3 90) (size 0.2 0.2) (rect_delta 0 0.1999 ) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at 0.58 0.4) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 0.34 -0.5 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd trapezoid (at 0.44 -0.3) (size 0.2 0.2) (rect_delta 0.1999 0 ) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 0.58 -0.4) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 1 smd rect (at -0.58 -0.4) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0 0.17 45) (size 0.24 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.58 0.4) (size 0.4 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd trapezoid (at -0.44 -0.3 270) (size 0.2 0.2) (rect_delta 0 0.19999 ) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd trapezoid (at -0.44 0.3 180) (size 0.2 0.2) (rect_delta 0.1999 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.34 0.5 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/UDFN-4_1x1mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B00DA5)
    (at 166.78 96.91 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value 2.2uf (at 0 1.27 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B00DC7)
    (at 166.58 100.16)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 2.2uf (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59B00B80)
    (at 167.98 101.64 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 1.27 225) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59B00B72)
    (at 159.57 101.77 135)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 1.27 135) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 135) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 135) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0 135) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59B00BA5)
    (at 159.54 93.36 225)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 1.27 225) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.27 225) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.27 225) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0 225) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B01032)
    (at 165.84 92.72)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 1uf (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B0102A)
    (at 165.85 93.59)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B0125E)
    (at 163.83 100.6)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 0.47uf (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B0114D)
    (at 166.58 101.1)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 2.2uf (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59B0114F)
    (at 166.57 102.03)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59B00A2B)
    (at 163.09 92.47)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value 330 (at 0 1.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer B.Cu) (tedit 59B01007)
    (at 167.77 93.26 315)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 1.2 315) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.25 315) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.2 315) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.45 0 315) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59B00FA1)
    (at 159.8 94.99 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /Boot))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59B01088)
    (at 167.41 95.28 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /Vbat))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59B01083)
    (at 167.42 93.52 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.2 90) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.25 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /Vbat))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59B00F21)
    (at 160.92 102.31 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.2 270) (layer F.SilkS) hide)
    (fp_text value 1K5 (at 0 1.25 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /D+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:USB_3_PADS (layer F.Cu) (tedit 59E9C2BE)
    (at 163.36 102.4 180)
    (fp_text reference J7 (at 0.3 1.6 180) (layer F.SilkS) hide)
    (fp_text value USB (at 0.1 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.25 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /D-))
    (pad 3 smd rect (at 1.25 0 180) (size 0.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /D+))
  )
  (module KiCadCustomLibs:SBUS_PADS (layer F.Cu) (tedit 59E9FD43)
    (at 158.9 97.52 270)
    (fp_text reference J8 (at 0.3 1.6 270) (layer F.SilkS) hide)
    (fp_text value SBUS (at 0.1 -1.6 270) (layer F.Fab) hide)
    (pad 1 smd oval (at -1 0 270) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 0 270) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at 1 0 270) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /SBUS))
  )
  (module KiCadCustomLibs:POWER2PIN (layer F.Cu) (tedit 59E9C3C3)
    (at 168.58 97.63 90)
    (fp_text reference J9 (at 0.1 1.8 90) (layer F.SilkS) hide)
    (fp_text value POWER (at 0.3 -1.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.9 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
  )
  (module KiCadCustomLibs:ESC_PADS (layer F.Cu) (tedit 59B0F52C)
    (at 168.79 100.39)
    (fp_text reference J10 (at 0.3 1.6) (layer F.SilkS) hide)
    (fp_text value LED_STRIP (at -0.1 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J10-Pad1)"))
  )
  (module KiCadCustomLibs:Ceramic_Resonator_SMD_3mm (layer F.Cu) (tedit 59E9C3AD)
    (at 163 93.9)
    (fp_text reference Y1 (at 0.1 2.3) (layer F.SilkS) hide)
    (fp_text value 8MHZ (at 0.1 -2.2) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.2 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 3 smd rect (at 1.2 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad6)"))
    (pad 2 smd rect (at 0 0) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module KiCadCustomLibs:Boot_Pin (layer F.Cu) (tedit 59E9EC0C)
    (at 158.7 95.37)
    (fp_text reference J2 (at 0.5 1.5) (layer F.SilkS) hide)
    (fp_text value Boot0 (at 0.1 -1.3) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /Boot))
  )
  (module KiCadCustomLibs:PAD1.4x0.6 (layer F.Cu) (tedit 59ED95A9)
    (at 168.44 92.81 45)
    (fp_text reference J6 (at 0.3 1.6 45) (layer F.SilkS) hide)
    (fp_text value ESC1 (at -0.1 -1.5 45) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 45) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /S1))
  )
  (module KiCadCustomLibs:PAD1.4x0.6 (layer F.Cu) (tedit 59ED95A9)
    (at 159.14 92.92 135)
    (fp_text reference J5 (at 0.3 1.6 135) (layer F.SilkS) hide)
    (fp_text value ESC2 (at -0.1 -1.5 135) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 135) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /S2))
  )
  (module KiCadCustomLibs:PAD1.4x0.6 (layer F.Cu) (tedit 59ED95A9)
    (at 159.16 102.21 45)
    (fp_text reference J3 (at 0.3 1.6 45) (layer F.SilkS) hide)
    (fp_text value ESC4 (at -0.1 -1.5 45) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 45) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /S4))
  )
  (module KiCadCustomLibs:PAD1.4x0.6 (layer F.Cu) (tedit 59ED95A9)
    (at 168.41 102.15 135)
    (fp_text reference J4 (at 0.3 1.6 135) (layer F.SilkS) hide)
    (fp_text value ESC3 (at -0.1 -1.5 135) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 135) (size 0.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /S3))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer F.Cu) (tedit 59F1D273)
    (at 161.77 100.6 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.27 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402_NoSilk (layer F.Cu) (tedit 59F2D811)
    (at 168.41 94.9 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.2 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.25 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.2 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 CS_MPU))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 20689 (at 163.4 97.6 90) (layer F.SilkS))
  (gr_text "(" (at 159.2 94.95 180) (layer F.SilkS))
  (gr_text - (at 159.8 96.5 270) (layer F.SilkS))
  (gr_line (start 169.3 93.1) (end 169.9 93.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 169.3 102.1) (end 169.3 93.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 169.9 102.1) (end 169.3 102.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 168.4 103.1) (end 168.4 103.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 159.4 103.1) (end 168.4 103.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 103.6) (end 169.9 102.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 103.6) (end 169.9 105.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 103.6) (end 171.4 103.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 168.4 92) (end 168.4 91.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 159.4 92) (end 168.4 92) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 91.6) (end 168.4 91.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 91.6) (end 171.4 91.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 169.9 91.6) (end 169.9 90.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 158.2 102.1) (end 158.2 93) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157.9 102.1) (end 158.2 102.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 159.4 103.6) (end 159.4 103.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.9 103.6) (end 159.4 103.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.9 103.6) (end 157.9 105.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.9 103.6) (end 156.4 103.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.9 91.6) (end 156.4 91.6) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 157.8 93) (end 158.2 93) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_line (start 159.4 91.6) (end 159.4 92) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.8 91.6) (end 157.8 93) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_arc (start 157.9 91.6) (end 157.9 90.1) (angle 90) (layer Edge.Cuts) (width 0.02))
  (gr_text LED_S (at 168.05 100.42 90) (layer F.SilkS))
  (gr_text 1S (at 166.44 95.77 90) (layer F.SilkS))
  (gr_text +USB- (at 162.76 101.41) (layer F.SilkS))
  (gr_text uFF3 (at 159 100.1 270) (layer F.SilkS))
  (gr_text - (at 167.61 98.41 90) (layer F.SilkS))
  (gr_text + (at 167.59 96.25) (layer F.SilkS))
  (gr_text - (at 164.6 101.55) (layer F.SilkS))
  (gr_text SBUS (at 160 97.9 270) (layer F.SilkS))
  (gr_text 3 (at 168.71 103.2) (layer F.SilkS))
  (gr_text 1 (at 168.7 91.94) (layer F.SilkS))
  (gr_text 2 (at 159.06 91.9) (layer F.SilkS))
  (gr_text 4 (at 159.09 103.22) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 158.06 91.82) (xy 169.58 91.79) (xy 169.53 103.3) (xy 157.99 103.3)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 158.08 91.82) (xy 169.6 91.79) (xy 169.55 103.32) (xy 157.95 103.32)
      )
    )
  )
)
