<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.155" x2="80" y2="0.155" width="0" layer="20"/>
<wire x1="80" y1="0.155" x2="80" y2="50.155" width="0" layer="20"/>
<wire x1="80" y1="50.155" x2="0" y2="50.155" width="0" layer="20"/>
<wire x1="0" y1="50.155" x2="0" y2="0.155" width="0" layer="20"/>
<text>Enabled by Plane Crazy Innovations
LITO-GDL5.2 GDL90 Processor
2018</text>
</plain>
<libraries>
<library name="POLCAP">
<packages>
<package name="E2-4">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2 mm, diameter 4 mm</description>
</package>
<package name="E3,5-8">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 3.5 mm, diameter 8 mm</description>
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.4">
<packages>
<package name="TEENSY_3.6_DIL">
</package>
</packages>
</library>
<library name="MAX3222E">
<packages>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="F15HP-HARTING">
<packages>
<package name="F15HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Murata_OKI-78SR">
<packages>
<package name="SIP3H">
<description>Murata specific SIP3 horizontal package (reversed from Recom/Cui horizontal pin config)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="POLCAP" package="E2-4" value=".1uF"/>
<element name="C10" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="POLCAP" package="E2-4" value=".1uF"/>
<element name="C6" library="POLCAP" package="E2-4" value=".1uF"/>
<element name="C7" library="POLCAP" package="E2-4" value=".1uF"/>
<element name="C8" library="POLCAP" package="E2-4" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="POLCAP" package="E3,5-8" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Teensy_3_and_LC_Series_Boards_v1.4" package="TEENSY_3.6_DIL" value="TEENSY_3.6_DIL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="MAX3222E" package="DIL18" value="MAX3222EEPN+"/>
<element name="IC3" library="MAX3222E" package="DIL18" value="MAX3222EEPN+"/>
<element name="X1" library="F15HP-HARTING" package="F15HP" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="IC4" library="Murata_OKI-78SR" package="SIP3H" value="OKI-78SR-5/1.5-W36H-C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C9" pad="+"/>
<contactref element="X1" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="GND"/>
<contactref element="IC1" pad="GND1"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC3" pad="16"/>
<contactref element="C8" pad="-"/>
<contactref element="C5" pad="-"/>
<contactref element="C6" pad="+"/>
<contactref element="C9" pad="-"/>
<contactref element="C10" pad="-"/>
<contactref element="C7" pad="+"/>
<contactref element="C11" pad="-"/>
<contactref element="IC1" pad="AGND"/>
<contactref element="X1" pad="11"/>
<contactref element="X1" pad="12"/>
<contactref element="X1" pad="13"/>
<contactref element="X1" pad="14"/>
<contactref element="X1" pad="15"/>
<contactref element="X1" pad="G2"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC3" pad="15"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="IC3" pad="14"/>
<contactref element="X1" pad="9"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="9"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC3" pad="8"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="15"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="14"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="9"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="8"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="2"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="17"/>
<contactref element="IC3" pad="17"/>
<contactref element="IC1" pad="3.3V"/>
<contactref element="IC1" pad="3.3V3"/>
<contactref element="C11" pad="+"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="N$19">
<contactref element="IC3" pad="12"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="0"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$21">
<contactref element="IC3" pad="13"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$28">
<contactref element="IC1" pad="31/A12"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$29">
<contactref element="IC3" pad="11"/>
<contactref element="IC1" pad="32/A13"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$9">
<contactref element="IC2" pad="4"/>
<contactref element="C1" pad="-"/>
</signal>
<signal name="N$10">
<contactref element="IC2" pad="5"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="N$11">
<contactref element="C2" pad="-"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="IC3" pad="2"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$23">
<contactref element="IC3" pad="5"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="N$26">
<contactref element="C3" pad="-"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="C4" pad="-"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$31">
<contactref element="IC2" pad="3"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="N$33">
<contactref element="C8" pad="+"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="C6" pad="-"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$32">
<contactref element="C7" pad="-"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="C10" pad="+"/>
<contactref element="IC1" pad="VIN"/>
<contactref element="IC4" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
