(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 76.2 22.86)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (property "version" "v1.0.0-3-g64319bd")
  (net 0 "")
  (net 1 "GND")
  (net 2 "/SCA")
  (net 3 "/SCL")
  (net 4 "Net-(J7-Pin_1)")
  (net 5 "Net-(J8-Pin_1)")
  (net 6 "Net-(J9-Pin_1)")
  (net 7 "Net-(J10-Pin_1)")
  (net 8 "Net-(J11-Pin_1)")
  (net 9 "Net-(J12-Pin_1)")
  (net 10 "Net-(J13-Pin_1)")
  (net 11 "Net-(J14-Pin_1)")
  (net 12 "Net-(J15-Pin_1)")
  (net 13 "Net-(J16-Pin_1)")
  (net 14 "Net-(J17-Pin_1)")
  (net 15 "Net-(J18-Pin_1)")
  (net 16 "Net-(J21-Pin_1)")
  (net 17 "Net-(J22-Pin_1)")
  (net 18 "Net-(J23-Pin_1)")
  (net 19 "Net-(J24-Pin_1)")
  (net 20 "Net-(J25-Pin_1)")
  (net 21 "Net-(J26-Pin_1)")
  (net 22 "Net-(J27-Pin_1)")
  (net 23 "Net-(J28-Pin_1)")
  (net 24 "Net-(J29-Pin_1)")
  (net 25 "Net-(J30-Pin_1)")
  (net 26 "Net-(J31-Pin_1)")
  (net 27 "Net-(J35-Pin_1)")
  (net 28 "Net-(J36-Pin_1)")
  (net 29 "Net-(J37-Pin_1)")
  (net 30 "Net-(J38-Pin_1)")
  (net 31 "/VDD")
  (net 32 "Net-(J32-Pin_1)")
  (net 33 "Net-(J33-Pin_1)")
  (net 34 "Net-(J19-Pin_1)")
  (net 35 "Net-(J20-Pin_1)")
  (net 36 "Net-(J34-Pin_1)")
  (net 37 "Net-(J39-Pin_1)")
  (net 38 "Net-(J40-Pin_1)")
  (net 39 "Net-(J41-Pin_1)")
  (net 40 "Net-(J42-Pin_1)")
  (net 41 "Net-(J3-Pin_1)")
  (net 42 "Net-(J5-Pin_1)")
  (net 43 "Net-(J43-Pin_1)")
  (net 44 "Net-(J44-Pin_1)")
  (net 45 "Net-(J45-Pin_1)")
  (net 46 "Net-(J46-Pin_1)")
  (net 47 "Net-(J47-Pin_1)")
  (net 48 "Net-(J48-Pin_1)")
  (net 49 "Net-(J49-Pin_1)")
  (net 50 "Net-(J50-Pin_1)")
  (net 51 "Net-(J51-Pin_1)")
  (net 52 "Net-(J52-Pin_1)")
  (net 53 "Net-(J53-Pin_1)")
  (net 54 "Net-(J54-Pin_1)")
  (net 55 "Net-(J55-Pin_1)")
  (net 56 "Net-(J56-Pin_1)")
  (net 57 "Net-(J57-Pin_1)")
  (net 58 "Net-(J58-Pin_1)")
  (net 59 "Net-(J59-Pin_1)")
  (net 60 "Net-(J60-Pin_1)")
  (net 61 "Net-(J61-Pin_1)")
  (net 62 "Net-(J62-Pin_1)")
  (net 63 "Net-(J63-Pin_1)")
  (net 64 "Net-(J64-Pin_1)")
  (net 65 "Net-(J65-Pin_1)")
  (net 66 "Net-(J66-Pin_1)")
  (net 67 "Net-(J67-Pin_1)")
  (net 68 "Net-(J68-Pin_1)")
  (net 69 "Net-(J69-Pin_1)")
  (net 70 "Net-(J70-Pin_1)")
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 27.94 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J9" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J9-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x30_P2.54mm" (layer "F.Cu")
    (at 96.52 96.52)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x30, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J37" (at 0 2.54 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x30_Socket" (at 0 4.04 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 0 -33.02) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_14") (pintype "passive") (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 0 -35.56) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_15") (pintype "passive") (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 0 -38.1) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_16") (pintype "passive") (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 0 -40.64) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_17") (pintype "passive") (thermal_bridge_angle 45))
    (pad "18" smd roundrect (at 0 -43.18) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_18") (pintype "passive") (thermal_bridge_angle 45))
    (pad "19" smd roundrect (at 0 -45.72) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_19") (pintype "passive") (thermal_bridge_angle 45))
    (pad "20" smd roundrect (at 0 -48.26) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_20") (pintype "passive") (thermal_bridge_angle 45))
    (pad "21" smd roundrect (at 0 -50.8) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_21") (pintype "passive") (thermal_bridge_angle 45))
    (pad "22" smd roundrect (at 0 -53.34) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_22") (pintype "passive") (thermal_bridge_angle 45))
    (pad "23" smd roundrect (at 0 -55.88) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_23") (pintype "passive") (thermal_bridge_angle 45))
    (pad "24" smd roundrect (at 0 -58.42) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_24") (pintype "passive") (thermal_bridge_angle 45))
    (pad "25" smd roundrect (at 0 -60.96) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_25") (pintype "passive") (thermal_bridge_angle 45))
    (pad "26" smd roundrect (at 0 -63.5) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_26") (pintype "passive") (thermal_bridge_angle 45))
    (pad "27" smd roundrect (at 0 -66.04) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_27") (pintype "passive") (thermal_bridge_angle 45))
    (pad "28" smd roundrect (at 0 -68.58) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_28") (pintype "passive") (thermal_bridge_angle 45))
    (pad "29" smd roundrect (at 0 -71.12) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_29") (pintype "passive") (thermal_bridge_angle 45))
    (pad "30" smd roundrect (at 0 -73.66) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J37-Pin_1)") (pinfunction "Pin_30") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x26_P2.54mm" (layer "F.Cu")
    (at 116.84 27.94 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x26, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J70" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x26_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 0 -33.02 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_14") (pintype "passive") (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 0 -35.56 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_15") (pintype "passive") (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 0 -38.1 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_16") (pintype "passive") (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 0 -40.64 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_17") (pintype "passive") (thermal_bridge_angle 45))
    (pad "18" smd roundrect (at 0 -43.18 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_18") (pintype "passive") (thermal_bridge_angle 45))
    (pad "19" smd roundrect (at 0 -45.72 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_19") (pintype "passive") (thermal_bridge_angle 45))
    (pad "20" smd roundrect (at 0 -48.26 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_20") (pintype "passive") (thermal_bridge_angle 45))
    (pad "21" smd roundrect (at 0 -50.8 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_21") (pintype "passive") (thermal_bridge_angle 45))
    (pad "22" smd roundrect (at 0 -53.34 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_22") (pintype "passive") (thermal_bridge_angle 45))
    (pad "23" smd roundrect (at 0 -55.88 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_23") (pintype "passive") (thermal_bridge_angle 45))
    (pad "24" smd roundrect (at 0 -58.42 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_24") (pintype "passive") (thermal_bridge_angle 45))
    (pad "25" smd roundrect (at 0 -60.96 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_25") (pintype "passive") (thermal_bridge_angle 45))
    (pad "26" smd roundrect (at 0 -63.5 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J70-Pin_1)") (pinfunction "Pin_26") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 73.66 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J59" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(J59-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 66.04 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J24" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J24-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x26_P2.54mm" (layer "F.Cu")
    (at 119.38 27.94 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x26, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J69" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x26_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 0 -33.02 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_14") (pintype "passive") (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 0 -35.56 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_15") (pintype "passive") (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 0 -38.1 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_16") (pintype "passive") (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 0 -40.64 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_17") (pintype "passive") (thermal_bridge_angle 45))
    (pad "18" smd roundrect (at 0 -43.18 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_18") (pintype "passive") (thermal_bridge_angle 45))
    (pad "19" smd roundrect (at 0 -45.72 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_19") (pintype "passive") (thermal_bridge_angle 45))
    (pad "20" smd roundrect (at 0 -48.26 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_20") (pintype "passive") (thermal_bridge_angle 45))
    (pad "21" smd roundrect (at 0 -50.8 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_21") (pintype "passive") (thermal_bridge_angle 45))
    (pad "22" smd roundrect (at 0 -53.34 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_22") (pintype "passive") (thermal_bridge_angle 45))
    (pad "23" smd roundrect (at 0 -55.88 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_23") (pintype "passive") (thermal_bridge_angle 45))
    (pad "24" smd roundrect (at 0 -58.42 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_24") (pintype "passive") (thermal_bridge_angle 45))
    (pad "25" smd roundrect (at 0 -60.96 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_25") (pintype "passive") (thermal_bridge_angle 45))
    (pad "26" smd roundrect (at 0 -63.5 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J69-Pin_1)") (pinfunction "Pin_26") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 99.71 99.06 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP4" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 30 "Net-(J38-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 35.56 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J44" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(J44-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 93.98 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J35" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J35-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 48.26 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J17" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J17-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x09_P2.54mm" (layer "F.Cu")
    (at 76.2 27.94 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x09, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J5" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x09_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 81.28 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J30" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(J30-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad" (layer "F.Cu")
    (at 119.38 96.52)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 91.44 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J66" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J66-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 30.48 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J42" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J42-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 63.5 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J55" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(J55-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 38.1 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J13" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 96.52 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J36" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J36-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 22.86 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J39" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(J39-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)" (layer "F.Cu")
    (at 77.438 54.61 -90)
    (property "MANUFACTURER" "JST")
    (property "STANDARD" "Manufacturer recommendations")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.545095 -1.767685 -90) (layer "F.SilkS") hide)
    (fp_text value "SM04B-SRSS-TB(LF)(SN)" (at 12.17039 5.74055 -90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -0.5 0 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/VDD") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0.5 0 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/SCA") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at 1.5 0 270) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SCL") (pinfunction "4") (pintype "passive"))
    (pad "S1" smd rect (at -2.8 3.875 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" smd rect (at 2.8 3.875 270) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
      (offset (xyz 0 -0.5 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 38.1 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J45" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J45-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x09_P2.54mm" (layer "F.Cu")
    (at 78.74 27.94 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x09, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J3" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x09_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 78.74 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J61" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J61-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad" (layer "F.Cu")
    (at 119.38 22.86)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 114.92 99.06)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP6" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 70 "Net-(J70-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 58.42 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J53" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(J53-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 25.4 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J8" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J8-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 95.87 99.06)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 29 "Net-(J37-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 66.04 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J56" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(J56-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x30_P2.54mm" (layer "F.Cu")
    (at 99.06 96.52)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x30, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J38" (at 0 2.54 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x30_Socket" (at 0 4.04 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
    (pad "14" smd roundrect (at 0 -33.02) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_14") (pintype "passive") (thermal_bridge_angle 45))
    (pad "15" smd roundrect (at 0 -35.56) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_15") (pintype "passive") (thermal_bridge_angle 45))
    (pad "16" smd roundrect (at 0 -38.1) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_16") (pintype "passive") (thermal_bridge_angle 45))
    (pad "17" smd roundrect (at 0 -40.64) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_17") (pintype "passive") (thermal_bridge_angle 45))
    (pad "18" smd roundrect (at 0 -43.18) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_18") (pintype "passive") (thermal_bridge_angle 45))
    (pad "19" smd roundrect (at 0 -45.72) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_19") (pintype "passive") (thermal_bridge_angle 45))
    (pad "20" smd roundrect (at 0 -48.26) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_20") (pintype "passive") (thermal_bridge_angle 45))
    (pad "21" smd roundrect (at 0 -50.8) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_21") (pintype "passive") (thermal_bridge_angle 45))
    (pad "22" smd roundrect (at 0 -53.34) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_22") (pintype "passive") (thermal_bridge_angle 45))
    (pad "23" smd roundrect (at 0 -55.88) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_23") (pintype "passive") (thermal_bridge_angle 45))
    (pad "24" smd roundrect (at 0 -58.42) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_24") (pintype "passive") (thermal_bridge_angle 45))
    (pad "25" smd roundrect (at 0 -60.96) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_25") (pintype "passive") (thermal_bridge_angle 45))
    (pad "26" smd roundrect (at 0 -63.5) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_26") (pintype "passive") (thermal_bridge_angle 45))
    (pad "27" smd roundrect (at 0 -66.04) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_27") (pintype "passive") (thermal_bridge_angle 45))
    (pad "28" smd roundrect (at 0 -68.58) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_28") (pintype "passive") (thermal_bridge_angle 45))
    (pad "29" smd roundrect (at 0 -71.12) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_29") (pintype "passive") (thermal_bridge_angle 45))
    (pad "30" smd roundrect (at 0 -73.66) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(J38-Pin_1)") (pinfunction "Pin_30") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 35.56 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J12" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J12-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 43.18 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J15" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J15-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 93.98 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J67" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J67-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 76.2 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J28" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(J28-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 68.58 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J25" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J25-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 27.94 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J41" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J41-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 33.02 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J43" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(J43-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 43.18 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J47" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(J47-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 40.64 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J46" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(J46-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 33.02 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J11" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 48.26 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J49" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J49-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 68.58 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J57" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(J57-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 121.92 92.06 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP5" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 69 "Net-(J69-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 60.96 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J22" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(J22-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 83.82 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J31" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(J31-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 60.96 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J54" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(J54-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x04_P2.54mm" (layer "F.Cu")
    (at 81.28 50.8 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/VDD") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/SCA") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 86.36 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J64" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J64-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 78.74 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J29" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(J29-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad" (layer "F.Cu")
    (at 76.2 22.86)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 40.64 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J14" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J14-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 96.52 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J68" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J68-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x05_P2.54mm" (layer "F.Cu")
    (at 83.82 50.8 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J18" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J18-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J18-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J18-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J18-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J18-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad" (layer "F.Cu")
    (at 76.2 96.52)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.25) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.5 4.5) (drill 2.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 91.44 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J34" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(J34-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 71.12 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J26" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(J26-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 88.9 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J33" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J33-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 73.66 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J27" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(J27-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 45.72 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J16" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J16-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x05_P2.54mm" (layer "F.Cu")
    (at 83.82 55.88 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J20" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J20-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J20-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J20-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J20-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(J20-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 45.72 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J48" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(J48-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 83.82 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J63" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J63-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 81.28 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J62" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J62-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 71.12 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J58" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(J58-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 80.66 99.06 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 180) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 41 "Net-(J3-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 86.36 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J32" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(J32-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 30.48 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J10" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J10-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x13_P2.54mm" (layer "F.Cu")
    (at 78.74 60.96 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x13, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J4" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x13_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J3-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 53.34 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J51" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(J51-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 22.86 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J7" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J7-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 25.4 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J40" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J40-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x05_P2.54mm" (layer "F.Cu")
    (at 83.82 58.42 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J21" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J21-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J21-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J21-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J21-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J21-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 81.28 63.5 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J23" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J23-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 55.88 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J52" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(J52-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 50.8 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J50" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(J50-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 88.9 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J65" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J65-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x13_P2.54mm" (layer "F.Cu")
    (at 76.2 60.96 180)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x13, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J6" (at 0 2.54 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x13_Socket" (at 0 4.04 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 180 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
    (pad "7" smd roundrect (at 0 -15.24 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_angle 45))
    (pad "8" smd roundrect (at 0 -17.78 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_8") (pintype "passive") (thermal_bridge_angle 45))
    (pad "9" smd roundrect (at 0 -20.32 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_9") (pintype "passive") (thermal_bridge_angle 45))
    (pad "10" smd roundrect (at 0 -22.86 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_10") (pintype "passive") (thermal_bridge_angle 45))
    (pad "11" smd roundrect (at 0 -25.4 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_11") (pintype "passive") (thermal_bridge_angle 45))
    (pad "12" smd roundrect (at 0 -27.94 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_12") (pintype "passive") (thermal_bridge_angle 45))
    (pad "13" smd roundrect (at 0 -30.48 180) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J5-Pin_1)") (pinfunction "Pin_13") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x05_P2.54mm" (layer "F.Cu")
    (at 83.82 53.34 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x05, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J19" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J19-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J19-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J19-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J19-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J19-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Proto:Proto_1x06_P2.54mm" (layer "F.Cu")
    (at 101.6 76.2 -90)
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J60" (at 0 2.54 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x06_Socket" (at 0 4.04 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.54 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at 0 0 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 0 -2.54 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at 0 -5.08 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_3") (pintype "passive") (thermal_bridge_angle 45))
    (pad "4" smd roundrect (at 0 -7.62 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_angle 45))
    (pad "5" smd roundrect (at 0 -10.16 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_5") (pintype "passive") (thermal_bridge_angle 45))
    (pad "6" smd roundrect (at 0 -12.7 270) (size 1.9 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J60-Pin_1)") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 73.66 92.06 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "project-protoboard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -1.8 90) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 42 "Net-(J5-Pin_1)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (gr_arc (start 123.19 96.52) (mid 122.074077 99.214077) (end 119.38 100.33)
    (layer "Edge.Cuts"))
  (gr_line (start 123.19 96.52) (end 123.19 22.86)
    (layer "Edge.Cuts"))
  (gr_line (start 72.39 22.86) (end 72.39 96.52)
    (layer "Edge.Cuts"))
  (gr_line (start 119.38 19.05) (end 76.2 19.05)
    (layer "Edge.Cuts"))
  (gr_line (start 76.2 100.33) (end 119.38 100.33)
    (layer "Edge.Cuts"))
  (gr_arc (start 119.38 19.05) (mid 122.074077 20.165923) (end 123.19 22.86)
    (layer "Edge.Cuts"))
  (gr_arc (start 76.2 100.33) (mid 73.505923 99.214077) (end 72.39 96.52)
    (layer "Edge.Cuts"))
  (gr_arc (start 72.39 22.86) (mid 73.505923 20.165923) (end 76.2 19.05)
    (layer "Edge.Cuts"))
  (gr_text "A" (at 78.994 56.642) (layer "F.SilkS"))
  (gr_text "Connect to" (at 84.582 99.568) (layer "F.SilkS"))
  (gr_text "+" (at 78.74 53.848) (layer "F.SilkS"))
  (gr_text "GND" (at 77.113 51.308) (layer "F.SilkS"))
  (gr_text "${version}" (at 122.174 87.63 90) (layer "F.SilkS"))
  (gr_text "SCL" (at 77.216 59.182) (layer "F.SilkS"))
  (gr_text "backplane" (at 102.616 99.568) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 72.39 100.33)
        (xy 72.39 19.05)
        (xy 123.19 19.05)
        (xy 123.19 100.33)
      )
    )
  )
)
