<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="20.32" x2="0" y2="0.02" width="0" layer="20"/>
<wire x1="0" y1="0.02" x2="112.7" y2="0.02" width="0" layer="20"/>
<wire x1="112.7" y1="0.02" x2="112.7" y2="20.32" width="0" layer="20"/>
<wire x1="112.7" y1="20.32" x2="0" y2="20.32" width="0" layer="20"/>
<hole x="2.54" y="17.78" drill="2.8"/>
<hole x="2.54" y="3.81" drill="2.8"/>
<hole x="110.49" y="17.78" drill="2.8"/>
<hole x="110.49" y="2.54" drill="2.8"/>
<text>GND</text>
<text>+5V</text>
<text>DAT</text>
<text>dunkyoung10@gmail.com</text>
<text>dunkyoung10@gmail.com</text>
<text>Trinket Stick</text>
<text>Duncan Young</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="todstuffnew">
<packages>
<package name="QFN16_4X4">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP11SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
<library name="OPL Eagle Library">
<packages>
<package name="B-SMD-5P">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH-SMD-RIGHT-ANGLE">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="todstuffnew" package="QFN16_4X4" value="PIC16F1455ML">
<attribute name="NAME"/>
</element>
<element name="C2" library="rcl" package="C0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0603" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="testpad" package="TP11SQ" value="TPTP11SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L2" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L7" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L8" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L9" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L10" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="J1" library="OPL Eagle Library" package="B-SMD-5P" value="MICRO-USB-5P-340015001">
<attribute name="NAME"/>
</element>
<element name="L3" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L4" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L5" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L6" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L11" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L12" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L13" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L14" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="R2" library="rcl" package="R0603" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0603" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0603" value="0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STRIP0" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="STRIP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="L15" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L16" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="C18" library="rcl" package="C0603" value="100nF"/>
<element name="C19" library="rcl" package="C0603" value="100nF"/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE_SWITCH-SMD-RIGHT-ANGLE" value="bootload">
<attribute name="PROD_ID" value="COMP-12265"/>
</element>
<element name="R5" library="rcl" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="bootload">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="F1" library="SparkFun-PowerIC" package="0603" value="PTC0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="L2" pad="3-GND"/>
<contactref element="L1" pad="3-GND"/>
<contactref element="L8" pad="3-GND"/>
<contactref element="L7" pad="3-GND"/>
<contactref element="L10" pad="3-GND"/>
<contactref element="L9" pad="3-GND"/>
<contactref element="J1" pad="5"/>
<contactref element="L4" pad="3-GND"/>
<contactref element="L3" pad="3-GND"/>
<contactref element="L6" pad="3-GND"/>
<contactref element="L5" pad="3-GND"/>
<contactref element="L12" pad="3-GND"/>
<contactref element="L11" pad="3-GND"/>
<contactref element="L14" pad="3-GND"/>
<contactref element="L13" pad="3-GND"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="STRIP0" pad="3"/>
<contactref element="STRIP1" pad="3"/>
<contactref element="L16" pad="3-GND"/>
<contactref element="L15" pad="3-GND"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="D+">
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="D-">
<contactref element="U1" pad="11"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="16"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="1-VDD"/>
<contactref element="L2" pad="1-VDD"/>
<contactref element="L7" pad="1-VDD"/>
<contactref element="L8" pad="1-VDD"/>
<contactref element="L9" pad="1-VDD"/>
<contactref element="L10" pad="1-VDD"/>
<contactref element="L3" pad="1-VDD"/>
<contactref element="L4" pad="1-VDD"/>
<contactref element="L5" pad="1-VDD"/>
<contactref element="L6" pad="1-VDD"/>
<contactref element="L11" pad="1-VDD"/>
<contactref element="L12" pad="1-VDD"/>
<contactref element="L13" pad="1-VDD"/>
<contactref element="L14" pad="1-VDD"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="STRIP0" pad="2"/>
<contactref element="STRIP1" pad="2"/>
<contactref element="L15" pad="1-VDD"/>
<contactref element="L16" pad="1-VDD"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="VPP">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="P1" pad="TP"/>
</signal>
<signal name="VUSB3V3">
<contactref element="U1" pad="10"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="PGD">
<contactref element="U1" pad="9"/>
</signal>
<signal name="PGC">
<contactref element="U1" pad="8"/>
</signal>
<signal name="DI">
<contactref element="U1" pad="7"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="L2" pad="4-DIN"/>
<contactref element="L1" pad="2-DOUT"/>
</signal>
<signal name="N$5">
<contactref element="L8" pad="4-DIN"/>
<contactref element="L7" pad="2-DOUT"/>
</signal>
<signal name="N$6">
<contactref element="L10" pad="4-DIN"/>
<contactref element="L9" pad="2-DOUT"/>
</signal>
<signal name="N$7">
<contactref element="L9" pad="4-DIN"/>
<contactref element="L8" pad="2-DOUT"/>
</signal>
<signal name="N$1">
<contactref element="L4" pad="4-DIN"/>
<contactref element="L3" pad="2-DOUT"/>
</signal>
<signal name="N$3">
<contactref element="L6" pad="4-DIN"/>
<contactref element="L5" pad="2-DOUT"/>
</signal>
<signal name="N$4">
<contactref element="L5" pad="4-DIN"/>
<contactref element="L4" pad="2-DOUT"/>
</signal>
<signal name="DO3">
<contactref element="L11" pad="4-DIN"/>
<contactref element="L10" pad="2-DOUT"/>
</signal>
<signal name="N$8">
<contactref element="L12" pad="4-DIN"/>
<contactref element="L11" pad="2-DOUT"/>
</signal>
<signal name="N$9">
<contactref element="L14" pad="4-DIN"/>
<contactref element="L13" pad="2-DOUT"/>
</signal>
<signal name="N$10">
<contactref element="L13" pad="4-DIN"/>
<contactref element="L12" pad="2-DOUT"/>
</signal>
<signal name="DO2">
<contactref element="L7" pad="4-DIN"/>
<contactref element="L6" pad="2-DOUT"/>
</signal>
<signal name="DO1">
<contactref element="L2" pad="2-DOUT"/>
<contactref element="L3" pad="4-DIN"/>
</signal>
<signal name="N$11">
<contactref element="L1" pad="4-DIN"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="2"/>
<contactref element="STRIP0" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="2"/>
<contactref element="STRIP1" pad="1"/>
</signal>
<signal name="DOUT">
<contactref element="R4" pad="1"/>
<contactref element="L16" pad="2-DOUT"/>
</signal>
<signal name="N$14">
<contactref element="L16" pad="4-DIN"/>
<contactref element="L15" pad="2-DOUT"/>
</signal>
<signal name="N$15">
<contactref element="L14" pad="2-DOUT"/>
<contactref element="L15" pad="4-DIN"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="6"/>
</signal>
<signal name="BOOTSW">
<contactref element="U1" pad="5"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="BOOTLED">
<contactref element="U1" pad="4"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="VUSB">
<contactref element="J1" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
