<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.254" x2="53.01" y2="-0.254" width="0.254" layer="20"/>
<wire x1="53.01" y1="-0.254" x2="53.01" y2="38.344" width="0.254" layer="20"/>
<wire x1="53.01" y1="38.344" x2="0" y2="38.344" width="0.254" layer="20"/>
<wire x1="0" y1="38.344" x2="0" y2="-0.254" width="0.254" layer="20"/>
<hole x="4.572" y="3.048" drill="2.8"/>
<hole x="4.572" y="35.052" drill="2.8"/>
<text>+</text>
<text>-</text>
<text>Red</text>
<text>Yel</text>
<text>Grn</text>
<text>Blu</text>
<text>Dischg</text>
<text>Float</text>
<text>Normal</text>
<text>Bulk</text>
<text>Reset</text>
<text>RV-Project.Com Charge State 
       Monitor V1.4</text>
<text>Euro</text>
<text>Kf7.62</text>
<text>Calibrate</text>
<text>Power</text>
<text>CAL</text>
<hole x="48.006" y="35.052" drill="2.8"/>
<hole x="48.006" y="3.048" drill="2.8"/>
<text>+</text>
<text>-</text>
<text>Board Clearance</text>
<text>Switch Centers</text>
<text>Mounting Holes</text>
<text>Bord Width</text>
<text>Switch/LED 
Centers</text>
<text>Switch/LED 
Centers</text>
<text>Switch/Mounting
Centers</text>
<text>Switch/Mounting
Centers</text>
<text>Collar</text>
<text>Switch Length (Actuated)</text>
<text>200MSP1T2B2M6</text>
<text>GND</text>
<text>Rev A</text>
<text>3/18/2018</text>
</plain>
<libraries>
<library name="alsstuff">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="GENERIC_0100_DEVICE_150_SPACING">
<description>&lt;h3&gt;Ceramic Capacitor&lt;/h3&gt;
Commonly used for small ceramic capacitors 0150 spacing.</description>
</package>
<package name="DIODE-ZENER">
</package>
<package name="1/4W_AXIAL">
<description>Standard Axial 1/4Watt Resistor&lt;p&gt;0.45" footprint</description>
</package>
<package name="BOURNS3296_W">
<description>Precisoin Trimmer 10turn

&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/54/3296-52802.pdf"&gt;Data Sheet&lt;/a&gt;</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="COMBOCONNECTOR">
</package>
<package name="ESWITCH800S">
</package>
<package name="ESWITCH200A">
</package>
<package name="CHINESE_TEST_PIN">
</package>
<package name="CREATIVECOMMONS">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="alsstuff" package="RADIAL_ELECTROLYTIC_100MIL" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C2" library="alsstuff" package="RADIAL_ELECTROLYTIC_100MIL" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C3" library="alsstuff" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C4" library="alsstuff" package="GENERIC_0100_DEVICE_150_SPACING" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="D1" library="alsstuff" package="DIODE-ZENER" value="11v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="TO92" value="78L05Z">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="alsstuff" package="COMBOCONNECTOR" value="COMBOCONN">
<attribute name="NAME"/>
</element>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="a-lib" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="a-lib" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="alsstuff" package="1/4W_AXIAL" value="330">
<attribute name="NAME"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="R2" library="alsstuff" package="1/4W_AXIAL" value="220">
<attribute name="NAME"/>
<attribute name="VALUE" value="220"/>
</element>
<element name="R3" library="alsstuff" package="1/4W_AXIAL" value="3.3K">
<attribute name="NAME"/>
<attribute name="VALUE" value="3.3K"/>
</element>
<element name="R4" library="alsstuff" package="1/4W_AXIAL" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE" value="1K"/>
</element>
<element name="R5" library="alsstuff" package="1/4W_AXIAL" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="alsstuff" package="BOURNS3296_W" value="5k">
<attribute name="MARKING" value="5k"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="5k"/>
</element>
<element name="U1" library="alsstuff" package="DIP08" value="TINY85-20-DIP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09445"/>
</element>
<element name="R7" library="alsstuff" package="1/4W_AXIAL" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE" value="22K"/>
</element>
<element name="S2" library="alsstuff" package="ESWITCH800S" value="ESWITCH800S">
<attribute name="NAME"/>
</element>
<element name="S1" library="alsstuff" package="ESWITCH200A" value="ESWITCH200A">
<attribute name="NAME"/>
</element>
<element name="TP1" library="alsstuff" package="CHINESE_TEST_PIN" value="CHINESE_TEST_PIN">
<attribute name="NAME"/>
</element>
<element name="TP2" library="alsstuff" package="CHINESE_TEST_PIN" value="CHINESE_TEST_PIN">
<attribute name="NAME"/>
</element>
<element name="U$1" library="alsstuff" package="CREATIVECOMMONS" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="1A"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="2A"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="P$2"/>
<contactref element="S1" pad="C"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="3"/>
<contactref element="R6" pad="2"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="5"/>
<contactref element="LED1" pad="K"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="6"/>
<contactref element="LED2" pad="K"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="7"/>
<contactref element="LED3" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="2"/>
<contactref element="LED4" pad="K"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
