(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 89)
    (tracks 153)
    (zones 0)
    (modules 3)
    (nets 39)
  )
  (page A4)
  (title_block
    (date 2019-05-16)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.45)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.1016)
    (solder_mask_min_width 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad19)")
  (net 2 "Net-(J1-Pad18)")
  (net 3 "Net-(J1-Pad17)")
  (net 4 "Net-(J1-Pad16)")
  (net 5 "Net-(J1-Pad15)")
  (net 6 "Net-(J1-Pad14)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad12)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad8)")
  (net 13 "Net-(J1-Pad7)")
  (net 14 "Net-(J1-Pad6)")
  (net 15 "Net-(J1-Pad5)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad2)")
  (net 19 "Net-(J1-Pad1)")
  (net 20 "Net-(J2-Pad2)")
  (net 21 "Net-(J2-Pad4)")
  (net 22 "Net-(J2-Pad6)")
  (net 23 "Net-(J2-Pad8)")
  (net 24 "Net-(J2-Pad10)")
  (net 25 "Net-(J2-Pad12)")
  (net 26 "Net-(J2-Pad14)")
  (net 27 "Net-(J2-Pad16)")
  (net 28 "Net-(J2-Pad18)")
  (net 29 "Net-(J2-Pad20)")
  (net 30 "Net-(J2-Pad22)")
  (net 31 "Net-(J2-Pad24)")
  (net 32 "Net-(J2-Pad26)")
  (net 33 "Net-(J2-Pad28)")
  (net 34 "Net-(J2-Pad30)")
  (net 35 "Net-(J2-Pad32)")
  (net 36 "Net-(J2-Pad34)")
  (net 37 "Net-(J2-Pad36)")
  (net 38 "Net-(J2-Pad38)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x19_P2.54mm_Vertical (layer F.Cu) (tedit 5CDE132A)
    (at 147.975 61.515001)
    (descr "Through hole straight socket strip, 2x19, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x19 2.54mm double row")
    (fp_text reference J2 (at -1.036 -4.365001) (layer F.SilkS) hide)
    (fp_text value Conn_02x19_Odd_Even (at -1.27 48.49) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 22.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 18 thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 20 thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 22 thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 24 thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 26 thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 28 thru_hole oval (at -2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 30 thru_hole oval (at -2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 32 thru_hole oval (at -2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 34 thru_hole oval (at -2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 36 thru_hole oval (at -2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 38 thru_hole oval (at -2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad38)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x19_P2.54mm_Vertical locked (layer B.Cu) (tedit 5CDE12B3)
    (at 151.13 61.515001 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J3 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x19 (at 0 -48.05) (layer B.Fab) hide)
    (fp_text user %R (at 0 -22.86 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad6)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad8)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad10)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad12)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad14)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad16)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad18)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad20)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad22)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad24)"))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad26)"))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad28)"))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad30)"))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad32)"))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad34)"))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad36)"))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad38)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x19_P2.54mm_Vertical (layer B.Cu) (tedit 5CDE1269)
    (at 158.75 61.515001 180)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS) hide)
    (fp_text value Conn_01x19 (at 0 -48.05 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 -22.86 90) (layer B.Fab))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Use extra long male pin header. \nTypical mating post length is 5.84mm.\nBreadboard hole is about 9mm deep so mating \nsection of post must be longer than that." (at 176.4665 58.547) (layer Cmts.User))
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "300 mils" (at 154.94 111.663) (layer Dwgs.User))
    (feature1 (pts (xy 158.75 107.2515) (xy 158.75 110.949421)))
    (feature2 (pts (xy 151.13 107.2515) (xy 151.13 110.949421)))
    (crossbar (pts (xy 151.13 110.363) (xy 158.75 110.363)))
    (arrow1a (pts (xy 158.75 110.363) (xy 157.623496 110.949421)))
    (arrow1b (pts (xy 158.75 110.363) (xy 157.623496 109.776579)))
    (arrow2a (pts (xy 151.13 110.363) (xy 152.256504 110.949421)))
    (arrow2b (pts (xy 151.13 110.363) (xy 152.256504 109.776579)))
  )
  (gr_text - (at 152.527 107.188) (layer B.SilkS))
  (gr_text - (at 152.527 104.648) (layer B.SilkS))
  (gr_text C4 (at 152.527 102.108) (layer B.SilkS))
  (gr_text AGND (at 152.527 99.568) (layer B.SilkS))
  (gr_text B13 (at 152.527 97.028) (layer B.SilkS))
  (gr_text B14 (at 152.527 94.488) (layer B.SilkS))
  (gr_text B15 (at 152.527 91.948) (layer B.SilkS))
  (gr_text B1 (at 152.527 89.408) (layer B.SilkS))
  (gr_text B2 (at 152.527 86.868) (layer B.SilkS))
  (gr_text GND (at 152.527 84.328) (layer B.SilkS))
  (gr_text B11 (at 152.527 81.788) (layer B.SilkS))
  (gr_text B12 (at 152.527 79.248) (layer B.SilkS))
  (gr_text A11 (at 152.527 76.708) (layer B.SilkS))
  (gr_text A12 (at 152.527 74.168) (layer B.SilkS))
  (gr_text - (at 152.527 71.628) (layer B.SilkS))
  (gr_text U5V (at 152.527 69.088) (layer B.SilkS))
  (gr_text C5 (at 152.527 66.548) (layer B.SilkS))
  (gr_text C6 (at 152.527 64.008) (layer B.SilkS))
  (gr_text C8 (at 152.527 61.468) (layer B.SilkS))
  (gr_text A3 (at 157.353 107.188) (layer B.SilkS))
  (gr_text A2 (at 157.353 104.648) (layer B.SilkS))
  (gr_text A10 (at 157.353 102.108) (layer B.SilkS))
  (gr_text B3 (at 157.353 99.568) (layer B.SilkS))
  (gr_text B5 (at 157.353 97.028) (layer B.SilkS))
  (gr_text B4 (at 157.353 94.488) (layer B.SilkS))
  (gr_text B10 (at 157.353 92.0115) (layer B.SilkS))
  (gr_text A8 (at 157.353 89.408) (layer B.SilkS))
  (gr_text A9 (at 157.353 86.868) (layer B.SilkS))
  (gr_text C7 (at 157.353 84.328) (layer B.SilkS))
  (gr_text B6 (at 157.353 81.788) (layer B.SilkS))
  (gr_text A7 (at 157.353 79.248) (layer B.SilkS))
  (gr_text A6 (at 157.353 76.708) (layer B.SilkS))
  (gr_text A5 (at 157.353 74.168) (layer B.SilkS))
  (gr_text GND (at 157.353 71.628) (layer B.SilkS))
  (gr_text AVdd (at 157.353 69.088) (layer B.SilkS))
  (gr_text C0/B8 (at 157.607 107.188) (layer F.SilkS))
  (gr_text C1/B9 (at 157.607 104.648) (layer F.SilkS))
  (gr_text B0 (at 157.607 102.108) (layer F.SilkS))
  (gr_text A4 (at 157.607 99.568) (layer F.SilkS))
  (gr_text A1 (at 157.607 97.028) (layer F.SilkS))
  (gr_text A0 (at 157.607 94.488) (layer F.SilkS))
  (gr_text - (at 157.607 91.948) (layer F.SilkS))
  (gr_text Vin (at 157.607 89.408) (layer F.SilkS))
  (gr_text GND (at 157.607 86.868) (layer F.SilkS))
  (gr_text GND (at 157.607 84.328) (layer F.SilkS))
  (gr_text 5v (at 157.607 81.788) (layer F.SilkS))
  (gr_text 3v3 (at 157.607 79.248) (layer F.SilkS))
  (gr_text ~RST~ (at 157.607 76.708) (layer F.SilkS))
  (gr_text IOref (at 157.607 74.168) (layer F.SilkS))
  (gr_text - (at 157.607 71.628) (layer F.SilkS))
  (gr_text GND (at 157.607 69.088) (layer F.SilkS))
  (gr_text E5V (at 157.607 66.548) (layer F.SilkS))
  (gr_text D2 (at 157.607 64.008) (layer F.SilkS))
  (gr_text C11 (at 157.607 61.468) (layer F.SilkS))
  (gr_text B9 (at 157.353 66.548) (layer B.SilkS))
  (gr_text B8 (at 157.353 64.008) (layer B.SilkS))
  (gr_text C9 (at 157.353 61.468) (layer B.SilkS))
  (dimension 3.155 (width 0.15) (layer Dwgs.User)
    (gr_text "3.155 mm" (at 149.5525 57.374) (layer Dwgs.User))
    (feature1 (pts (xy 151.13 61.515001) (xy 151.13 58.087579)))
    (feature2 (pts (xy 147.975 61.515001) (xy 147.975 58.087579)))
    (crossbar (pts (xy 147.975 58.674) (xy 151.13 58.674)))
    (arrow1a (pts (xy 151.13 58.674) (xy 150.003496 59.260421)))
    (arrow1b (pts (xy 151.13 58.674) (xy 150.003496 58.087579)))
    (arrow2a (pts (xy 147.975 58.674) (xy 149.101504 59.260421)))
    (arrow2b (pts (xy 147.975 58.674) (xy 149.101504 58.087579)))
  )
  (gr_text C3 (at 152.4 107.188) (layer F.SilkS))
  (gr_text C2 (at 152.4 104.648) (layer F.SilkS))
  (gr_text Vbat (at 152.4 102.108) (layer F.SilkS))
  (gr_text H1 (at 152.4 99.568) (layer F.SilkS))
  (gr_text H0 (at 152.4 97.028) (layer F.SilkS))
  (gr_text C15 (at 152.4 94.488) (layer F.SilkS))
  (gr_text C14 (at 152.4 91.948) (layer F.SilkS))
  (gr_text C13 (at 152.4 89.408) (layer F.SilkS))
  (gr_text B7 (at 152.4 86.868) (layer F.SilkS))
  (gr_text GND (at 152.4 84.328) (layer F.SilkS))
  (gr_text A15 (at 152.4 81.788) (layer F.SilkS))
  (gr_text A14 (at 152.4 79.248) (layer F.SilkS))
  (gr_text A13 (at 152.4 76.708) (layer F.SilkS))
  (gr_text - (at 152.4 74.168) (layer F.SilkS))
  (gr_text - (at 152.4 71.628) (layer F.SilkS))
  (gr_text Boot0 (at 152.4 69.088) (layer F.SilkS))
  (gr_text VDD (at 152.4 66.548) (layer F.SilkS))
  (gr_text C12 (at 152.4 64.008) (layer F.SilkS))
  (gr_text C10 (at 152.4 61.468) (layer F.SilkS))
  (dimension 49.784 (width 0.15) (layer Dwgs.User)
    (gr_text "49.784 mm" (at 166.273 84.328 270) (layer Dwgs.User))
    (feature1 (pts (xy 159.258 109.22) (xy 165.559421 109.22)))
    (feature2 (pts (xy 159.258 59.436) (xy 165.559421 59.436)))
    (crossbar (pts (xy 164.973 59.436) (xy 164.973 109.22)))
    (arrow1a (pts (xy 164.973 109.22) (xy 164.386579 108.093496)))
    (arrow1b (pts (xy 164.973 109.22) (xy 165.559421 108.093496)))
    (arrow2a (pts (xy 164.973 59.436) (xy 164.386579 60.562504)))
    (arrow2b (pts (xy 164.973 59.436) (xy 165.559421 60.562504)))
  )
  (dimension 17.78 (width 0.15) (layer Dwgs.User)
    (gr_text "17.78 mm" (at 152.019 54.453) (layer Dwgs.User))
    (feature1 (pts (xy 160.909 60.579) (xy 160.909 55.166579)))
    (feature2 (pts (xy 143.129 60.579) (xy 143.129 55.166579)))
    (crossbar (pts (xy 143.129 55.753) (xy 160.909 55.753)))
    (arrow1a (pts (xy 160.909 55.753) (xy 159.782496 56.339421)))
    (arrow1b (pts (xy 160.909 55.753) (xy 159.782496 55.166579)))
    (arrow2a (pts (xy 143.129 55.753) (xy 144.255504 56.339421)))
    (arrow2b (pts (xy 143.129 55.753) (xy 144.255504 55.166579)))
  )
  (gr_arc (start 160.02 60.198) (end 160.782 60.198) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 160.02 108.458) (end 160.02 109.22) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.018 108.458) (end 143.256 108.458) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.018 59.436) (end 160.02 59.436) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 144.018 60.198) (end 144.018 59.436) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.256 108.458) (end 143.256 60.198) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.02 109.22) (end 144.018 109.22) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.782 60.198) (end 160.782 108.458) (layer Edge.Cuts) (width 0.05))
)
