(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (color "Polyimide") (thickness 1.51) (material "Kapton") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.1016)
    (allow_soldermask_bridges_in_footprints yes)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(BT1-PadP1)")
  (net 3 "+3.3V")
  (net 4 "/INP_BTN")
  (net 5 "/LED_GREEN")
  (net 6 "Net-(D2-Pad5)")
  (net 7 "/LED_BLUE")
  (net 8 "unconnected-(U1-GND-Pad21)")
  (net 9 "GNDA")
  (net 10 "unconnected-(U1-VCM-Pad15)")
  (net 11 "unconnected-(U1-DRVN-Pad17)")
  (net 12 "unconnected-(U1-DRVP-Pad18)")
  (net 13 "/CS_SD")
  (net 14 "/MOSI_SD")
  (net 15 "/SCK_SD")
  (net 16 "/MISO_SD")
  (net 17 "/SD_Detect")
  (net 18 "/Pi_SD_CS")
  (net 19 "/Pi_SD_TX_MOSI")
  (net 20 "/Pi_SD_RX_MISO")
  (net 21 "/Pi_SD_SCK")
  (net 22 "/BATT_I{slash}P")
  (net 23 "/MUX_SEL")
  (net 24 "/ALERT_PMIC")
  (net 25 "/VBUS")
  (net 26 "/HUB_DETECT")
  (net 27 "/SDA_BMI270")
  (net 28 "/SCL_BMI270")
  (net 29 "/SCL_0")
  (net 30 "/SDA_0")
  (net 31 "/SCL_1")
  (net 32 "/SDA_1")
  (net 33 "/INT_RTC")
  (net 34 "/LED_RED")
  (net 35 "/VSYS")
  (net 36 "unconnected-(SW1-C-Pad3)")
  (net 37 "unconnected-(SW2-Pad1)")
  (net 38 "/RST_HW")
  (net 39 "unconnected-(SW2-Pad4)")
  (net 40 "unconnected-(SW3-Pad1)")
  (net 41 "unconnected-(SW3-Pad4)")
  (net 42 "/Pico_SPI0_SCK")
  (net 43 "/Pico_SPI0_TX")
  (net 44 "/Pico_SPI0_RX")
  (net 45 "/Pico_SPI0_CS")
  (net 46 "/Pico_SPI1_SCK")
  (net 47 "/Pico_SPI1_TX")
  (net 48 "/Pico_SPI1_RX")
  (net 49 "/Pico_SPI1_CS")
  (net 50 "/INT_BMI270")
  (net 51 "/CLKOUT_RTC")
  (net 52 "Net-(U2-CLKOE)")
  (net 53 "unconnected-(U6-GPIO15-Pad20)")
  (net 54 "unconnected-(J2-DAT2-PadP1)")
  (net 55 "unconnected-(J2-DAT1-PadP8)")
  (net 56 "Net-(U2-EVI)")
  (net 57 "unconnected-(U1-INT2B-Pad1)")
  (net 58 "unconnected-(U1-INTB-Pad2)")
  (net 59 "unconnected-(U1-PA10_A2_D2-Pad3)")
  (net 60 "unconnected-(U1-PA11_A3_D3-Pad4)")
  (net 61 "unconnected-(U1-PA8_A4_D4_SDA-Pad5)")
  (net 62 "unconnected-(U1-PA9_A5_D5_SCL-Pad6)")
  (net 63 "unconnected-(U1-PB08_A6_D6_TX-Pad7)")
  (net 64 "unconnected-(U1-5V-Pad14)")
  (net 65 "unconnected-(U1-1.8v-Pad16)")
  (net 66 "unconnected-(U3-ASDX-Pad2)")
  (net 67 "unconnected-(U3-ASCX-Pad3)")
  (net 68 "unconnected-(U3-INT2-Pad9)")
  (net 69 "unconnected-(U3-OSCB-Pad10)")
  (net 70 "unconnected-(U3-OSDO-Pad11)")
  (net 71 "/IR_OUT")
  (net 72 "unconnected-(U6-GND-Pad8)")
  (net 73 "unconnected-(U6-GND-Pad18)")
  (net 74 "unconnected-(U6-GND-Pad23)")
  (net 75 "unconnected-(U6-GPIO26_ADC0-Pad31)")
  (net 76 "unconnected-(U6-GPIO27_ADC1-Pad32)")
  (net 77 "unconnected-(U6-AGND-Pad33)")
  (net 78 "unconnected-(U6-ADC_VREF-Pad35)")
  (net 79 "unconnected-(U6-SWCLK-Pad41)")
  (net 80 "unconnected-(U6-SWDIO-Pad43)")
  (net 81 "unconnected-(a2-MP1-PadMOUNTING-HOLE)")
  (net 82 "unconnected-(a2-20-PadP$20)")
  (net 83 "unconnected-(a2-48-PadP$48)")
  (net 84 "unconnected-(a2-52-PadP$52)")
  (net 85 "unconnected-(a2-29-PadP$29)")
  (net 86 "unconnected-(J2-SHIELD-PadSH1)")
  (net 87 "unconnected-(a2-47-PadP$47)")
  (net 88 "unconnected-(a2-70-PadP$70)")
  (net 89 "unconnected-(U6-GND-Pad13)")
  (net 90 "unconnected-(a2-32-PadP$32)")
  (net 91 "unconnected-(a2-26-PadP$26)")
  (net 92 "unconnected-(U6-GND-Pad28)")
  (net 93 "unconnected-(a2-44-PadP$44)")
  (net 94 "unconnected-(a2-35-PadP$35)")
  (net 95 "unconnected-(a2-41-PadP$41)")
  (net 96 "unconnected-(a2-53-PadP$53)")
  (net 97 "Net-(U2-VDD)")
  (net 98 "unconnected-(U1-ECGP-Pad19)")
  (net 99 "unconnected-(U1-ECGN-Pad20)")
  (net 100 "unconnected-(a2-58-PadP$58)")
  (net 101 "unconnected-(a2-56-PadP$56)")
  (net 102 "unconnected-(a2-42-PadP$42)")
  (net 103 "unconnected-(a2-40-PadP$40)")
  (net 104 "unconnected-(a2-38-PadP$38)")
  (net 105 "unconnected-(a2-36-PadP$36)")
  (net 106 "unconnected-(a2-34-PadP$34)")
  (net 107 "unconnected-(a2-10-PadP$10)")
  (net 108 "unconnected-(a2-8-PadP$8)")
  (net 109 "unconnected-(a2-6-PadP$6)")
  (net 110 "unconnected-(a2-4-PadP$4)")
  (net 111 "unconnected-(a2-2-PadP$2)")
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 166.96 91.1925 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -2.5875 0.25 -180) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/SD_Detect") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 127.3875 63.05)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0.1425 -1.425) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SCL_0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 122 71.0625 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.4875 -0.05 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(U2-CLKOE)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "AAAF5060QBFSURZGS:LED_AAAF5060QBFSURZGS" (layer "F.Cu")
    (at 161.45 77.9 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/AAAF5060QBFSURZGS/Kingbright/view-part/?ref=eda")
    (property "Description" "\nRed, Green, Blue (RGB) 630nm Red, 525nm Green, 465nm Blue LED Indication - Discrete 1.9V Red, 3.3V Green, 3.3V Blue 6-SMD, J-Lead\n")
    (property "MANUFACTURER" "Kingbright")
    (property "MAXIMUM_PACKAGE_HEIGHT" "2.3 mm")
    (property "MF" "Kingbright")
    (property "MP" "AAAF5060QBFSURZGS")
    (property "PARTREV" "V.1")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=214595&manufacturer=Kingbright&part_name=AAAF5060QBFSURZGS&search_term=aaaf5060qbfsurzgs")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/AAAF5060QBFSURZGS/Kingbright/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "D2" (at -1.275 -4.085) (layer "F.SilkS"))
    (fp_text value "AAAF5060QBFSURZGS" (at 8.885 4.185) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.7 -2 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -2.7 0 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -2.7 2 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.7 2 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/LED_GREEN") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" smd rect (at 2.7 0 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(D2-Pad5)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" smd rect (at 2.7 -2 180) (size 3 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/LED_BLUE") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "BMI270:XDCR_BMI270" (layer "F.Cu")
    (at 154.308 69.4655)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/BMI270/Bosch+Sensortec/view-part/?ref=eda")
    (property "Description" "\nAccelerometer, Gyroscope, 6 Axis Sensor I²C, SPI Output\n")
    (property "MANUFACTURER" "Bosch Sensortec")
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.87mm")
    (property "MF" "Bosch Sensortec")
    (property "MP" "BMI270")
    (property "PATREV" "1.0")
    (property "Package" "LGA-14 Bosch Sensortec")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3595167&manufacturer=Bosch Sensortec&part_name=BMI270&search_term=bmi270")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/BMI270/Bosch+Sensortec/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "U3" (at -0.008 -2.0314) (layer "F.SilkS"))
    (fp_text value "BMI270" (at 2.4304 2.0314) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1625 -0.75) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "SDO") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -1.1625 -0.25) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "unconnected-(U3-ASDX-Pad2)") (pinfunction "ASDX") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -1.1625 0.25) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "unconnected-(U3-ASCX-Pad3)") (pinfunction "ASCX") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "4" smd rect (at -1.1625 0.75) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/INT_BMI270") (pinfunction "INT1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "5" smd rect (at -0.5 0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "VDDIO") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "6" smd rect (at 0 0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GNDIO") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "7" smd rect (at 0.5 0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "8" smd rect (at 1.1625 0.75) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "9" smd rect (at 1.1625 0.25) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "unconnected-(U3-INT2-Pad9)") (pinfunction "INT2") (pintype "bidirectional+no_connect") (solder_mask_margin 0.102))
    (pad "10" smd rect (at 1.1625 -0.25) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "unconnected-(U3-OSCB-Pad10)") (pinfunction "OSCB") (pintype "input+no_connect") (solder_mask_margin 0.102))
    (pad "11" smd rect (at 1.1625 -0.75) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "unconnected-(U3-OSDO-Pad11)") (pinfunction "OSDO") (pintype "output+no_connect") (solder_mask_margin 0.102))
    (pad "12" smd rect (at 0.5 -0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "CSB") (pintype "input") (solder_mask_margin 0.102))
    (pad "13" smd rect (at 0 -0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SCL_BMI270") (pinfunction "SCX") (pintype "input") (solder_mask_margin 0.102))
    (pad "14" smd rect (at -0.5 -0.9125 90) (size 0.475 0.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDA_BMI270") (pinfunction "SDX") (pintype "bidirectional") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 154.1375 76.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0.0125 1.45) (layer "F.SilkS"))
    (fp_text value "75R" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/LED_RED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D2-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 132.44 67.5945 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -2.2555 0.16 180) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/INP_BTN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PTS810_SJM_250_SMTR_LFS:SW_PTS810_SJM_250_SMTR_LFS" (layer "F.Cu")
    (at 118.345 63.137 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/PTS810%20SJM%20250%20SMTR%20LFS/C%2526K/view-part/?ref=eda")
    (property "Description" "\nTactile Switch SPST-NO Top Actuated Surface Mount\n")
    (property "MANUFACTURER" "CnK")
    (property "MF" "C&K")
    (property "MP" "PTS810 SJM 250 SMTR LFS")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=522770&manufacturer=C&amp;K&part_name=PTS810 SJM 250 SMTR LFS&search_term=None")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/PTS810%20SJM%20250%20SMTR%20LFS/C%2526K/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "SW2" (at 0.227 2.615) (layer "F.SilkS"))
    (fp_text value "PTS810_SJM_250_SMTR_LFS" (at 0 2.926) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(SW2-Pad1)") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/RST_HW") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(SW2-Pad4)") (pintype "passive+no_connect") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 144.4 64.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/SCL_0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "M.2-Templates:M.2-B-KEY" (layer "F.Cu")
    (at 125.14 86.54)
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "a2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "M.2-B+M-KEY" (at 0 0) (layer "F.SilkS") hide)
    (fp_line (start -38.64 -26.36) (end -38.64 19.64)
      (layer "Edge.Cuts"))
    (fp_line (start -38.14 20.14) (end 42.16 20.14)
      (layer "Edge.Cuts"))
    (fp_line (start 42.16 -26.86) (end -38.14 -26.86)
      (layer "Edge.Cuts"))
    (fp_line (start 42.36 -13.81) (end 42.36 -26.66)
      (layer "Edge.Cuts"))
    (fp_line (start 42.36 19.94) (end 42.36 7.09)
      (layer "Edge.Cuts"))
    (fp_line (start 42.86 6.59) (end 46.16 6.59)
      (layer "Edge.Cuts"))
    (fp_line (start 43.46 -9.56) (end 46.36 -9.56)
      (layer "Edge.Cuts"))
    (fp_line (start 43.46 -8.36) (end 46.36 -8.36)
      (layer "Edge.Cuts"))
    (fp_line (start 46.16 -13.31) (end 42.86 -13.31)
      (layer "Edge.Cuts"))
    (fp_line (start 46.36 -9.56) (end 46.36 -13.11)
      (layer "Edge.Cuts"))
    (fp_line (start 46.36 6.39) (end 46.36 -8.36)
      (layer "Edge.Cuts"))
    (fp_arc (start -38.64 -26.36) (mid -38.493553 -26.713553) (end -38.14 -26.86)
      (layer "Edge.Cuts"))
    (fp_arc (start -38.14 20.14) (mid -38.493553 19.993553) (end -38.64 19.64)
      (layer "Edge.Cuts"))
    (fp_arc (start 42.16 -26.86) (mid 42.301421 -26.801421) (end 42.36 -26.66)
      (layer "Edge.Cuts"))
    (fp_arc (start 42.36 7.09) (mid 42.506447 6.736447) (end 42.86 6.59)
      (layer "Edge.Cuts"))
    (fp_arc (start 42.36 19.94) (mid 42.301421 20.081421) (end 42.16 20.14)
      (layer "Edge.Cuts"))
    (fp_arc (start 42.86 -13.31) (mid 42.506447 -13.456447) (end 42.36 -13.81)
      (layer "Edge.Cuts"))
    (fp_arc (start 42.86 -8.96) (mid 43.035736 -9.384264) (end 43.46 -9.56)
      (layer "Edge.Cuts"))
    (fp_arc (start 43.46 -8.36) (mid 43.035736 -8.535736) (end 42.86 -8.96)
      (layer "Edge.Cuts"))
    (fp_arc (start 46.16 -13.31) (mid 46.301421 -13.251421) (end 46.36 -13.11)
      (layer "Edge.Cuts"))
    (fp_arc (start 46.36 6.39) (mid 46.301421 6.531421) (end 46.16 6.59)
      (layer "Edge.Cuts"))
    (pad "MOUNTING-HOLE" thru_hole circle (at -38.64 -3.36 90) (size 5.5 5.5) (drill 3.5) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(a2-MP1-PadMOUNTING-HOLE)") (pinfunction "MP1") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$1" smd rect (at 45.11 -12.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$2" smd rect (at 45.11 -12.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 111 "unconnected-(a2-2-PadP$2)") (pinfunction "2") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$3" smd rect (at 45.11 -12.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$4" smd rect (at 45.11 -11.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "unconnected-(a2-4-PadP$4)") (pinfunction "4") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$5" smd rect (at 45.11 -11.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "5") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$6" smd rect (at 45.11 -11.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "unconnected-(a2-6-PadP$6)") (pinfunction "6") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$7" smd rect (at 45.11 -11.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "7") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$8" smd rect (at 45.11 -10.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "unconnected-(a2-8-PadP$8)") (pinfunction "8") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$9" smd rect (at 45.11 -10.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "9") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$10" smd rect (at 45.11 -10.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "unconnected-(a2-10-PadP$10)") (pinfunction "10") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$11" smd rect (at 45.11 -10.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "11") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$20" smd rect (at 45.11 -7.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "unconnected-(a2-20-PadP$20)") (pinfunction "20") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$21" smd rect (at 45.11 -7.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "21") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$22" smd rect (at 45.11 -7.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/HUB_DETECT") (pinfunction "22") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$23" smd rect (at 45.11 -7.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "23") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$24" smd rect (at 45.11 -6.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/HUB_DETECT") (pinfunction "24") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$25" smd rect (at 45.11 -6.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "25") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$26" smd rect (at 45.11 -6.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "unconnected-(a2-26-PadP$26)") (pinfunction "26") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$27" smd rect (at 45.11 -6.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "27") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$28" smd rect (at 45.11 -5.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/ALERT_PMIC") (pinfunction "28") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$29" smd rect (at 45.11 -5.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "unconnected-(a2-29-PadP$29)") (pinfunction "29") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$30" smd rect (at 45.11 -5.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/ALERT_PMIC") (pinfunction "30") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$31" smd rect (at 45.11 -5.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/Pi_SD_SCK") (pinfunction "31") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$32" smd rect (at 45.11 -4.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "unconnected-(a2-32-PadP$32)") (pinfunction "32") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$33" smd rect (at 45.11 -4.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/Pi_SD_SCK") (pinfunction "33") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$34" smd rect (at 45.11 -4.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "unconnected-(a2-34-PadP$34)") (pinfunction "34") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$35" smd rect (at 45.11 -4.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(a2-35-PadP$35)") (pinfunction "35") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$36" smd rect (at 45.11 -3.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "unconnected-(a2-36-PadP$36)") (pinfunction "36") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$37" smd rect (at 45.11 -3.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "37") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$38" smd rect (at 45.11 -3.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "unconnected-(a2-38-PadP$38)") (pinfunction "38") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$39" smd rect (at 45.11 -3.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "39") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$40" smd rect (at 45.11 -2.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "unconnected-(a2-40-PadP$40)") (pinfunction "40") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$41" smd rect (at 45.11 -2.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(a2-41-PadP$41)") (pinfunction "41") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$42" smd rect (at 45.11 -2.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "unconnected-(a2-42-PadP$42)") (pinfunction "42") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$43" smd rect (at 45.11 -2.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/MUX_SEL") (pinfunction "43") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$44" smd rect (at 45.11 -1.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "unconnected-(a2-44-PadP$44)") (pinfunction "44") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$45" smd rect (at 45.11 -1.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/MUX_SEL") (pinfunction "45") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$46" smd rect (at 45.11 -1.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/Pi_SD_RX_MISO") (pinfunction "46") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$47" smd rect (at 45.11 -1.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "unconnected-(a2-47-PadP$47)") (pinfunction "47") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$48" smd rect (at 45.11 -0.86 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "unconnected-(a2-48-PadP$48)") (pinfunction "48") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$49" smd rect (at 45.11 -0.61 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/SD_Detect") (pinfunction "49") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$50" smd rect (at 45.11 -0.36 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/Pi_SD_TX_MOSI") (pinfunction "50") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$51" smd rect (at 45.11 -0.11 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/SD_Detect") (pinfunction "51") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$52" smd rect (at 45.11 0.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "unconnected-(a2-52-PadP$52)") (pinfunction "52") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$53" smd rect (at 45.11 0.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "unconnected-(a2-53-PadP$53)") (pinfunction "53") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$54" smd rect (at 45.11 0.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "/Pi_SD_CS") (pinfunction "54") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$55" smd rect (at 45.11 0.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "55") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$56" smd rect (at 45.11 1.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "unconnected-(a2-56-PadP$56)") (pinfunction "56") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$57" smd rect (at 45.11 1.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "57") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$58" smd rect (at 45.11 1.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "unconnected-(a2-58-PadP$58)") (pinfunction "58") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$59" smd rect (at 45.11 1.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$60" smd rect (at 45.11 2.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$61" smd rect (at 45.11 2.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$62" smd rect (at 45.11 2.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$63" smd rect (at 45.11 2.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$64" smd rect (at 45.11 3.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$65" smd rect (at 45.11 3.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$66" smd rect (at 45.11 3.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
    (pad "P$67" smd rect (at 45.11 3.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "67") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$68" smd rect (at 45.11 4.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "68") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$69" smd rect (at 45.11 4.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "69") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$70" smd rect (at 45.11 4.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "unconnected-(a2-70-PadP$70)") (pinfunction "70") (pintype "bidirectional+no_connect") (solder_mask_margin 0.1016))
    (pad "P$71" smd rect (at 45.11 4.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "71") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$72" smd rect (at 45.11 5.14 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/VBUS") (pinfunction "72") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$73" smd rect (at 45.11 5.39 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "73") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$74" smd rect (at 45.11 5.64 90) (size 0.35 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/VBUS") (pinfunction "74") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "P$75" smd rect (at 45.11 5.89 90) (size 0.35 2.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "75") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "PTS810_SJM_250_SMTR_LFS:SW_PTS810_SJM_250_SMTR_LFS" (layer "F.Cu")
    (at 134.207 63.137 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/PTS810%20SJM%20250%20SMTR%20LFS/C%2526K/view-part/?ref=eda")
    (property "Description" "\nTactile Switch SPST-NO Top Actuated Surface Mount\n")
    (property "MANUFACTURER" "CnK")
    (property "MF" "C&K")
    (property "MP" "PTS810 SJM 250 SMTR LFS")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=522770&manufacturer=C&amp;K&part_name=PTS810 SJM 250 SMTR LFS&search_term=None")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/PTS810%20SJM%20250%20SMTR%20LFS/C%2526K/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "SW3" (at 0.073 2.615) (layer "F.SilkS"))
    (fp_text value "PTS810_SJM_250_SMTR_LFS" (at 13.91 2.665) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(SW3-Pad1)") (pintype "passive+no_connect") (solder_mask_margin 0.102))
    (pad "2" smd rect (at 2.075 -1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/INP_BTN") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 2.075 1.075 180) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(SW3-Pad4)") (pintype "passive+no_connect") (solder_mask_margin 0.102))
  )
  (footprint "MicroSD_1051620001:MOLEX_1051620001" (layer "F.Cu")
    (at 162.455 99.775 -90)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/1051620001/Molex/view-part/?ref=eda")
    (property "Description" "\n9 (8 + 1) Position Card Connector Secure Digital - microSD™ Surface Mount, Right Angle Gold\n")
    (property "MANUFACTURER" "MOLEX")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.45mm")
    (property "MF" "Molex")
    (property "MP" "1051620001")
    (property "PARTREV" "D")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=2753561&manufacturer=Molex&part_name=1051620001&search_term=1051620001")
    (property "SNAPEDA_PN" "1051620001")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/1051620001/Molex/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "J2" (at 1.025 7.555) (layer "F.SilkS"))
    (fp_text value "1051620001" (at -0.382 5.949 90) (layer "F.Fab") hide)
    (pad "G1" smd rect (at 5.34 0.135 270) (size 1.05 1.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "G2" smd rect (at 5.34 -2.475 270) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "G3" smd rect (at -5.31 -1.905 270) (size 1.05 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "G4" smd rect (at -5.31 1.28 270) (size 1.05 2.39) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P1" smd rect (at 3.565 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "unconnected-(J2-DAT2-PadP1)") (pinfunction "DAT2") (pintype "bidirectional+no_connect") (solder_mask_margin 0.0762))
    (pad "P2" smd rect (at 2.465 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/CS_SD") (pinfunction "DAT3/CS") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P3" smd rect (at 1.365 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MOSI_SD") (pinfunction "CMD/MOSI") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P4" smd rect (at 0.265 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P5" smd rect (at -0.835 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/SCK_SD") (pinfunction "CLK/SCK") (pintype "input") (solder_mask_margin 0.0762))
    (pad "P6" smd rect (at -1.935 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.0762))
    (pad "P7" smd rect (at -3.035 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/MISO_SD") (pinfunction "DAT0/MISO") (pintype "bidirectional") (solder_mask_margin 0.0762))
    (pad "P8" smd rect (at -4.135 4.085 270) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "unconnected-(J2-DAT1-PadP8)") (pinfunction "DAT1") (pintype "bidirectional+no_connect") (solder_mask_margin 0.0762))
    (pad "P9" smd rect (at 5.325 1.405 270) (size 0.72 0.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/SD_Detect") (pinfunction "DET") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "SH1" smd rect (at -2.13 -3.15 270) (size 2.91 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "unconnected-(J2-SHIELD-PadSH1)") (pinfunction "SHIELD") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (pad "SH2" smd rect (at 2.05 -3.15 270) (size 2.91 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "unconnected-(J2-SHIELD-PadSH1)") (pinfunction "SHIELD") (pintype "passive+no_connect") (solder_mask_margin 0.0762))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 164.68 95.125)
          (xy 164.68 103.625)
          (xy 160.68 103.625)
          (xy 160.68 95.125)
        )
      )
    )
    (zone (net 0) (net_name "") (layers "*.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 164.68 95.125)
          (xy 164.68 103.625)
          (xy 160.68 103.625)
          (xy 160.68 95.125)
        )
      )
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 150.1 69.3625 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 2.2125 -0.15 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SDA_BMI270") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_Lever_1P2T_NKK_GW12LxH" (layer "F.Cu")
    (at 93.632 67.912 180)
    (descr "Switch, single pole double throw, right angle, http://www.nkkswitches.com/pdf/GW.pdf")
    (tags "switch single-pole double-throw spdt ON-ON horizontal")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Switch, single pole double throw")
    (property "ki_keywords" "switch single-pole double-throw spdt ON-ON")
    (attr through_hole)
    (fp_text reference "SW1" (at 2.932 -2.938) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at 2.54 12.48) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.464 3.386) (layer "F.Fab"))
    (pad "" thru_hole circle (at 0 5.08 180) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle (at 5.08 5.08 180) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 35 "/VSYS") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 22 "/BATT_I{slash}P") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.2 1.2) (drill 0.6) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(SW1-C-Pad3)") (pinfunction "C") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Lever_1P2T_NKK_GW12LxH.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 126.75 71.95 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -0.1425 -1.386) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/INT_RTC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TMUX1574PWR:SOP65P640X120-16N" (layer "F.Cu")
    (at 158 88.4 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TMUX1574PWR/Texas+Instruments/view-part/?ref=eda")
    (property "Description" "\n5-V, 2:1 (SPDT), 4-channel analog switch with powered-off protection & 1.8-V input logic\n")
    (property "MF" "Texas Instruments")
    (property "MP" "TMUX1574PWR")
    (property "Package" "TSSOP-16 Texas Instruments")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3213992&manufacturer=Texas Instruments&part_name=TMUX1574PWR&search_term=tmux1574")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TMUX1574PWR/Texas+Instruments/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "U4" (at 0.1 -3.5 180) (layer "F.SilkS"))
    (fp_text value "TMUX1574PWR" (at 7.295 3.635) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -2.87 -2.275 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 23 "/MUX_SEL") (pinfunction "SEL") (pintype "input") (solder_mask_margin 0.102))
    (pad "2" smd roundrect (at -2.87 -1.625 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 49 "/Pico_SPI1_CS") (pinfunction "S1A") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "3" smd roundrect (at -2.87 -0.975 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 18 "/Pi_SD_CS") (pinfunction "S1B") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "4" smd roundrect (at -2.87 -0.325 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 13 "/CS_SD") (pinfunction "D1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "5" smd roundrect (at -2.87 0.325 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 47 "/Pico_SPI1_TX") (pinfunction "S2A") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "6" smd roundrect (at -2.87 0.975 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 19 "/Pi_SD_TX_MOSI") (pinfunction "S2B") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "7" smd roundrect (at -2.87 1.625 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 14 "/MOSI_SD") (pinfunction "D2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "8" smd roundrect (at -2.87 2.275 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "9" smd roundrect (at 2.87 2.275 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 15 "/SCK_SD") (pinfunction "D3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "10" smd roundrect (at 2.87 1.625 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 21 "/Pi_SD_SCK") (pinfunction "S3B") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "11" smd roundrect (at 2.87 0.975 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 46 "/Pico_SPI1_SCK") (pinfunction "S3A") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "12" smd roundrect (at 2.87 0.325 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 16 "/MISO_SD") (pinfunction "D4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "13" smd roundrect (at 2.87 -0.325 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 20 "/Pi_SD_RX_MISO") (pinfunction "S4B") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "14" smd roundrect (at 2.87 -0.975 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 48 "/Pico_SPI1_RX") (pinfunction "S4A") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "15" smd roundrect (at 2.87 -1.625 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 1 "GND") (pinfunction "~{EN}") (pintype "input") (solder_mask_margin 0.102))
    (pad "16" smd roundrect (at 2.87 -2.275 180) (size 1.57 0.41) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.05)
      (net 3 "+3.3V") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 126.9 67.6125 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.2875 0.05 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(U2-EVI)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PRT_14417:CONN_PRT-14417_SPK" (layer "F.Cu")
    (at 162.05 64.4485 180)
    (tags "PRT-14417 ")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "PRT-14417")
    (attr smd)
    (fp_text reference "J3" (at 0.25 3.6985 unlocked) (layer "F.SilkS"))
    (fp_text value "PRT-14417" (at 0 -2.1015 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.5 -2.1015 180) (size 0.6096 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -0.499999 -2.1015 180) (size 0.6096 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 0.499999 -2.1015 180) (size 0.6096 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/SDA_BMI270") (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at 1.5 -2.1015 180) (size 0.6096 1.5494) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/SCL_BMI270") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at -2.799999 1.773501 180) (size 1.1938 1.8034) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 2.799999 1.773501 180) (size 1.1938 1.8034) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "RV-8803-C7:RV8803" (layer "F.Cu")
    (at 124.262 67.5945)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/RV-8803-C7-32.768KHZ-3PPM-TA-QC/Micro+Crystal/view-part/?ref=eda")
    (property "Description" "\nReal-Time Clock Module, Temperature compensated, in 1.5 x 3.2 mm package\n")
    (property "MANUFACTURER" "Micro Crystal")
    (property "MAXIMUM_PACKAGE_HEIGHT" "0.8 mm")
    (property "MF" "Micro Crystal")
    (property "MP" "RV-8803-C7-32.768KHZ-3PPM-TA-QC")
    (property "PARTREV" "5.1/06.2018")
    (property "Package" "QFN-8 Micro Crystal")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=5559019&manufacturer=Micro Crystal&part_name=RV-8803-C7-32.768KHZ-3PPM-TA-QC&search_term=rv8803")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RV-8803-C7-32.768KHZ-3PPM-TA-QC/Micro+Crystal/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "U2" (at -0.212 2.5555) (layer "F.SilkS"))
    (fp_text value "RV-8803-C7-32.768KHZ-3PPM-TA-QC" (at 1.402 -2.5) (layer "F.Fab") hide)
    (pad "1" smd rect (at -0.6 -1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SDA_0") (pinfunction "SDA") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -0.6 -0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/CLKOUT_RTC") (pinfunction "CLKOUT") (pintype "output") (solder_mask_margin 0.102))
    (pad "3" smd rect (at -0.6 0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "Net-(U2-VDD)") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at -0.6 1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(U2-CLKOE)") (pinfunction "CLKOE") (pintype "input") (solder_mask_margin 0.102))
    (pad "5" smd rect (at 0.6 1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "6" smd rect (at 0.6 0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/INT_RTC") (pinfunction "~{INT}") (pintype "output") (solder_mask_margin 0.102))
    (pad "7" smd rect (at 0.6 -0.45) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(U2-EVI)") (pinfunction "EVI") (pintype "input") (solder_mask_margin 0.102))
    (pad "8" smd rect (at 0.6 -1.35) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/SCL_0") (pinfunction "SCL") (pintype "input") (solder_mask_margin 0.102))
  )
  (footprint "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH" (layer "F.Cu")
    (at 116.554 87.673 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at -0.103967 10.173781 90) (layer "F.SilkS") hide)
    (fp_text value "Pico" (at -0.103967 12.332781 90) (layer "F.Fab") hide)
    (fp_text user "AGND" (at 13.773 -7.104 135) (layer "F.SilkS") hide)
    (fp_text user "GP17" (at 14.054 21.59 135) (layer "F.SilkS") hide)
    (fp_text user "GP11" (at -14.2 11.43 135) (layer "F.SilkS") hide)
    (fp_text user "GP0" (at -13.8 -24.13 135) (layer "F.SilkS") hide)
    (fp_text user "GP3" (at -13.8 -13.97 135) (layer "F.SilkS") hide)
    (fp_text user "GP8" (at -13.8 1.27 135) (layer "F.SilkS") hide)
    (fp_text user "GP20" (at 13.873 11.046 135) (layer "F.SilkS") hide)
    (fp_text user "GND" (at -13.8 -6.35 135) (layer "F.SilkS") hide)
    (fp_text user "GP21" (at 13.723 8.546 135) (layer "F.SilkS") hide)
    (fp_text user "GP6" (at -13.8 -3.81 135) (layer "F.SilkS") hide)
    (fp_text user "GP9" (at -13.8 3.81 135) (layer "F.SilkS") hide)
    (fp_text user "GND" (at -13.8 6.35 135) (layer "F.SilkS") hide)
    (fp_text user "GND" (at 13.8 19.05 135) (layer "F.SilkS") hide)
    (fp_text user "GP14" (at -14.1 21.59 135) (layer "F.SilkS") hide)
    (fp_text user "GP27" (at 13.573 -4.454 135) (layer "F.SilkS") hide)
    (fp_text user "RUN" (at 13.673 0.846 135) (layer "F.SilkS") hide)
    (fp_text user "GP19" (at 13.823 13.646 135) (layer "F.SilkS") hide)
    (fp_text user "GP4" (at -13.8 -11.43 135) (layer "F.SilkS") hide)
    (fp_text user "GP16" (at 14.054 24.13 135) (layer "F.SilkS") hide)
    (fp_text user "GP2" (at -13.9 -16.51 135) (layer "F.SilkS") hide)
    (fp_text user "GP13" (at -14.054 16.51 135) (layer "F.SilkS") hide)
    (fp_text user "GP26" (at 13.573 -1.554 135) (layer "F.SilkS") hide)
    (fp_text user "GP12" (at -14.2 13.97 135) (layer "F.SilkS") hide)
    (fp_text user "GND" (at -13.8 -19.05 135) (layer "F.SilkS") hide)
    (fp_text user "GP22" (at 13.973 3.396 135) (layer "F.SilkS") hide)
    (fp_text user "GP18" (at 13.923 15.796 135) (layer "F.SilkS") hide)
    (fp_text user "GP15" (at -14.054 24.13 135) (layer "F.SilkS") hide)
    (fp_text user "GND" (at 13.573 6.146 135) (layer "F.SilkS") hide)
    (fp_text user "GP1" (at -13.9 -21.6 135) (layer "F.SilkS") hide)
    (fp_text user "SWCLK" (at -5.7 26.2 90) (layer "F.SilkS") hide)
    (fp_text user "GP7" (at -13.7 -1.3 135) (layer "F.SilkS") hide)
    (fp_text user "SWDIO" (at 5.6 26.2 90) (layer "F.SilkS") hide)
    (fp_text user "GND" (at -13.8 19.05 135) (layer "F.SilkS") hide)
    (fp_text user "GP10" (at -14.054 8.89 135) (layer "F.SilkS") hide)
    (fp_text user "GP5" (at -13.8 -8.89 135) (layer "F.SilkS") hide)
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2 90) (layer "Cmts.User") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab") hide)
    (pad "1" smd rect (at -9.89 -24.13 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 50 "/INT_BMI270") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" smd rect (at -9.89 -21.59 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 71 "/IR_OUT") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "3" smd rect (at -9.89 -19.05 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -9.89 -16.51 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 42 "/Pico_SPI0_SCK") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd rect (at -9.89 -13.97 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 43 "/Pico_SPI0_TX") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd rect (at -9.89 -11.43 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 44 "/Pico_SPI0_RX") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd rect (at -9.89 -8.89 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 45 "/Pico_SPI0_CS") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd rect (at -9.89 -6.35 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 72 "unconnected-(U6-GND-Pad8)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "9" smd rect (at -9.89 -3.81 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 34 "/LED_RED") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "10" smd rect (at -9.89 -1.27 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 5 "/LED_GREEN") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "11" smd rect (at -9.89 1.27 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 7 "/LED_BLUE") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd rect (at -9.89 3.81 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 17 "/SD_Detect") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd rect (at -9.89 6.35 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 89 "unconnected-(U6-GND-Pad13)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "14" smd rect (at -9.89 8.89 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 46 "/Pico_SPI1_SCK") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "15" smd rect (at -9.89 11.43 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 47 "/Pico_SPI1_TX") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" smd rect (at -9.89 13.97 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 48 "/Pico_SPI1_RX") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "17" smd rect (at -9.89 16.51 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 49 "/Pico_SPI1_CS") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "18" smd rect (at -9.89 19.05 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 73 "unconnected-(U6-GND-Pad18)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "19" smd rect (at -9.89 21.59 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 23 "/MUX_SEL") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "20" smd rect (at -9.89 24.13 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 53 "unconnected-(U6-GPIO15-Pad20)") (pinfunction "GPIO15") (pintype "bidirectional+no_connect"))
    (pad "21" smd rect (at 9.89 24.13 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 30 "/SDA_0") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "22" smd rect (at 9.89 21.59 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 29 "/SCL_0") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "23" smd rect (at 9.89 19.05 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 74 "unconnected-(U6-GND-Pad23)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "24" smd rect (at 9.89 16.51 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 32 "/SDA_1") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "25" smd rect (at 9.89 13.97 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 31 "/SCL_1") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "26" smd rect (at 9.89 11.43 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 33 "/INT_RTC") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" smd rect (at 9.89 8.89 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 24 "/ALERT_PMIC") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "28" smd rect (at 9.89 6.35 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 92 "unconnected-(U6-GND-Pad28)") (pinfunction "GND") (pintype "power_in+no_connect"))
    (pad "29" smd rect (at 9.89 3.81 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 51 "/CLKOUT_RTC") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "30" smd rect (at 9.89 1.27 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 26 "/HUB_DETECT") (pinfunction "RUN") (pintype "input"))
    (pad "31" smd rect (at 9.89 -1.27 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 75 "unconnected-(U6-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect (at 9.89 -3.81 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 76 "unconnected-(U6-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional+no_connect"))
    (pad "33" smd rect (at 9.89 -6.35 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 77 "unconnected-(U6-AGND-Pad33)") (pinfunction "AGND") (pintype "power_in+no_connect"))
    (pad "34" smd rect (at 9.89 -8.89 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 4 "/INP_BTN") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "35" smd rect (at 9.89 -11.43 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 78 "unconnected-(U6-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "power_in+no_connect"))
    (pad "36" smd rect (at 9.89 -13.97 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 3 "+3.3V") (pinfunction "3V3") (pintype "power_in"))
    (pad "37" smd rect (at 9.89 -16.51 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 38 "/RST_HW") (pinfunction "3V3_EN") (pintype "input"))
    (pad "38" smd rect (at 9.89 -19.05 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "39" smd rect (at 9.89 -21.59 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 35 "/VSYS") (pinfunction "VSYS") (pintype "power_in"))
    (pad "40" smd rect (at 9.89 -24.13 90) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 25 "/VBUS") (pinfunction "VBUS") (pintype "power_in"))
    (pad "41" smd rect (at -2.54 25.9 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 79 "unconnected-(U6-SWCLK-Pad41)") (pinfunction "SWCLK") (pintype "input+no_connect"))
    (pad "42" smd rect (at 0 25.9 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 9 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd rect (at 2.54 25.9 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 80 "unconnected-(U6-SWDIO-Pad43)") (pinfunction "SWDIO") (pintype "bidirectional+no_connect"))
    (model "C:/Users/ncara/OneDrive/IoT/Tools/KiCad/RP-Pico Libraries/Pico.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/viggi/Documents/GitHub/KiCad-RP-Pico/RP-Pico Libraries/Pico.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 145.45 72.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at -0.148 1.412) (layer "F.SilkS"))
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 130.3 67.5125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at -2.6375 -0.15) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/INP_BTN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-3" (layer "F.Cu")
    (at 117.502 70.948)
    (descr "SOT, 3 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178D.PDF inferred 3-pin variant), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "40V 0.2A Dual Small Signal Schottky Diodes")
    (property "ki_keywords" "Schottky, Diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "BAS70-05" (at 0 2.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(BT1-PadP1)") (pintype "passive"))
    (pad "2" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "3" smd roundrect (at 1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(U2-VDD)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 149.8 72.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0.2 1.45) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 154.2875 72.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -0.0625 -1.55) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 94.996 103.886 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -0.114 -3.046 180) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0.136 13.604 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.114 3.404) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 71 "/IR_OUT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 156.35 64.1 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "JP1" (at 3.148 0 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Bridged12" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -1.3 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 31 "/SCL_1") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 28 "/SCL_BMI270") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 29 "/SCL_0") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "MS860702BA01:TE_MS860702BA01-50" (layer "F.Cu")
    (at 145.983 69.278 90)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/MS860702BA01-50/TE+Connectivity+ALCOSWITCH+Switches/view-part/?ref=eda")
    (property "Comment" "MS860702BA01-50")
    (property "DESCRIPTION" "Pressure Temp Humidity Sensor")
    (property "Description" "\nHumidity, Pressure, Temperature Sensor I²C Output\n")
    (property "MANUFACTURER" "TE Connectivity")
    (property "MF" "TE Connectivity")
    (property "MP" "MS860702BA01-50")
    (property "MPN" "MS860702BA01-50")
    (property "PARTREV" "06/2017")
    (property "Package" "QFN-8 TE Connectivity")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=555056&manufacturer=TE Connectivity&part_name=MS860702BA01-50&search_term=ms8607-02ba01")
    (property "STANDARD" "Manufacturer recommendation")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/MS860702BA01-50/TE+Connectivity+ALCOSWITCH+Switches/view-part/?ref=snap")
    (attr smd)
    (fp_text reference "U5" (at 2.332 0.009 180) (layer "F.SilkS"))
    (fp_text value "MS860702BA01-50" (at 3.702178 3.620446 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -1.1 -1.875 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3.3V") (pinfunction "VDD") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -1.1 -0.625 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (pad "3" smd rect (at -1.1 0.625 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "4" smd rect (at -1.1 1.875 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (pad "5" smd rect (at 1.1 1.875 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (pad "6" smd rect (at 1.1 0.625 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (solder_mask_margin 0.102))
    (pad "7" smd rect (at 1.1 -0.625 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SDA_0") (pinfunction "SDA") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "8" smd rect (at 1.1 -1.875 90) (size 1.1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/SCL_0") (pinfunction "SCL") (pintype "input") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 123.6735 63.137 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0.1735 1.437) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SDA_0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 120.5 67.6 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.35 0.35) (layer "F.SilkS"))
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(U2-VDD)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 148.4125 64.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -0.1655 1.386) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SDA_0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BAT-HLD-012-SMT:BAT_BAT-HLD-012-SMT" (layer "F.Cu")
    (at 105.3 65.85 180)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/BAT-HLD-012-SMT/Linx+Technologies+Inc./view-part/?ref=eda")
    (property "Description" "\nHolder for CR1216 and CR1225 Batteries, Surface-Mount, Bulk Packaging\n")
    (property "MANUFACTURER" "Linx Technologies")
    (property "MF" "Linx Technologies")
    (property "MP" "BAT-HLD-012-SMT")
    (property "PARTREV" "A")
    (property "Package" "None")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=104817&manufacturer=Linx Technologies&part_name=BAT-HLD-012-SMT&search_term=None")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/BAT-HLD-012-SMT/Linx+Technologies+Inc./view-part/?ref=snap")
    (attr smd)
    (fp_text reference "BT1" (at -2.255 -6.589) (layer "F.SilkS"))
    (fp_text value "BAT-HLD-012-SMT" (at -0.616 6.16) (layer "F.Fab"))
    (pad "N" smd circle (at 0 0 180) (size 10.2 10.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.102))
    (pad "P1" smd rect (at -7.65 -0.05 180) (size 2.5 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(BT1-PadP1)") (pintype "passive") (solder_mask_margin 0.102))
    (pad "P2" smd rect (at 7.65 -0.05 180) (size 2.5 5.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(BT1-PadP1)") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 157.85 69.4655 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.4155 0.2 -180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/SCL_BMI270") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (at 159.55 72.65)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at -0.05 1.3) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 152.5 64 90)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "3-pole Solder Jumper, pins 1+2 closed/bridged")
    (property "ki_keywords" "Solder Jumper SPDT")
    (attr exclude_from_pos_files)
    (net_tie_pad_groups "1, 2, 3")
    (fp_text reference "JP2" (at 2.994 0 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_3_Bridged12" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -1.3 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 32 "/SDA_1") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.55 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.55 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0 90) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 27 "/SDA_BMI270") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 30 "/SDA_0") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.55 0.75)
            (xy -0.55 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "PMIC_Castellated_Daughter:PinSocket_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (at 106.73 89.16 180)
    (descr "SMD")
    (tags "SMD")
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (zone_connect 0)
    (attr smd allow_missing_courtyard)
    (fp_text reference "J1" (at -14.71 8.63) (layer "B.SilkS") hide)
    (fp_text value "Conn_02x04_Top_Bottom" (at 0 -10.39 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 14.16 2.15 90) (layer "B.Fab"))
    (pad "ALERT" connect oval (at -14.89 5.96 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 24 "/ALERT_PMIC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "BATT" connect oval (at 14.16 3.42 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 22 "/BATT_I{slash}P") (pinfunction "Pin_6") (pintype "passive"))
    (pad "GND" connect oval (at 14.16 5.96 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "SCL" connect oval (at -14.89 0.88 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 29 "/SCL_0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "SCL" connect oval (at 14.16 0.88 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (pinfunction "Pin_7") (pintype "passive"))
    (pad "SDA" connect oval (at -14.89 -1.66 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 30 "/SDA_0") (pinfunction "Pin_8") (pintype "passive"))
    (pad "SDA" connect oval (at 14.16 -1.66 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (pinfunction "Pin_8") (pintype "passive"))
    (pad "VBUS" connect oval (at -14.89 3.42 180) (size 2.1 1.3) (layers "B.Cu" "B.Mask")
      (net 25 "/VBUS") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0.5 4 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "B.Cu")
    (at 162.56 62.738 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "MAX30001_tinybreakout:MAX30001-21P-2.54-21X17.8MM" (layer "B.Cu")
    (at 145.72782 78.16688 -90)
    (property "Sheetfile" "MINDER BioDAQ system.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Protocentral tinyECG max30001 breakout board")
    (attr smd)
    (fp_text reference "U1" (at 9.3345 21.7805 90) (layer "B.SilkS") hide)
    (fp_text value "~" (at 8.89 10.795 90) (layer "B.SilkS") hide)
    (pad "1" smd oval (at 0.83312 18.11782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "unconnected-(U1-INT2B-Pad1)") (pinfunction "INT2B") (pintype "unspecified+no_connect"))
    (pad "2" smd oval (at 0.83312 15.57782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "unconnected-(U1-INTB-Pad2)") (pinfunction "INTB") (pintype "unspecified+no_connect"))
    (pad "3" smd oval (at 0.83312 13.03782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "unconnected-(U1-PA10_A2_D2-Pad3)") (pinfunction "PA10_A2_D2") (pintype "unspecified+no_connect"))
    (pad "4" smd oval (at 0.83312 10.49782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "unconnected-(U1-PA11_A3_D3-Pad4)") (pinfunction "PA11_A3_D3") (pintype "unspecified+no_connect"))
    (pad "5" smd oval (at 0.83312 7.95782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "unconnected-(U1-PA8_A4_D4_SDA-Pad5)") (pinfunction "PA8_A4_D4_SDA") (pintype "unspecified+no_connect"))
    (pad "6" smd oval (at 0.83312 5.41782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "unconnected-(U1-PA9_A5_D5_SCL-Pad6)") (pinfunction "PA9_A5_D5_SCL") (pintype "unspecified+no_connect"))
    (pad "7" smd oval (at 0.83312 2.87782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "unconnected-(U1-PB08_A6_D6_TX-Pad7)") (pinfunction "PB08_A6_D6_TX") (pintype "unspecified+no_connect"))
    (pad "8" smd oval (at 16.99768 2.87782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "/Pico_SPI0_CS") (pinfunction "MAX_CS") (pintype "unspecified"))
    (pad "9" smd oval (at 16.99768 5.41782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "/Pico_SPI0_SCK") (pinfunction "MAX_SCK") (pintype "unspecified"))
    (pad "10" smd oval (at 16.99768 7.95782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "/Pico_SPI0_RX") (pinfunction "MAX_MISO") (pintype "unspecified"))
    (pad "11" smd oval (at 16.99768 10.49782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "/Pico_SPI0_TX") (pinfunction "MAX_MOSI") (pintype "unspecified"))
    (pad "12" smd oval (at 16.99768 13.03782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "+3.3V") (pinfunction "3V3") (pintype "unspecified"))
    (pad "13" smd oval (at 16.99768 15.57782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "GNDA") (pinfunction "GND") (pintype "unspecified"))
    (pad "14" smd oval (at 16.99768 18.11782 270) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "unconnected-(U1-5V-Pad14)") (pinfunction "5V") (pintype "unspecified+no_connect"))
    (pad "15" smd oval (at 1.076901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "unconnected-(U1-VCM-Pad15)") (pinfunction "VCM") (pintype "unspecified+no_connect"))
    (pad "16" smd oval (at 3.616901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "unconnected-(U1-1.8v-Pad16)") (pinfunction "1.8v") (pintype "unspecified+no_connect"))
    (pad "17" smd oval (at 6.156901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "unconnected-(U1-DRVN-Pad17)") (pinfunction "DRVN") (pintype "unspecified+no_connect"))
    (pad "18" smd oval (at 8.696901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "unconnected-(U1-DRVP-Pad18)") (pinfunction "DRVP") (pintype "unspecified+no_connect"))
    (pad "19" smd oval (at 11.236901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "unconnected-(U1-ECGP-Pad19)") (pinfunction "ECGP") (pintype "unspecified+no_connect"))
    (pad "20" smd oval (at 13.776901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "unconnected-(U1-ECGN-Pad20)") (pinfunction "ECGN") (pintype "power_out+no_connect"))
    (pad "21" smd oval (at 16.316901 -0.176213) (size 2.74828 1.99898) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "unconnected-(U1-GND-Pad21)") (pinfunction "GND") (pintype "unspecified+no_connect"))
  )
  (gr_text "SDA" (at 90.73 90.05 90) (layer "B.SilkS"))
  (gr_text "MAX30001" (at 134.3 85.55) (layer "B.SilkS"))
  (gr_text "GND" (at 98.05 101.95) (layer "B.SilkS"))
  (gr_text "SDA" (at 123.6 91.34 270) (layer "B.SilkS"))
  (gr_text "VBUS" (at 123.6 86.73 270) (layer "B.SilkS"))
  (gr_text "BATT_I/P" (at 90.73 84.34 90) (layer "B.SilkS"))
  (gr_text "3.3V" (at 101 101.95) (layer "B.SilkS"))
  (gr_text "IR Out" (at 95.6 101.85) (layer "B.SilkS"))
  (gr_text "SCL" (at 90.73 87.87 90) (layer "B.SilkS"))
  (gr_text "IR control" (at 105.65 105.5) (layer "B.SilkS"))
  (gr_text "GND" (at 90.73 82.24 90) (layer "B.SilkS"))
  (gr_text "SCL" (at 123.6 89.08 270) (layer "B.SilkS"))
  (gr_text "ALERT" (at 123.6 84.17 270) (layer "B.SilkS"))
  (gr_text "RaspberryPi Pico W" (at 96.85 86.2) (layer "F.SilkS"))
  (gr_text "ON" (at 93.05 69.65) (layer "F.SilkS"))
  (gr_text "OFF" (at 87.2 69.8) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 153.35 68.65)
        (xy 155.3 68.65)
        (xy 155.3 70.45)
        (xy 153.3 70.4)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 85.05 55.15)
        (xy 170.05 55.25)
        (xy 169.65 70.9)
        (xy 174.85 70.7)
        (xy 174.95 94.7)
        (xy 168.65 94.7)
        (xy 168.85 107.45)
        (xy 85.05 108.3)
        (xy 85.1 55.15)
      )
    )
  )
  (zone (net 3) (net_name "+3.3V") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 85.2 59.35)
        (xy 169.95 58.6)
        (xy 169.65 71.05)
        (xy 174.85 70.95)
        (xy 175.05 94.95)
        (xy 168.5 94.9)
        (xy 168.75 107.65)
        (xy 85.05 108.35)
      )
    )
  )
)
