<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="22.06625" y1="7.62" x2="1.27" y2="7.62" width="0.254" layer="20"/>
<wire x1="1.27" y1="7.62" x2="0" y2="8.89" width="0.254" layer="20" curve="-90"/>
<wire x1="0" y1="8.89" x2="0" y2="15.24" width="0.254" layer="20"/>
<wire x1="0" y1="15.24" x2="1.27" y2="16.51" width="0.254" layer="20" curve="-90"/>
<wire x1="1.27" y1="16.51" x2="22.06625" y2="16.51" width="0.254" layer="20"/>
<text>KD0GLS 2018</text>
<text>+</text>
<text>-</text>
<text>CR2032</text>
<wire x1="22.06625" y1="16.51" x2="22.06625" y2="7.62" width="0.254" layer="20" curve="-315.825657"/>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CR2032_HOLDER">
<description>MPD P/N BS-7
Digi-Key P/N BS-7-ND</description>
</package>
<package name="CONN_BREAKAWAY_2X3_DUAL_ROW_SPACING">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BT1" library="kd0gls" package="CR2032_HOLDER" value="CR2032_HOLDER"/>
<element name="J1" library="kd0gls" package="CONN_BREAKAWAY_2X3_DUAL_ROW_SPACING" value="CONN_BREAKAWAY_2X3_DUAL_ROW_SPACING"/>
</elements>
<signals>
<signal name="+">
<contactref element="BT1" pad="+"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="-">
<contactref element="BT1" pad="-"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
