<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.0.0">
<drawing>
<board>
<plain>
<wire x1="50.8" y1="28.575" x2="-60.96" y2="28.575" width="0" layer="20"/>
<wire x1="-60.96" y1="-28.575" x2="50.8" y2="-28.575" width="0" layer="20"/>
<wire x1="50.8" y1="-28.575" x2="50.8" y2="28.575" width="0" layer="20"/>
<wire x1="-60.96" y1="-28.575" x2="-60.96" y2="28.575" width="0" layer="20"/>
<text>Copyright (C) 2015-2016 Herbert Pötzl
Licensed under CERN OHL v.1.2</text>
<text>AXIOM Beta
Main Board</text>
<text>HIGH SPEED IO</text>
<hole x="-27.305" y="20.955" drill="1.2"/>
<hole x="-24.765" y="20.955" drill="1.2"/>
<hole x="24.765" y="20.955" drill="1.2"/>
<hole x="27.305" y="20.955" drill="1.2"/>
<hole x="-27.305" y="-20.955" drill="1.2"/>
<hole x="-24.765" y="-20.955" drill="1.2"/>
<hole x="24.765" y="-20.955" drill="1.2"/>
<hole x="27.305" y="-20.955" drill="1.2"/>
<text>0</text>
<text>V0.36
R1.0</text>
<text>Solder On
Center Area</text>
<text>JX1</text>
<text>JX2</text>
<text>VC</text>
<text>EC</text>
<text>FC</text>
<text>Solder On
Center Area</text>
<text>61083-10*400LF</text>
<text>61083-10*400LF</text>
<text>FX10A-100S/10</text>
<text>FX10A-100S/10</text>
<text>DF12-20DP</text>
<text>DF12-20DP</text>
<text>Please
keep mask
on both
sides.</text>
<text>Please
keep mask
on both
sides.</text>
<text>Please
keep mask
on both
sides.</text>
<text>Please
keep mask
on both
sides.</text>
<text>AXIOM BETA MAIN BOARD
TOP SIDE     V0.36 R1.0</text>
<text>AXIOM BETA MAIN BOARD
BOTTOM SIDE  V0.36 R1.0</text>
</plain>
<libraries>
<library name="microzed">
<packages>
<package name="µZ-NOHOLES-R">
<description>BergStak 61083 (mating connector to MicroZed)&lt;BR&gt;
Rotated and pin reversed to match the polarization peg holes.</description>
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX100_NOTEXT">
</package>
</packages>
</library>
<library name="fx10">
<packages>
<package name="FX10A-100S/10">
</package>
</packages>
</library>
<library name="PCIe">
<packages>
<package name="PCIE-36-NOPEG">
</package>
</packages>
</library>
<library name="pincon">
<packages>
<package name="2X02">
</package>
<package name="62101621821">
<description>&lt;b&gt;WR-PHD 2.00mm Dual SMT Socket Header Low Profile, 16 Pins</description>
</package>
</packages>
</library>
<library name="df12">
<packages>
<package name="DF12(XX)-20DP-0.5V">
</package>
</packages>
</library>
<library name="pinpad">
<description>Generated from &lt;b&gt;csp25.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1.2/0.6">
</package>
</packages>
</library>
<library name="generic-rcl">
<packages>
<package name="0603-A">
</package>
<package name="0201-B">
</package>
<package name="0402-B">
</package>
<package name="0805-A">
</package>
</packages>
</library>
<library name="machxo2">
<packages>
<package name="MACHXO2-100TQFP">
</package>
</packages>
</library>
<library name="pca9540">
<packages>
<package name="SOP65P490X300-8N">
</package>
</packages>
</library>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="1X02M/90-S">
</package>
</packages>
</library>
<library name="transistor">
<packages>
<package name="SOT416">
<description>&lt;li&gt;&lt;b&gt;SOT416&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;Plastic surface-mounted package; 3 leads
&lt;li&gt;&lt;u&gt;JEDEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;IEC&lt;/u&gt;: --
&lt;li&gt;&lt;u&gt;JEITA&lt;/u&gt;: SC-75&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="buzzer">
<packages>
<package name="KSSG23J12">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MICROMELF-R">
<description>&lt;b&gt;Micro Melf Diode Reflow soldering&lt;/b&gt; VISHAY mcl4148.pdf</description>
</package>
</packages>
</library>
<library name="pic16f1718">
<packages>
<package name="QFN40P400X400X55-29N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
<variantdef name="Beta"/>
</variantdefs>
<elements>
<element name="ZED1" library="microzed" package="µZ-NOHOLES-R" value="µZ-FCI-NOHOLES-R"/>
<element name="LOGO1" library="ohw-logo" package="OSHW_FILLX100_NOTEXT" value="OSHW_LOGO_FILLX0100-NT"/>
<element name="X-EAST" library="fx10" package="FX10A-100S/10" value="FX10-100/10S"/>
<element name="X-WEST" library="fx10" package="FX10A-100S/10" value="FX10-100/10S"/>
<element name="PCIE-NORTH" library="PCIe" package="PCIE-36-NOPEG" value="PCIE-36-AXIOM-NOPEG">
<attribute name="NAME"/>
</element>
<element name="PCIE-SOUTH" library="PCIe" package="PCIE-36-NOPEG" value="PCIE-36-AXIOM-NOPEG">
<attribute name="NAME"/>
</element>
<element name="PWR-NW" library="pincon" package="2X02" value="PINHD-2X02_2.54">
<attribute name="NAME"/>
</element>
<element name="PWR-NE" library="pincon" package="2X02" value="PINHD-2X02_2.54">
<attribute name="NAME"/>
</element>
<element name="PWR-SE" library="pincon" package="2X02" value="PINHD-2X02_2.54">
<attribute name="NAME"/>
</element>
<element name="PWR-SW" library="pincon" package="2X02" value="PINHD-2X02_2.54">
<attribute name="NAME"/>
</element>
<element name="PAD13" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD12" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD14" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD5" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD4" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD6" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD16" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD15" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD2" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD9" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD7" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD10" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="C1" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1'" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2'" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7'" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8'" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3'" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4'" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5'" library="generic-rcl" package="0805-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6'" library="generic-rcl" package="0603-A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RFW" library="machxo2" package="MACHXO2-100TQFP" value="MACHXO2-100">
<attribute name="NAME"/>
</element>
<element name="C9" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C10" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C19" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C28" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C20" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C29" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C12" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C13" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C21" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C22" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C23" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C24" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C25" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C26" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C27" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C11" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="U1" library="pca9540" package="SOP65P490X300-8N" value="PCA9540BDP">
<attribute name="PACKAGE" value="TSSOP8"/>
<attribute name="OC_NEWARK" value="55W4318"/>
<attribute name="MPN" value="PCA9540BDP"/>
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="OC_FARNELL" value="2212116"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="generic-rcl" package="0402-B" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB-SE" library="df12" package="DF12(XX)-20DP-0.5V" value="DF12(XX)-20DP-0.5V">
<attribute name="NAME"/>
</element>
<element name="PB-NW" library="df12" package="DF12(XX)-20DP-0.5V" value="DF12(XX)-20DP-0.5V">
<attribute name="NAME"/>
</element>
<element name="RFE" library="machxo2" package="MACHXO2-100TQFP" value="MACHXO2-100">
<attribute name="NAME"/>
</element>
<element name="C14" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C15" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C30" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C39" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C31" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C40" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C17" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C18" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="C32" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C33" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C34" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C35" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C36" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C37" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C38" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C16" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="PAD3" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD11" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="JP1" library="pinhead-2" package="1X02M/90-S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT416" value="NX3008NBKT">
<attribute name="NAME"/>
</element>
<element name="T2" library="transistor" package="SOT416" value="NX3008NBKT">
<attribute name="NAME"/>
</element>
<element name="R10" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SP1" library="buzzer" package="KSSG23J12" value="KSSG23J12">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="MICROMELF-R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="PAD1" library="pinpad" package="1.2/0.6" value="PINPAD1.27MM"/>
<element name="HDR-NW" library="pincon" package="62101621821" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HDR-SW" library="pincon" package="62101621821" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HDR-SE" library="pincon" package="62101621821" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HDR-NE" library="pincon" package="62101621821" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="generic-rcl" package="0201-B" value="100R">
<attribute name="NAME"/>
</element>
<element name="R16" library="generic-rcl" package="0201-B" value="100R">
<attribute name="NAME"/>
</element>
<element name="R17" library="generic-rcl" package="0201-B" value="100R">
<attribute name="NAME"/>
</element>
<element name="R9" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="generic-rcl" package="0402-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="pic16f1718" package="QFN40P400X400X55-29N" value="PIC16F1718-I/MV">
<attribute name="OC_NEWARK" value=""/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="MPN" value="PIC16F1718-I/MV"/>
<attribute name="PACKAGE" value="28-UQFN"/>
<attribute name="NAME"/>
</element>
<element name="C41" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="R7" library="generic-rcl" package="0402-B" value="50R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="pic16f1718" package="QFN40P400X400X55-29N" value="PIC16F1718-I/MV">
<attribute name="OC_NEWARK" value=""/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="MPN" value="PIC16F1718-I/MV"/>
<attribute name="PACKAGE" value="28-UQFN"/>
<attribute name="NAME"/>
</element>
<element name="C42" library="generic-rcl" package="0402-B" value="100n">
<attribute name="NAME"/>
</element>
<element name="R8" library="generic-rcl" package="0402-B" value="50R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="generic-rcl" package="0402-B" value="10k">
<attribute name="NAME"/>
</element>
<element name="R19" library="generic-rcl" package="0402-B" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
<element name="C44" library="generic-rcl" package="0402-B" value="10n">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ZED1" pad="33"/>
<contactref element="ZED1" pad="51"/>
<contactref element="ZED1" pad="95"/>
<contactref element="ZED1" pad="72"/>
<contactref element="ZED1" pad="22"/>
<contactref element="ZED1" pad="16"/>
<contactref element="ZED1" pad="86"/>
<contactref element="ZED1" pad="15"/>
<contactref element="ZED1" pad="96"/>
<contactref element="ZED1" pad="34"/>
<contactref element="ZED1" pad="77"/>
<contactref element="ZED1" pad="46"/>
<contactref element="ZED1" pad="28"/>
<contactref element="ZED1" pad="71"/>
<contactref element="ZED1" pad="52"/>
<contactref element="ZED1" pad="85"/>
<contactref element="ZED1" pad="66"/>
<contactref element="ZED1" pad="40"/>
<contactref element="ZED1" pad="27"/>
<contactref element="ZED1" pad="65"/>
<contactref element="ZED1" pad="21"/>
<contactref element="ZED1" pad="45"/>
<contactref element="ZED1" pad="39"/>
<contactref element="ZED1" pad="115"/>
<contactref element="ZED1" pad="116"/>
<contactref element="ZED1" pad="121"/>
<contactref element="ZED1" pad="122"/>
<contactref element="ZED1" pad="127"/>
<contactref element="ZED1" pad="128"/>
<contactref element="ZED1" pad="133"/>
<contactref element="ZED1" pad="134"/>
<contactref element="ZED1" pad="139"/>
<contactref element="ZED1" pad="140"/>
<contactref element="ZED1" pad="145"/>
<contactref element="ZED1" pad="146"/>
<contactref element="ZED1" pad="151"/>
<contactref element="ZED1" pad="152"/>
<contactref element="ZED1" pad="165"/>
<contactref element="ZED1" pad="166"/>
<contactref element="ZED1" pad="171"/>
<contactref element="ZED1" pad="172"/>
<contactref element="ZED1" pad="177"/>
<contactref element="ZED1" pad="185"/>
<contactref element="ZED1" pad="186"/>
<contactref element="ZED1" pad="191"/>
<contactref element="ZED1" pad="192"/>
<contactref element="X-WEST" pad="5"/>
<contactref element="X-WEST" pad="20"/>
<contactref element="X-WEST" pad="82"/>
<contactref element="X-WEST" pad="23"/>
<contactref element="X-WEST" pad="77"/>
<contactref element="X-EAST" pad="20"/>
<contactref element="X-EAST" pad="5"/>
<contactref element="X-EAST" pad="23"/>
<contactref element="X-EAST" pad="77"/>
<contactref element="X-EAST" pad="82"/>
<contactref element="X-WEST" pad="71"/>
<contactref element="X-WEST" pad="29"/>
<contactref element="X-WEST" pad="26"/>
<contactref element="X-WEST" pad="76"/>
<contactref element="X-EAST" pad="71"/>
<contactref element="X-EAST" pad="76"/>
<contactref element="X-EAST" pad="26"/>
<contactref element="X-EAST" pad="29"/>
<contactref element="X-EAST" pad="32"/>
<contactref element="X-EAST" pad="58"/>
<contactref element="X-EAST" pad="44"/>
<contactref element="X-EAST" pad="52"/>
<contactref element="X-EAST" pad="50"/>
<contactref element="X-EAST" pad="38"/>
<contactref element="X-EAST" pad="70"/>
<contactref element="X-EAST" pad="64"/>
<contactref element="X-EAST" pad="57"/>
<contactref element="X-EAST" pad="69"/>
<contactref element="X-EAST" pad="63"/>
<contactref element="X-EAST" pad="51"/>
<contactref element="X-EAST" pad="43"/>
<contactref element="X-EAST" pad="31"/>
<contactref element="X-EAST" pad="49"/>
<contactref element="X-EAST" pad="37"/>
<contactref element="X-WEST" pad="50"/>
<contactref element="X-WEST" pad="64"/>
<contactref element="X-WEST" pad="38"/>
<contactref element="X-WEST" pad="70"/>
<contactref element="X-WEST" pad="32"/>
<contactref element="X-WEST" pad="58"/>
<contactref element="X-WEST" pad="44"/>
<contactref element="X-WEST" pad="52"/>
<contactref element="X-WEST" pad="51"/>
<contactref element="X-WEST" pad="57"/>
<contactref element="X-WEST" pad="69"/>
<contactref element="X-WEST" pad="63"/>
<contactref element="X-WEST" pad="43"/>
<contactref element="X-WEST" pad="31"/>
<contactref element="X-WEST" pad="49"/>
<contactref element="X-WEST" pad="37"/>
<contactref element="PCIE-NORTH" pad="A18"/>
<contactref element="PCIE-NORTH" pad="A15"/>
<contactref element="PCIE-NORTH" pad="A1"/>
<contactref element="PCIE-NORTH" pad="A10"/>
<contactref element="PCIE-NORTH" pad="A4"/>
<contactref element="PCIE-NORTH" pad="A7"/>
<contactref element="PCIE-NORTH" pad="A12"/>
<contactref element="PCIE-NORTH" pad="B18"/>
<contactref element="PCIE-NORTH" pad="B15"/>
<contactref element="PCIE-SOUTH" pad="A7"/>
<contactref element="PCIE-SOUTH" pad="A18"/>
<contactref element="PCIE-SOUTH" pad="A4"/>
<contactref element="PCIE-SOUTH" pad="A12"/>
<contactref element="PCIE-SOUTH" pad="A15"/>
<contactref element="PCIE-SOUTH" pad="A10"/>
<contactref element="PCIE-SOUTH" pad="A1"/>
<contactref element="PCIE-SOUTH" pad="B18"/>
<contactref element="PCIE-SOUTH" pad="B15"/>
<contactref element="PAD9" pad="1"/>
<contactref element="PAD16" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2'" pad="2"/>
<contactref element="C1'" pad="2"/>
<contactref element="C8'" pad="2"/>
<contactref element="C7'" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4'" pad="2"/>
<contactref element="C3'" pad="2"/>
<contactref element="C6'" pad="2"/>
<contactref element="C5'" pad="2"/>
<contactref element="RFW" pad="56"/>
<contactref element="RFW" pad="72"/>
<contactref element="RFW" pad="79"/>
<contactref element="RFW" pad="92"/>
<contactref element="RFW" pad="44"/>
<contactref element="RFW" pad="33"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="RFW" pad="6"/>
<contactref element="RFW" pad="22"/>
<contactref element="U1" pad="6"/>
<contactref element="PB-SE" pad="5"/>
<contactref element="PB-NW" pad="5"/>
<contactref element="RFE" pad="56"/>
<contactref element="RFE" pad="72"/>
<contactref element="RFE" pad="79"/>
<contactref element="RFE" pad="92"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="RFE" pad="6"/>
<contactref element="RFE" pad="22"/>
<contactref element="RFE" pad="33"/>
<contactref element="RFE" pad="44"/>
<contactref element="X-EAST" pad="G2"/>
<contactref element="X-EAST" pad="G4"/>
<contactref element="X-EAST" pad="G6"/>
<contactref element="X-EAST" pad="G8"/>
<contactref element="X-EAST" pad="G10"/>
<contactref element="X-EAST" pad="G1"/>
<contactref element="X-EAST" pad="G3"/>
<contactref element="X-EAST" pad="G5"/>
<contactref element="X-EAST" pad="G7"/>
<contactref element="X-EAST" pad="G9"/>
<contactref element="X-WEST" pad="G2"/>
<contactref element="X-WEST" pad="G4"/>
<contactref element="X-WEST" pad="G6"/>
<contactref element="X-WEST" pad="G8"/>
<contactref element="X-WEST" pad="G10"/>
<contactref element="X-WEST" pad="G1"/>
<contactref element="X-WEST" pad="G3"/>
<contactref element="X-WEST" pad="G5"/>
<contactref element="X-WEST" pad="G7"/>
<contactref element="X-WEST" pad="G9"/>
<contactref element="T1" pad="2"/>
<contactref element="PAD8" pad="1"/>
<contactref element="PAD1" pad="1"/>
<contactref element="HDR-SW" pad="1"/>
<contactref element="HDR-SW" pad="2"/>
<contactref element="HDR-NE" pad="1"/>
<contactref element="HDR-NE" pad="2"/>
<contactref element="U2" pad="29"/>
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="5"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U3" pad="29"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="16"/>
<contactref element="C42" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="JX1_00_P">
<contactref element="ZED1" pad="11"/>
<contactref element="X-EAST" pad="25"/>
</signal>
<signal name="JX1_00_N">
<contactref element="ZED1" pad="13"/>
<contactref element="X-EAST" pad="27"/>
</signal>
<signal name="JX1_01_P">
<contactref element="ZED1" pad="12"/>
<contactref element="HDR-NE" pad="15"/>
</signal>
<signal name="JX1_01_N">
<contactref element="ZED1" pad="14"/>
<contactref element="HDR-NE" pad="13"/>
</signal>
<signal name="JX1_02_P">
<contactref element="ZED1" pad="17"/>
<contactref element="X-EAST" pad="22"/>
</signal>
<signal name="JX1_02_N">
<contactref element="ZED1" pad="19"/>
<contactref element="X-EAST" pad="24"/>
</signal>
<signal name="JX1_03_N">
<contactref element="ZED1" pad="20"/>
<contactref element="HDR-NE" pad="14"/>
</signal>
<signal name="JX1_03_P">
<contactref element="ZED1" pad="18"/>
<contactref element="HDR-NE" pad="16"/>
</signal>
<signal name="JX2_08_N">
<contactref element="ZED1" pad="143"/>
<contactref element="X-EAST" pad="59"/>
</signal>
<signal name="JX2_08_P">
<contactref element="ZED1" pad="141"/>
<contactref element="X-EAST" pad="61"/>
</signal>
<signal name="JX2_01_P">
<contactref element="ZED1" pad="118"/>
<contactref element="X-EAST" pad="75"/>
</signal>
<signal name="JX2_01_N">
<contactref element="ZED1" pad="120"/>
<contactref element="X-EAST" pad="73"/>
</signal>
<signal name="JX2_00_P">
<contactref element="ZED1" pad="117"/>
<contactref element="HDR-SE" pad="16"/>
</signal>
<signal name="JX2_00_N">
<contactref element="ZED1" pad="119"/>
<contactref element="HDR-SE" pad="14"/>
</signal>
<signal name="JX2_03_P">
<contactref element="ZED1" pad="124"/>
<contactref element="X-EAST" pad="80"/>
</signal>
<signal name="JX2_03_N">
<contactref element="ZED1" pad="126"/>
<contactref element="X-EAST" pad="78"/>
</signal>
<signal name="JX2_21_P">
<contactref element="ZED1" pad="182"/>
<contactref element="X-WEST" pad="24"/>
</signal>
<signal name="JX2_23_P">
<contactref element="ZED1" pad="188"/>
<contactref element="X-WEST" pad="27"/>
</signal>
<signal name="BANK13_02_P">
<contactref element="ZED1" pad="91"/>
<contactref element="PCIE-NORTH" pad="A17"/>
</signal>
<signal name="BANK13_02_N">
<contactref element="ZED1" pad="93"/>
<contactref element="PCIE-NORTH" pad="A16"/>
</signal>
<signal name="BANK13_03_P">
<contactref element="ZED1" pad="92"/>
<contactref element="PCIE-NORTH" pad="A13"/>
</signal>
<signal name="BANK13_03_N">
<contactref element="ZED1" pad="94"/>
<contactref element="PCIE-NORTH" pad="A14"/>
</signal>
<signal name="BANK13_04_P">
<contactref element="ZED1" pad="193"/>
<contactref element="PCIE-SOUTH" pad="A5"/>
</signal>
<signal name="BANK13_04_N">
<contactref element="ZED1" pad="195"/>
<contactref element="PCIE-SOUTH" pad="A6"/>
</signal>
<signal name="BANK13_06_P">
<contactref element="ZED1" pad="197"/>
<contactref element="PCIE-SOUTH" pad="A9"/>
</signal>
<signal name="BANK13_06_N">
<contactref element="ZED1" pad="199"/>
<contactref element="PCIE-SOUTH" pad="A8"/>
</signal>
<signal name="BANK13_00_P">
<contactref element="ZED1" pad="87"/>
<contactref element="PCIE-NORTH" pad="B16"/>
</signal>
<signal name="BANK13_00_N">
<contactref element="ZED1" pad="89"/>
<contactref element="PCIE-NORTH" pad="B17"/>
</signal>
<signal name="BANK13_01_P">
<contactref element="ZED1" pad="88"/>
<contactref element="RFW" pad="39"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="BANK13_01_N">
<contactref element="ZED1" pad="90"/>
<contactref element="RFW" pad="38"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="JX2_21_N">
<contactref element="ZED1" pad="184"/>
<contactref element="X-WEST" pad="22"/>
</signal>
<signal name="JX2_23_N">
<contactref element="ZED1" pad="190"/>
<contactref element="X-WEST" pad="25"/>
</signal>
<signal name="JX2_11_N">
<contactref element="ZED1" pad="150"/>
<contactref element="X-EAST" pad="54"/>
</signal>
<signal name="JX2_11_P">
<contactref element="ZED1" pad="148"/>
<contactref element="X-EAST" pad="56"/>
</signal>
<signal name="JX2_04_N">
<contactref element="ZED1" pad="131"/>
<contactref element="RFE" pad="38"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="JX2_04_P">
<contactref element="ZED1" pad="129"/>
<contactref element="RFE" pad="39"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="JX2_06_N">
<contactref element="ZED1" pad="137"/>
<contactref element="X-EAST" pad="65"/>
</signal>
<signal name="JX2_06_P">
<contactref element="ZED1" pad="135"/>
<contactref element="X-EAST" pad="67"/>
</signal>
<signal name="JX1_11_N">
<contactref element="ZED1" pad="44"/>
<contactref element="X-EAST" pad="47"/>
</signal>
<signal name="JX1_11_P">
<contactref element="ZED1" pad="42"/>
<contactref element="X-EAST" pad="45"/>
</signal>
<signal name="JX1_12_N">
<contactref element="ZED1" pad="49"/>
<contactref element="X-WEST" pad="56"/>
</signal>
<signal name="JX1_12_P">
<contactref element="ZED1" pad="47"/>
<contactref element="X-WEST" pad="54"/>
</signal>
<signal name="JX1_10_N">
<contactref element="ZED1" pad="43"/>
<contactref element="X-EAST" pad="48"/>
</signal>
<signal name="JX1_10_P">
<contactref element="ZED1" pad="41"/>
<contactref element="X-EAST" pad="46"/>
</signal>
<signal name="JX2_07_N">
<contactref element="ZED1" pad="138"/>
<contactref element="X-EAST" pad="66"/>
</signal>
<signal name="JX2_07_P">
<contactref element="ZED1" pad="136"/>
<contactref element="X-EAST" pad="68"/>
</signal>
<signal name="JX2_05_N">
<contactref element="ZED1" pad="132"/>
<contactref element="X-EAST" pad="72"/>
</signal>
<signal name="JX2_05_P">
<contactref element="ZED1" pad="130"/>
<contactref element="X-EAST" pad="74"/>
</signal>
<signal name="JX2_13_N">
<contactref element="ZED1" pad="156"/>
<contactref element="X-WEST" pad="46"/>
</signal>
<signal name="JX2_13_P">
<contactref element="ZED1" pad="154"/>
<contactref element="X-WEST" pad="48"/>
</signal>
<signal name="JX2_09_N">
<contactref element="ZED1" pad="144"/>
<contactref element="X-EAST" pad="60"/>
</signal>
<signal name="JX2_09_P">
<contactref element="ZED1" pad="142"/>
<contactref element="X-EAST" pad="62"/>
</signal>
<signal name="JX1_13_N">
<contactref element="ZED1" pad="50"/>
<contactref element="X-WEST" pad="55"/>
</signal>
<signal name="JX1_13_P">
<contactref element="ZED1" pad="48"/>
<contactref element="X-WEST" pad="53"/>
</signal>
<signal name="JX1_09_N">
<contactref element="ZED1" pad="38"/>
<contactref element="X-EAST" pad="41"/>
</signal>
<signal name="JX1_09_P">
<contactref element="ZED1" pad="36"/>
<contactref element="X-EAST" pad="39"/>
</signal>
<signal name="JX2_02_N">
<contactref element="ZED1" pad="125"/>
<contactref element="HDR-SE" pad="13"/>
</signal>
<signal name="JX1_23_N">
<contactref element="ZED1" pad="84"/>
<contactref element="PCIE-NORTH" pad="A9"/>
</signal>
<signal name="JX1_23_P">
<contactref element="ZED1" pad="82"/>
<contactref element="PCIE-NORTH" pad="A8"/>
</signal>
<signal name="JX1_07_N">
<contactref element="ZED1" pad="32"/>
<contactref element="X-EAST" pad="35"/>
</signal>
<signal name="JX1_07_P">
<contactref element="ZED1" pad="30"/>
<contactref element="X-EAST" pad="33"/>
</signal>
<signal name="JX1_04_N">
<contactref element="ZED1" pad="25"/>
<contactref element="X-EAST" pad="30"/>
</signal>
<signal name="JX1_04_P">
<contactref element="ZED1" pad="23"/>
<contactref element="X-EAST" pad="28"/>
</signal>
<signal name="JX1_14_N">
<contactref element="ZED1" pad="55"/>
<contactref element="X-WEST" pad="62"/>
</signal>
<signal name="JX2_15_P">
<contactref element="ZED1" pad="162"/>
<contactref element="X-WEST" pad="42"/>
</signal>
<signal name="JX2_15_N">
<contactref element="ZED1" pad="164"/>
<contactref element="X-WEST" pad="40"/>
</signal>
<signal name="JX1_06_N">
<contactref element="ZED1" pad="31"/>
<contactref element="X-EAST" pad="36"/>
</signal>
<signal name="JX1_06_P">
<contactref element="ZED1" pad="29"/>
<contactref element="X-EAST" pad="34"/>
</signal>
<signal name="JX2_10_N">
<contactref element="ZED1" pad="149"/>
<contactref element="X-EAST" pad="53"/>
</signal>
<signal name="JX2_10_P">
<contactref element="ZED1" pad="147"/>
<contactref element="X-EAST" pad="55"/>
</signal>
<signal name="JX2_12_N">
<contactref element="ZED1" pad="155"/>
<contactref element="X-WEST" pad="45"/>
</signal>
<signal name="JX2_12_P">
<contactref element="ZED1" pad="153"/>
<contactref element="X-WEST" pad="47"/>
</signal>
<signal name="JX2_20_N">
<contactref element="ZED1" pad="183"/>
<contactref element="PCIE-SOUTH" pad="A17"/>
</signal>
<signal name="JX2_20_P">
<contactref element="ZED1" pad="181"/>
<contactref element="PCIE-SOUTH" pad="A16"/>
</signal>
<signal name="JX1_16_N">
<contactref element="ZED1" pad="63"/>
<contactref element="X-WEST" pad="68"/>
</signal>
<signal name="JX1_16_P">
<contactref element="ZED1" pad="61"/>
<contactref element="X-WEST" pad="66"/>
</signal>
<signal name="JX2_18_N">
<contactref element="ZED1" pad="175"/>
<contactref element="PCIE-SOUTH" pad="B17"/>
</signal>
<signal name="JX2_18_P">
<contactref element="ZED1" pad="173"/>
<contactref element="PCIE-SOUTH" pad="B16"/>
</signal>
<signal name="JX2_19_N">
<contactref element="ZED1" pad="176"/>
<contactref element="X-WEST" pad="28"/>
</signal>
<signal name="JX2_19_P">
<contactref element="ZED1" pad="174"/>
<contactref element="X-WEST" pad="30"/>
</signal>
<signal name="JX2_17_N">
<contactref element="ZED1" pad="170"/>
<contactref element="X-WEST" pad="34"/>
</signal>
<signal name="JX2_17_P">
<contactref element="ZED1" pad="168"/>
<contactref element="X-WEST" pad="36"/>
</signal>
<signal name="JX1_18_N">
<contactref element="ZED1" pad="69"/>
<contactref element="X-WEST" pad="74"/>
</signal>
<signal name="JX1_18_P">
<contactref element="ZED1" pad="67"/>
<contactref element="X-WEST" pad="72"/>
</signal>
<signal name="JX2_16_N">
<contactref element="ZED1" pad="169"/>
<contactref element="X-WEST" pad="33"/>
</signal>
<signal name="JX2_16_P">
<contactref element="ZED1" pad="167"/>
<contactref element="X-WEST" pad="35"/>
</signal>
<signal name="JX1_19_N">
<contactref element="ZED1" pad="70"/>
<contactref element="PCIE-NORTH" pad="A3"/>
</signal>
<signal name="JX1_19_P">
<contactref element="ZED1" pad="68"/>
<contactref element="PCIE-NORTH" pad="A2"/>
</signal>
<signal name="JX1_17_N">
<contactref element="ZED1" pad="64"/>
<contactref element="X-WEST" pad="67"/>
</signal>
<signal name="JX1_17_P">
<contactref element="ZED1" pad="62"/>
<contactref element="X-WEST" pad="65"/>
</signal>
<signal name="CSO_NE_V">
<contactref element="PAD2" pad="1"/>
<contactref element="C4'" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C3'" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="ZED1" pad="7"/>
</signal>
<signal name="PCIE_I2C_V">
<contactref element="ZED1" pad="198"/>
<contactref element="PCIE-SOUTH" pad="B3"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="PCIE-NORTH" pad="B3"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="W_SDA">
<contactref element="X-WEST" pad="17"/>
<contactref element="RFW" pad="37"/>
</signal>
<signal name="W_SCL">
<contactref element="X-WEST" pad="15"/>
<contactref element="RFW" pad="36"/>
</signal>
<signal name="W_I2C_V">
<contactref element="X-WEST" pad="11"/>
<contactref element="PWR-SW" pad="1"/>
</signal>
<signal name="N_SCL">
<contactref element="X-EAST" pad="1"/>
<contactref element="RFE" pad="28"/>
</signal>
<signal name="N_SDA">
<contactref element="X-EAST" pad="3"/>
<contactref element="RFE" pad="30"/>
</signal>
<signal name="N_SDI">
<contactref element="X-EAST" pad="6"/>
<contactref element="RFE" pad="29"/>
</signal>
<signal name="N_SDO">
<contactref element="X-EAST" pad="4"/>
<contactref element="RFE" pad="43"/>
</signal>
<signal name="N_SCK">
<contactref element="X-EAST" pad="2"/>
<contactref element="RFE" pad="42"/>
</signal>
<signal name="N_I2C_V">
<contactref element="X-EAST" pad="9"/>
<contactref element="PWR-NE" pad="4"/>
</signal>
<signal name="S_VE_OV">
<contactref element="X-EAST" pad="99"/>
<contactref element="PB-SE" pad="4"/>
</signal>
<signal name="S_VS_OV">
<contactref element="X-EAST" pad="97"/>
<contactref element="PB-SE" pad="6"/>
</signal>
<signal name="S_VW_OV">
<contactref element="X-EAST" pad="95"/>
<contactref element="PB-SE" pad="8"/>
</signal>
<signal name="S_VE_UV">
<contactref element="X-EAST" pad="89"/>
<contactref element="PB-SE" pad="16"/>
</signal>
<signal name="S_VS_UV">
<contactref element="X-EAST" pad="87"/>
<contactref element="PB-SE" pad="18"/>
</signal>
<signal name="S_VW_UV">
<contactref element="X-EAST" pad="85"/>
<contactref element="PB-SE" pad="20"/>
</signal>
<signal name="S_VE_CV">
<contactref element="X-EAST" pad="100"/>
<contactref element="PB-SE" pad="13"/>
</signal>
<signal name="S_VS_CV">
<contactref element="X-EAST" pad="98"/>
<contactref element="PB-SE" pad="15"/>
</signal>
<signal name="S_VW_CV">
<contactref element="X-EAST" pad="96"/>
<contactref element="PB-SE" pad="17"/>
</signal>
<signal name="S_CHK_V">
<contactref element="X-EAST" pad="92"/>
<contactref element="PB-SE" pad="14"/>
</signal>
<signal name="E_VE_UV">
<contactref element="X-EAST" pad="91"/>
<contactref element="PB-SE" pad="12"/>
</signal>
<signal name="E_VE_OV">
<contactref element="X-EAST" pad="93"/>
<contactref element="PB-SE" pad="10"/>
</signal>
<signal name="E_VE_CV">
<contactref element="X-EAST" pad="90"/>
<contactref element="PB-SE" pad="19"/>
</signal>
<signal name="N_SPI_V">
<contactref element="X-EAST" pad="10"/>
<contactref element="PWR-NE" pad="2"/>
</signal>
<signal name="E_SCL">
<contactref element="X-EAST" pad="15"/>
<contactref element="RFE" pad="36"/>
</signal>
<signal name="E_SDA">
<contactref element="X-EAST" pad="17"/>
<contactref element="RFE" pad="37"/>
</signal>
<signal name="E_SPI_V">
<contactref element="X-EAST" pad="21"/>
<contactref element="PWR-NE" pad="3"/>
</signal>
<signal name="E_I2C_V">
<contactref element="X-EAST" pad="11"/>
<contactref element="PWR-NE" pad="1"/>
</signal>
<signal name="E_SCK">
<contactref element="X-EAST" pad="12"/>
<contactref element="RFE" pad="21"/>
</signal>
<signal name="E_EN">
<contactref element="X-EAST" pad="14"/>
<contactref element="RFE" pad="20"/>
</signal>
<signal name="E_SDI">
<contactref element="X-EAST" pad="16"/>
<contactref element="RFE" pad="24"/>
</signal>
<signal name="E_SDO">
<contactref element="X-EAST" pad="18"/>
<contactref element="RFE" pad="25"/>
</signal>
<signal name="N_VW_OV">
<contactref element="X-WEST" pad="99"/>
<contactref element="PB-NW" pad="4"/>
</signal>
<signal name="N_VN_OV">
<contactref element="X-WEST" pad="97"/>
<contactref element="PB-NW" pad="6"/>
</signal>
<signal name="N_VE_OV">
<contactref element="X-WEST" pad="95"/>
<contactref element="PB-NW" pad="8"/>
</signal>
<signal name="N_VW_UV">
<contactref element="X-WEST" pad="89"/>
<contactref element="PB-NW" pad="16"/>
</signal>
<signal name="N_VN_UV">
<contactref element="X-WEST" pad="87"/>
<contactref element="PB-NW" pad="18"/>
</signal>
<signal name="N_VE_UV">
<contactref element="X-WEST" pad="85"/>
<contactref element="PB-NW" pad="20"/>
</signal>
<signal name="N_VW_CV">
<contactref element="X-WEST" pad="100"/>
<contactref element="PB-NW" pad="13"/>
</signal>
<signal name="N_VN_CV">
<contactref element="X-WEST" pad="98"/>
<contactref element="PB-NW" pad="15"/>
</signal>
<signal name="N_VE_CV">
<contactref element="X-WEST" pad="96"/>
<contactref element="PB-NW" pad="17"/>
</signal>
<signal name="N_CHK_V">
<contactref element="X-WEST" pad="92"/>
<contactref element="PB-NW" pad="14"/>
</signal>
<signal name="S_SDO">
<contactref element="X-WEST" pad="4"/>
<contactref element="RFW" pad="29"/>
</signal>
<signal name="S_SCK">
<contactref element="X-WEST" pad="2"/>
<contactref element="RFW" pad="28"/>
</signal>
<signal name="S_SCL">
<contactref element="X-WEST" pad="1"/>
<contactref element="RFW" pad="34"/>
</signal>
<signal name="W_VW_UV">
<contactref element="X-WEST" pad="91"/>
<contactref element="PB-NW" pad="12"/>
</signal>
<signal name="TCK">
<contactref element="X-WEST" pad="12"/>
<contactref element="RFW" pad="43"/>
</signal>
<signal name="S_SDA">
<contactref element="X-WEST" pad="3"/>
<contactref element="RFW" pad="35"/>
</signal>
<signal name="S_SPI_V">
<contactref element="X-WEST" pad="10"/>
<contactref element="PWR-SW" pad="2"/>
</signal>
<signal name="S_I2C_V">
<contactref element="X-WEST" pad="9"/>
<contactref element="PWR-SW" pad="4"/>
</signal>
<signal name="S_SDI">
<contactref element="X-WEST" pad="6"/>
<contactref element="RFW" pad="30"/>
</signal>
<signal name="W_VW_OV">
<contactref element="X-WEST" pad="93"/>
<contactref element="PB-NW" pad="10"/>
</signal>
<signal name="W_VW_CV">
<contactref element="X-WEST" pad="90"/>
<contactref element="PB-NW" pad="19"/>
</signal>
<signal name="TDO">
<contactref element="X-WEST" pad="18"/>
<contactref element="RFW" pad="40"/>
</signal>
<signal name="TDI">
<contactref element="X-WEST" pad="16"/>
<contactref element="RFW" pad="41"/>
</signal>
<signal name="TMS">
<contactref element="X-WEST" pad="14"/>
<contactref element="RFW" pad="42"/>
</signal>
<signal name="JTAG_V">
<contactref element="X-WEST" pad="21"/>
<contactref element="PWR-SW" pad="3"/>
</signal>
<signal name="JX1_14_P">
<contactref element="ZED1" pad="53"/>
<contactref element="X-WEST" pad="60"/>
</signal>
<signal name="JX2_02_P">
<contactref element="ZED1" pad="123"/>
<contactref element="HDR-SE" pad="15"/>
</signal>
<signal name="JX1_05_N">
<contactref element="ZED1" pad="26"/>
<contactref element="RFE" pad="35"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="JX1_05_P">
<contactref element="ZED1" pad="24"/>
<contactref element="RFE" pad="34"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="JX1_15_N">
<contactref element="ZED1" pad="56"/>
<contactref element="X-WEST" pad="61"/>
</signal>
<signal name="JX1_15_P">
<contactref element="ZED1" pad="54"/>
<contactref element="X-WEST" pad="59"/>
</signal>
<signal name="JX1_20_P">
<contactref element="ZED1" pad="73"/>
<contactref element="X-WEST" pad="78"/>
</signal>
<signal name="JX1_20_N">
<contactref element="ZED1" pad="75"/>
<contactref element="X-WEST" pad="80"/>
</signal>
<signal name="JX1_21_P">
<contactref element="ZED1" pad="74"/>
<contactref element="PCIE-NORTH" pad="A5"/>
</signal>
<signal name="JX1_21_N">
<contactref element="ZED1" pad="76"/>
<contactref element="PCIE-NORTH" pad="A6"/>
</signal>
<signal name="JX1_22_P">
<contactref element="ZED1" pad="81"/>
<contactref element="X-WEST" pad="73"/>
</signal>
<signal name="JX1_22_N">
<contactref element="ZED1" pad="83"/>
<contactref element="X-WEST" pad="75"/>
</signal>
<signal name="JX2_22_P">
<contactref element="ZED1" pad="187"/>
<contactref element="PCIE-SOUTH" pad="A14"/>
</signal>
<signal name="JX2_22_N">
<contactref element="ZED1" pad="189"/>
<contactref element="PCIE-SOUTH" pad="A13"/>
</signal>
<signal name="JX2_14_N">
<contactref element="ZED1" pad="163"/>
<contactref element="X-WEST" pad="39"/>
</signal>
<signal name="JX2_14_P">
<contactref element="ZED1" pad="161"/>
<contactref element="X-WEST" pad="41"/>
</signal>
<signal name="JX1_08_P">
<contactref element="ZED1" pad="35"/>
<contactref element="X-EAST" pad="40"/>
</signal>
<signal name="JX1_08_N">
<contactref element="ZED1" pad="37"/>
<contactref element="X-EAST" pad="42"/>
</signal>
<signal name="BANK13_05_N">
<contactref element="ZED1" pad="196"/>
<contactref element="PCIE-SOUTH" pad="A3"/>
</signal>
<signal name="BANK13_05_P">
<contactref element="ZED1" pad="194"/>
<contactref element="PCIE-SOUTH" pad="A2"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$8">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="N$35">
</signal>
<signal name="N$36">
</signal>
<signal name="N$37">
</signal>
<signal name="N$38">
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="JX1_SE_0">
<contactref element="ZED1" pad="9"/>
<contactref element="RFE" pad="88"/>
<contactref element="R8" pad="1"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="JX1_SE_1">
<contactref element="ZED1" pad="10"/>
</signal>
<signal name="JX2_SE_0">
<contactref element="ZED1" pad="113"/>
</signal>
<signal name="JX2_SE_1">
<contactref element="ZED1" pad="114"/>
</signal>
<signal name="BANK13_SE_0">
<contactref element="ZED1" pad="200"/>
<contactref element="RFW" pad="88"/>
<contactref element="R7" pad="1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="VP_0_P">
<contactref element="ZED1" pad="97"/>
</signal>
<signal name="VP_0_N">
<contactref element="ZED1" pad="99"/>
</signal>
<signal name="DXP_0_P">
<contactref element="ZED1" pad="98"/>
</signal>
<signal name="DXP_0_N">
<contactref element="ZED1" pad="100"/>
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$55">
</signal>
<signal name="N$60">
</signal>
<signal name="N$62">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="B_SDA">
<contactref element="PB-SE" pad="3"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="B_SCL">
<contactref element="PB-SE" pad="1"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="A_SCL">
<contactref element="PB-NW" pad="1"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="A_SDA">
<contactref element="PB-NW" pad="3"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="!SS!_W">
<contactref element="RFW" pad="27"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="SCK_W">
<contactref element="RFW" pad="31"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="SDI_W">
<contactref element="RFW" pad="49"/>
<contactref element="U2" pad="21"/>
</signal>
<signal name="SDO_W">
<contactref element="RFW" pad="32"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$209">
<contactref element="PCIE-SOUTH" pad="A11"/>
</signal>
<signal name="PCIE_S_SCL">
<contactref element="PCIE-SOUTH" pad="B2"/>
<contactref element="U1" pad="8"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="PCIE_S_IO0">
<contactref element="PCIE-SOUTH" pad="B4"/>
<contactref element="RFW" pad="1"/>
</signal>
<signal name="PCIE_S_IO2">
<contactref element="PCIE-SOUTH" pad="B6"/>
<contactref element="RFW" pad="98"/>
</signal>
<signal name="PCIE_S_IO4">
<contactref element="PCIE-SOUTH" pad="B8"/>
<contactref element="RFW" pad="96"/>
</signal>
<signal name="PCIE_S_IO6">
<contactref element="PCIE-SOUTH" pad="B10"/>
<contactref element="RFW" pad="84"/>
</signal>
<signal name="PCIE_N_IO6">
<contactref element="PCIE-NORTH" pad="B10"/>
<contactref element="RFW" pad="69"/>
</signal>
<signal name="PCIE_N_IO4">
<contactref element="PCIE-NORTH" pad="B8"/>
<contactref element="RFW" pad="71"/>
</signal>
<signal name="PCIE_N_IO2">
<contactref element="PCIE-NORTH" pad="B6"/>
<contactref element="RFW" pad="74"/>
</signal>
<signal name="PCIE_N_IO0">
<contactref element="PCIE-NORTH" pad="B4"/>
<contactref element="RFW" pad="83"/>
</signal>
<signal name="PCIE_N_SCL">
<contactref element="PCIE-NORTH" pad="B2"/>
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$256">
<contactref element="PCIE-NORTH" pad="A11"/>
</signal>
<signal name="C_SI_W">
<contactref element="PAD12" pad="1"/>
<contactref element="RFW" pad="19"/>
</signal>
<signal name="C_CK_W">
<contactref element="PAD13" pad="1"/>
<contactref element="RFW" pad="18"/>
</signal>
<signal name="C_SO_W">
<contactref element="PAD14" pad="1"/>
<contactref element="RFW" pad="15"/>
</signal>
<signal name="C_SI_E">
<contactref element="PAD4" pad="1"/>
<contactref element="RFE" pad="19"/>
</signal>
<signal name="C_CK_E">
<contactref element="PAD5" pad="1"/>
<contactref element="RFE" pad="18"/>
</signal>
<signal name="C_SO_E">
<contactref element="PAD6" pad="1"/>
<contactref element="RFE" pad="15"/>
</signal>
<signal name="CSO_NW_V">
<contactref element="PAD15" pad="1"/>
<contactref element="C1'" pad="1"/>
<contactref element="C2'" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="PWR-NW" pad="1"/>
</signal>
<signal name="RFAB_W_V">
<contactref element="RFW" pad="50"/>
<contactref element="RFW" pad="100"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="PWR-NW" pad="3"/>
</signal>
<signal name="CSO_SE_V">
<contactref element="PAD7" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7'" pad="1"/>
<contactref element="C8'" pad="1"/>
<contactref element="PWR-SE" pad="1"/>
</signal>
<signal name="RFAB_E_V">
<contactref element="RFE" pad="50"/>
<contactref element="RFE" pad="100"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="PWR-SE" pad="3"/>
</signal>
<signal name="CSO_SW_V">
<contactref element="PAD10" pad="1"/>
<contactref element="C6'" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5'" pad="1"/>
<contactref element="ZED1" pad="112"/>
</signal>
<signal name="PCIE_N_V">
<contactref element="ZED1" pad="80"/>
<contactref element="ZED1" pad="79"/>
<contactref element="PCIE-NORTH" pad="B13"/>
</signal>
<signal name="PCIE_S_V">
<contactref element="ZED1" pad="180"/>
<contactref element="ZED1" pad="179"/>
<contactref element="PCIE-SOUTH" pad="B13"/>
</signal>
<signal name="RES4">
<contactref element="X-EAST" pad="79"/>
</signal>
<signal name="RES5">
<contactref element="X-EAST" pad="81"/>
</signal>
<signal name="RES6">
<contactref element="X-EAST" pad="83"/>
</signal>
<signal name="RES1">
<contactref element="X-WEST" pad="79"/>
</signal>
<signal name="RES2">
<contactref element="X-WEST" pad="81"/>
</signal>
<signal name="RES3">
<contactref element="X-WEST" pad="83"/>
</signal>
<signal name="N_VW_RS">
<contactref element="PB-NW" pad="9"/>
<contactref element="X-WEST" pad="84"/>
</signal>
<signal name="N_VN_RS">
<contactref element="PB-NW" pad="11"/>
<contactref element="X-WEST" pad="86"/>
</signal>
<signal name="N_VE_RS">
<contactref element="PB-NW" pad="7"/>
<contactref element="X-WEST" pad="88"/>
</signal>
<signal name="S_VE_RS">
<contactref element="X-EAST" pad="84"/>
<contactref element="PB-SE" pad="9"/>
</signal>
<signal name="S_VS_RS">
<contactref element="X-EAST" pad="86"/>
<contactref element="PB-SE" pad="11"/>
</signal>
<signal name="S_VW_RS">
<contactref element="X-EAST" pad="88"/>
<contactref element="PB-SE" pad="7"/>
</signal>
<signal name="SN_W">
<contactref element="RFW" pad="48"/>
<contactref element="U2" pad="22"/>
</signal>
<signal name="DONE_W">
<contactref element="RFW" pad="76"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="INITN_W">
<contactref element="RFW" pad="77"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="PROGRAMN_W">
<contactref element="RFW" pad="81"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="JTAGENB_W">
<contactref element="RFW" pad="82"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="TMS_W">
<contactref element="RFW" pad="90"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="TCK_W">
<contactref element="RFW" pad="91"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="TDI_W">
<contactref element="RFW" pad="94"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="TDO_W">
<contactref element="RFW" pad="95"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="PCIE_SDA">
<contactref element="RFW" pad="85"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="PCIE_SCL">
<contactref element="RFW" pad="86"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="PCIE_S_5V">
<contactref element="PCIE-SOUTH" pad="B12"/>
<contactref element="ZED1" pad="159"/>
<contactref element="ZED1" pad="160"/>
</signal>
<signal name="PCIE_N_5V">
<contactref element="PCIE-NORTH" pad="B12"/>
<contactref element="ZED1" pad="60"/>
<contactref element="ZED1" pad="59"/>
</signal>
<signal name="XX3_P">
<contactref element="RFW" pad="24"/>
<contactref element="HDR-SW" pad="14"/>
</signal>
<signal name="XX4_P">
<contactref element="RFW" pad="20"/>
<contactref element="HDR-SW" pad="13"/>
</signal>
<signal name="XX4_N">
<contactref element="RFW" pad="21"/>
<contactref element="HDR-SW" pad="15"/>
</signal>
<signal name="XX3_N">
<contactref element="RFW" pad="25"/>
<contactref element="HDR-SW" pad="16"/>
</signal>
<signal name="XX2_P">
<contactref element="RFW" pad="53"/>
<contactref element="HDR-NW" pad="16"/>
</signal>
<signal name="XX1_P">
<contactref element="RFW" pad="51"/>
<contactref element="HDR-NW" pad="15"/>
</signal>
<signal name="XX2_N">
<contactref element="RFW" pad="54"/>
<contactref element="HDR-NW" pad="14"/>
</signal>
<signal name="XX1_N">
<contactref element="RFW" pad="52"/>
<contactref element="HDR-NW" pad="13"/>
</signal>
<signal name="PCIE_N_SDA">
<contactref element="PCIE-NORTH" pad="B1"/>
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PCIE_S_SDA">
<contactref element="PCIE-SOUTH" pad="B1"/>
<contactref element="U1" pad="7"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="PCIE_S_IO1">
<contactref element="PCIE-SOUTH" pad="B5"/>
<contactref element="RFW" pad="2"/>
</signal>
<signal name="PCIE_S_IO3">
<contactref element="PCIE-SOUTH" pad="B7"/>
<contactref element="RFW" pad="99"/>
</signal>
<signal name="PCIE_S_IO5">
<contactref element="PCIE-SOUTH" pad="B9"/>
<contactref element="RFW" pad="97"/>
</signal>
<signal name="PCIE_S_IO7">
<contactref element="PCIE-SOUTH" pad="B11"/>
<contactref element="RFW" pad="87"/>
</signal>
<signal name="PCIE_N_IO1">
<contactref element="PCIE-NORTH" pad="B5"/>
<contactref element="RFW" pad="78"/>
</signal>
<signal name="PCIE_N_IO3">
<contactref element="PCIE-NORTH" pad="B7"/>
<contactref element="RFW" pad="75"/>
</signal>
<signal name="PCIE_N_IO5">
<contactref element="PCIE-NORTH" pad="B9"/>
<contactref element="RFW" pad="70"/>
</signal>
<signal name="PCIE_N_IO7">
<contactref element="PCIE-NORTH" pad="B11"/>
<contactref element="RFW" pad="68"/>
</signal>
<signal name="SH_NW_IO0">
<contactref element="RFW" pad="67"/>
<contactref element="HDR-NW" pad="4"/>
</signal>
<signal name="SH_SW_IO0">
<contactref element="RFW" pad="4"/>
<contactref element="HDR-SW" pad="4"/>
</signal>
<signal name="SH_SW_IO1">
<contactref element="RFW" pad="3"/>
<contactref element="HDR-SW" pad="3"/>
</signal>
<signal name="SH_SW_IO2">
<contactref element="RFW" pad="8"/>
<contactref element="HDR-SW" pad="6"/>
</signal>
<signal name="SH_SW_IO6">
<contactref element="RFW" pad="12"/>
<contactref element="HDR-SW" pad="10"/>
</signal>
<signal name="SH_SW_IO8">
<contactref element="RFW" pad="16"/>
<contactref element="HDR-SW" pad="12"/>
</signal>
<signal name="SH_SW_IO3">
<contactref element="RFW" pad="7"/>
<contactref element="HDR-SW" pad="5"/>
</signal>
<signal name="SH_SW_IO4">
<contactref element="RFW" pad="10"/>
<contactref element="HDR-SW" pad="8"/>
</signal>
<signal name="SH_SW_IO7">
<contactref element="RFW" pad="13"/>
<contactref element="HDR-SW" pad="9"/>
</signal>
<signal name="SH_SW_IO9">
<contactref element="RFW" pad="17"/>
<contactref element="HDR-SW" pad="11"/>
</signal>
<signal name="SH_SW_IO5">
<contactref element="RFW" pad="9"/>
<contactref element="HDR-SW" pad="7"/>
</signal>
<signal name="SH_NW_IO2">
<contactref element="RFW" pad="65"/>
<contactref element="HDR-NW" pad="6"/>
</signal>
<signal name="SH_NW_IO4">
<contactref element="RFW" pad="63"/>
<contactref element="HDR-NW" pad="8"/>
</signal>
<signal name="SH_NW_IO6">
<contactref element="RFW" pad="60"/>
<contactref element="HDR-NW" pad="10"/>
</signal>
<signal name="SH_NW_IO8">
<contactref element="RFW" pad="58"/>
<contactref element="HDR-NW" pad="12"/>
</signal>
<signal name="SH_NW_IO9">
<contactref element="RFW" pad="57"/>
<contactref element="HDR-NW" pad="11"/>
</signal>
<signal name="SH_NW_IO7">
<contactref element="RFW" pad="59"/>
<contactref element="HDR-NW" pad="9"/>
</signal>
<signal name="SH_NW_IO5">
<contactref element="RFW" pad="62"/>
<contactref element="HDR-NW" pad="7"/>
</signal>
<signal name="SH_NW_IO3">
<contactref element="RFW" pad="64"/>
<contactref element="HDR-NW" pad="5"/>
</signal>
<signal name="SH_NW_IO1">
<contactref element="RFW" pad="66"/>
<contactref element="HDR-NW" pad="3"/>
</signal>
<signal name="!SS!_E">
<contactref element="RFE" pad="27"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="SCK_E">
<contactref element="RFE" pad="31"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="SDI_E">
<contactref element="RFE" pad="49"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="SDO_E">
<contactref element="RFE" pad="32"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="N_IO0">
<contactref element="RFE" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="E_IO1">
<contactref element="RFE" pad="98"/>
</signal>
<signal name="E_IO3">
<contactref element="RFE" pad="96"/>
</signal>
<signal name="S_IO4">
<contactref element="RFE" pad="69"/>
</signal>
<signal name="S_IO2">
<contactref element="RFE" pad="71"/>
</signal>
<signal name="S_IO0">
<contactref element="RFE" pad="75"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="E_IO6">
<contactref element="RFE" pad="84"/>
</signal>
<signal name="SN_E">
<contactref element="RFE" pad="48"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="DONE_E">
<contactref element="RFE" pad="76"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="INITN_E">
<contactref element="RFE" pad="77"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="PROGRAMN_E">
<contactref element="RFE" pad="81"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="JTAGENB_E">
<contactref element="RFE" pad="82"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="TMS_E">
<contactref element="RFE" pad="90"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="TCK_E">
<contactref element="RFE" pad="91"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="TDI_E">
<contactref element="RFE" pad="94"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="TDO_E">
<contactref element="RFE" pad="95"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="IO_SDA">
<contactref element="RFE" pad="85"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="IO_SCL">
<contactref element="RFE" pad="86"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="S_IO7">
<contactref element="RFE" pad="53"/>
</signal>
<signal name="S_IO9">
<contactref element="RFE" pad="51"/>
</signal>
<signal name="S_IO6">
<contactref element="RFE" pad="54"/>
</signal>
<signal name="S_IO8">
<contactref element="RFE" pad="52"/>
</signal>
<signal name="N_IO1">
<contactref element="RFE" pad="2"/>
</signal>
<signal name="E_IO0">
<contactref element="RFE" pad="99"/>
</signal>
<signal name="E_IO2">
<contactref element="RFE" pad="97"/>
</signal>
<signal name="E_IO5">
<contactref element="RFE" pad="87"/>
</signal>
<signal name="E_IO7">
<contactref element="RFE" pad="83"/>
</signal>
<signal name="S_IO1">
<contactref element="RFE" pad="74"/>
</signal>
<signal name="S_IO3">
<contactref element="RFE" pad="70"/>
</signal>
<signal name="S_IO5">
<contactref element="RFE" pad="68"/>
</signal>
<signal name="SH_SE_IO0">
<contactref element="RFE" pad="67"/>
<contactref element="HDR-SE" pad="4"/>
</signal>
<signal name="SH_NE_IO0">
<contactref element="RFE" pad="4"/>
<contactref element="HDR-NE" pad="4"/>
</signal>
<signal name="SH_NE_IO1">
<contactref element="RFE" pad="3"/>
<contactref element="HDR-NE" pad="3"/>
</signal>
<signal name="SH_NE_IO2">
<contactref element="RFE" pad="8"/>
<contactref element="HDR-NE" pad="6"/>
</signal>
<signal name="SH_NE_IO6">
<contactref element="RFE" pad="12"/>
<contactref element="HDR-NE" pad="10"/>
</signal>
<signal name="SH_NE_IO8">
<contactref element="RFE" pad="16"/>
<contactref element="HDR-NE" pad="12"/>
</signal>
<signal name="SH_NE_IO3">
<contactref element="RFE" pad="7"/>
<contactref element="HDR-NE" pad="5"/>
</signal>
<signal name="SH_NE_IO4">
<contactref element="RFE" pad="10"/>
<contactref element="HDR-NE" pad="8"/>
</signal>
<signal name="SH_NE_IO7">
<contactref element="RFE" pad="13"/>
<contactref element="HDR-NE" pad="9"/>
</signal>
<signal name="SH_NE_IO9">
<contactref element="RFE" pad="17"/>
<contactref element="HDR-NE" pad="11"/>
</signal>
<signal name="SH_NE_IO5">
<contactref element="RFE" pad="9"/>
<contactref element="HDR-NE" pad="7"/>
</signal>
<signal name="SH_SE_IO2">
<contactref element="RFE" pad="65"/>
<contactref element="HDR-SE" pad="6"/>
</signal>
<signal name="SH_SE_IO4">
<contactref element="RFE" pad="63"/>
<contactref element="HDR-SE" pad="8"/>
</signal>
<signal name="SH_SE_IO6">
<contactref element="RFE" pad="60"/>
<contactref element="HDR-SE" pad="10"/>
</signal>
<signal name="SH_SE_IO8">
<contactref element="RFE" pad="58"/>
<contactref element="HDR-SE" pad="12"/>
</signal>
<signal name="SH_SE_IO9">
<contactref element="RFE" pad="57"/>
<contactref element="HDR-SE" pad="11"/>
</signal>
<signal name="SH_SE_IO7">
<contactref element="RFE" pad="59"/>
<contactref element="HDR-SE" pad="9"/>
</signal>
<signal name="SH_SE_IO5">
<contactref element="RFE" pad="62"/>
<contactref element="HDR-SE" pad="7"/>
</signal>
<signal name="SH_SE_IO3">
<contactref element="RFE" pad="64"/>
<contactref element="HDR-SE" pad="5"/>
</signal>
<signal name="SH_SE_IO1">
<contactref element="RFE" pad="66"/>
<contactref element="HDR-SE" pad="3"/>
</signal>
<signal name="C_EN_E">
<contactref element="PAD3" pad="1"/>
<contactref element="RFE" pad="14"/>
</signal>
<signal name="C_EN_W">
<contactref element="PAD11" pad="1"/>
<contactref element="RFW" pad="14"/>
</signal>
<signal name="PCIE_S_VCCIO">
<contactref element="PCIE-SOUTH" pad="B14"/>
<contactref element="ZED1" pad="178"/>
</signal>
<signal name="PEX_S_V">
<contactref element="ZED1" pad="157"/>
<contactref element="ZED1" pad="158"/>
<contactref element="SP1" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="PEX_N_V">
<contactref element="ZED1" pad="58"/>
<contactref element="ZED1" pad="57"/>
<contactref element="JP1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="PCIE_N_VCCIO">
<contactref element="PCIE-NORTH" pad="B14"/>
<contactref element="ZED1" pad="78"/>
</signal>
<signal name="N$105">
<contactref element="JP1" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="C43" pad="2"/>
</signal>
<signal name="N$115">
<contactref element="SP1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$112">
<contactref element="R13" pad="1"/>
<contactref element="T2" pad="3"/>
<contactref element="C44" pad="2"/>
</signal>
<signal name="N$113">
<contactref element="D1" pad="C"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N_SPI_EN">
<contactref element="X-EAST" pad="8"/>
<contactref element="RFE" pad="45"/>
</signal>
<signal name="N_I2C_EN">
<contactref element="X-EAST" pad="7"/>
<contactref element="U3" pad="28"/>
</signal>
<signal name="E_I2C_EN">
<contactref element="X-EAST" pad="13"/>
<contactref element="U3" pad="27"/>
</signal>
<signal name="!E_RESET!">
<contactref element="X-EAST" pad="19"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="W_I2C_EN">
<contactref element="X-WEST" pad="13"/>
<contactref element="U2" pad="27"/>
</signal>
<signal name="S_SPI_EN">
<contactref element="X-WEST" pad="8"/>
<contactref element="RFW" pad="45"/>
</signal>
<signal name="S_I2C_EN">
<contactref element="X-WEST" pad="7"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="!W_RESET!">
<contactref element="X-WEST" pad="19"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="S_CHK_EN">
<contactref element="X-EAST" pad="94"/>
</signal>
<signal name="N_CHK_EN">
<contactref element="X-WEST" pad="94"/>
</signal>
<signal name="N$1111">
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="C43" pad="1"/>
</signal>
<signal name="N$1112">
<contactref element="R11" pad="1"/>
<contactref element="T2" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="A_!RST">
<contactref element="PB-NW" pad="2"/>
<contactref element="U2" pad="26"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="B_!RST">
<contactref element="PB-SE" pad="2"/>
<contactref element="U3" pad="26"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="PB22B_W">
<contactref element="RFW" pad="47"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="PB22B_E">
<contactref element="U3" pad="23"/>
<contactref element="RFE" pad="47"/>
</signal>
<signal name="SH_NW_VIO">
<contactref element="HDR-NW" pad="1"/>
<contactref element="PWR-NW" pad="2"/>
<contactref element="RFW" pad="93"/>
<contactref element="RFW" pad="80"/>
<contactref element="RFW" pad="5"/>
<contactref element="RFW" pad="11"/>
<contactref element="RFW" pad="23"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="RFW" pad="73"/>
<contactref element="RFW" pad="55"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="RFW" pad="26"/>
<contactref element="RFW" pad="46"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="C41" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="SH_NW_V">
<contactref element="HDR-NW" pad="2"/>
<contactref element="PWR-NW" pad="4"/>
</signal>
<signal name="SH_SE_VIO">
<contactref element="HDR-SE" pad="1"/>
<contactref element="PWR-SE" pad="2"/>
<contactref element="RFE" pad="93"/>
<contactref element="RFE" pad="80"/>
<contactref element="RFE" pad="5"/>
<contactref element="RFE" pad="11"/>
<contactref element="RFE" pad="23"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="RFE" pad="73"/>
<contactref element="RFE" pad="55"/>
<contactref element="RFE" pad="46"/>
<contactref element="RFE" pad="26"/>
<contactref element="C40" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="U3" pad="17"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="SH_SE_V">
<contactref element="HDR-SE" pad="2"/>
<contactref element="PWR-SE" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
