(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 28)
    (no_connects 0)
    (area 127.924999 67.924999 184.075001 125.075001)
    (thickness 1.6)
    (drawings 27)
    (tracks 111)
    (zones 0)
    (modules 11)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.0254)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 3V3)
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(P1-Pad2)")
  (net 6 "Net-(P1-Pad3)")
  (net 7 "Net-(P1-Pad4)")
  (net 8 "Net-(P1-Pad5)")
  (net 9 GND)
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R3-Pad1)")
  (net 13 "Net-(SW1-Pad2)")
  (net 14 CE)
  (net 15 CSN)
  (net 16 "Net-(U1-Pad5)")
  (net 17 "Net-(U1-Pad6)")
  (net 18 "Net-(U1-Pad7)")
  (net 19 "Net-(U1-Pad8)")
  (net 20 "Net-(U2-Pad16)")
  (net 21 "Net-(U2-Pad14)")
  (net 22 "Net-(U2-Pad12)")
  (net 23 "Net-(U2-Pad11)")
  (net 24 "Net-(U2-Pad10)")
  (net 25 "Net-(U2-Pad9)")
  (net 26 "Net-(U2-Pad8)")
  (net 27 "Net-(U2-Pad7)")
  (net 28 "Net-(U2-Pad1)")
  (net 29 "Net-(U2-Pad17)")
  (net 30 "Net-(U2-Pad19)")
  (net 31 "Net-(U2-Pad20)")
  (net 32 "Net-(U2-Pad24)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.0254)
    (uvia_drill 0)
    (add_net CE)
    (add_net CSN)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (net_class Power ""
    (clearance 0.3048)
    (trace_width 0.6096)
    (via_dia 1.3716)
    (via_drill 0.6858)
    (uvia_dia 0.0254)
    (uvia_drill 0)
    (add_net 3V3)
    (add_net GND)
  )
  (module AdafruitFeather:ADAFRUIT_FEATHER (layer F.Cu) (tedit 58446256)
    (at 160.02 99.06 90)
    (fp_text reference U2 (at -26.416 0 180) (layer F.SilkS) hide)
    (fp_text value ADAFRUIT_FEATHER (at -24.384 0 180) (layer F.Fab) hide)
    (pad "" thru_hole circle (at -22.86 -8.89 90) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -22.86 8.89 90) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 22.86 8.89 90) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 22.86 -8.89 90) (size 3.302 3.302) (drill 2.54) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -19.05 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U2-Pad16)"))
    (pad 15 thru_hole circle (at -16.51 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 2 3V3))
    (pad 14 thru_hole circle (at -13.97 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U2-Pad14)"))
    (pad 13 thru_hole circle (at -11.43 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 12 thru_hole circle (at -8.89 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U2-Pad12)"))
    (pad 11 thru_hole circle (at -6.35 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U2-Pad11)"))
    (pad 10 thru_hole circle (at -3.81 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad10)"))
    (pad 9 thru_hole circle (at -1.27 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at 1.27 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at 3.81 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at 6.35 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad5)"))
    (pad 5 thru_hole circle (at 8.89 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad6)"))
    (pad 4 thru_hole circle (at 11.43 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad7)"))
    (pad 3 thru_hole circle (at 13.97 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad4)"))
    (pad 2 thru_hole circle (at 16.51 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad5)"))
    (pad 1 thru_hole rect (at 19.05 10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U2-Pad1)"))
    (pad 18 thru_hole circle (at -6.35 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SW1-Pad2)"))
    (pad 17 thru_hole rect (at -8.89 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad17)"))
    (pad 19 thru_hole circle (at -3.81 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at -1.27 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U2-Pad20)"))
    (pad 21 thru_hole circle (at 1.27 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R1-Pad1)"))
    (pad 22 thru_hole circle (at 3.81 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(R2-Pad1)"))
    (pad 23 thru_hole circle (at 6.35 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R3-Pad1)"))
    (pad 24 thru_hole circle (at 8.89 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 11.43 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 15 CSN))
    (pad 26 thru_hole circle (at 13.97 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 14 CE))
    (pad 27 thru_hole circle (at 16.51 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad3)"))
    (pad 28 thru_hole circle (at 19.05 -10.16 90) (size 1.778 1.778) (drill 0.9906) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58446247)
    (at 142 110)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module LEDs:LED-RGB-5MM_Common_Cathode (layer F.Cu) (tedit 584474C5)
    (at 177.8 114.3)
    (descr "5mm common cathode RGB LED")
    (tags "RGB LED 5mm Common Cathode")
    (fp_text reference D1 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value LED_RBG (at 0 6.25) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 4 thru_hole oval (at 0 3.81) (size 1.905 1.1176) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad4)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58445F1B)
    (at 142.24 96.52 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value R (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58445F17)
    (at 142.24 92.71 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value R (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58445F13)
    (at 142.24 88.9 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value R (at 5.08 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5844623D)
    (at 142 82)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AdafruitFeather:Socket_nRF24L01 (layer F.Cu) (tedit 58438BC9)
    (at 157.48 80.01 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference U1 (at 3.81 -2.54 270) (layer F.SilkS) hide)
    (fp_text value nRF24L01+ (at 0 -3.1 270) (layer F.Fab))
    (pad 2 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 3V3))
    (pad 1 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 4 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 CSN))
    (pad 3 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 CE))
    (pad 6 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad6)"))
    (pad 5 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad5)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad8)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad7)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_JST:JST_XH_S06B-XH-A_06x2.50mm_Angled (layer F.Cu) (tedit 5844627E)
    (at 151.13 71.12 180)
    (descr "JST XH series connector, S06B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference P1 (at 17.78 0 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 6.25 10.3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad5)"))
    (pad 6 thru_hole circle (at 12.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 GND))
    (model Connectors_JST.3dshapes/JST_XH_S06B-XH-A_06x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_S06B-XH-A_06x2.50mm_Angled (layer F.Cu) (tedit 58446288)
    (at 173.99 71.12 180)
    (descr "JST XH series connector, S06B-XH-A, side entry type, through hole")
    (tags "connector jst xh tht side horizontal angled 2.50mm")
    (fp_text reference P2 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 6.25 10.3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 10 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad5)"))
    (pad 6 thru_hole circle (at 12.5 0 180) (size 1.75 1.75) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 GND))
    (model Connectors_JST.3dshapes/JST_XH_S06B-XH-A_06x2.50mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switches:DPST_TE_SSJ12R04 (layer F.Cu) (tedit 584474BD)
    (at 137.16 123.19 180)
    (fp_text reference SW1 (at 0 3 180) (layer F.SilkS) hide)
    (fp_text value SPST (at 0 -5.4 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -1.99898 0 180) (size 1.524 1.524) (drill 0.97028) (layers *.Cu *.Mask F.SilkS)
      (net 9 GND))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.97028) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at 1.99898 0 180) (size 1.524 1.524) (drill 0.97028) (layers *.Cu *.Mask F.SilkS))
    (model 3D/Switches/TE_SSJ12R04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Cat Trainer\nMMA8452 / i2c Sensor\nrev. 1a" (at 160.02 109.22 90) (layer F.SilkS))
  (gr_text "Cat Trainer\nMMA8452 / i2c Sensor\nrev. 1a" (at 160.02 109.22 90) (layer B.SilkS))
  (gr_line (start 184 68) (end 184 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 68) (end 184 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 101) (end 128 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 101) (end 128 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 108) (end 135 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 108) (end 135 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128 125) (end 128 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184 125) (end 128 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 177 53.65) (layer Dwgs.User))
    (feature1 (pts (xy 170 76) (xy 170 52.3)))
    (feature2 (pts (xy 184 76) (xy 184 52.3)))
    (crossbar (pts (xy 184 55) (xy 170 55)))
    (arrow1a (pts (xy 170 55) (xy 171.126504 54.413579)))
    (arrow1b (pts (xy 170 55) (xy 171.126504 55.586421)))
    (arrow2a (pts (xy 184 55) (xy 182.873496 54.413579)))
    (arrow2b (pts (xy 184 55) (xy 182.873496 55.586421)))
  )
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 135 53.65) (layer Dwgs.User))
    (feature1 (pts (xy 128 76) (xy 128 52.3)))
    (feature2 (pts (xy 142 76) (xy 142 52.3)))
    (crossbar (pts (xy 142 55) (xy 128 55)))
    (arrow1a (pts (xy 128 55) (xy 129.126504 54.413579)))
    (arrow1b (pts (xy 128 55) (xy 129.126504 55.586421)))
    (arrow2a (pts (xy 142 55) (xy 140.873496 54.413579)))
    (arrow2b (pts (xy 142 55) (xy 140.873496 55.586421)))
  )
  (gr_line (start 177 101) (end 184 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 108) (end 177 101) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184 108) (end 177 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184 125) (end 184 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 197.35 104.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 184 101) (xy 198.7 101)))
    (feature2 (pts (xy 184 108) (xy 198.7 108)))
    (crossbar (pts (xy 196 108) (xy 196 101)))
    (arrow1a (pts (xy 196 101) (xy 196.586421 102.126504)))
    (arrow1b (pts (xy 196 101) (xy 195.413579 102.126504)))
    (arrow2a (pts (xy 196 108) (xy 196.586421 106.873496)))
    (arrow2b (pts (xy 196 108) (xy 195.413579 106.873496)))
  )
  (dimension 17 (width 0.3) (layer Dwgs.User)
    (gr_text "17.000 mm" (at 197.35 116.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 184 108) (xy 198.7 108)))
    (feature2 (pts (xy 184 125) (xy 198.7 125)))
    (crossbar (pts (xy 196 125) (xy 196 108)))
    (arrow1a (pts (xy 196 108) (xy 196.586421 109.126504)))
    (arrow1b (pts (xy 196 108) (xy 195.413579 109.126504)))
    (arrow2a (pts (xy 196 125) (xy 196.586421 123.873496)))
    (arrow2b (pts (xy 196 125) (xy 195.413579 123.873496)))
  )
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 131.5 66.65) (layer Dwgs.User))
    (feature1 (pts (xy 135 76) (xy 135 65.3)))
    (feature2 (pts (xy 128 76) (xy 128 65.3)))
    (crossbar (pts (xy 128 68) (xy 135 68)))
    (arrow1a (pts (xy 135 68) (xy 133.873496 68.586421)))
    (arrow1b (pts (xy 135 68) (xy 133.873496 67.413579)))
    (arrow2a (pts (xy 128 68) (xy 129.126504 68.586421)))
    (arrow2b (pts (xy 128 68) (xy 129.126504 67.413579)))
  )
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 180.5 66.65) (layer Dwgs.User))
    (feature1 (pts (xy 177 76) (xy 177 65.3)))
    (feature2 (pts (xy 184 76) (xy 184 65.3)))
    (crossbar (pts (xy 184 68) (xy 177 68)))
    (arrow1a (pts (xy 177 68) (xy 178.126504 67.413579)))
    (arrow1b (pts (xy 177 68) (xy 178.126504 68.586421)))
    (arrow2a (pts (xy 184 68) (xy 182.873496 67.413579)))
    (arrow2b (pts (xy 184 68) (xy 182.873496 68.586421)))
  )
  (dimension 56 (width 0.3) (layer Dwgs.User)
    (gr_text "56.000 mm" (at 156 57.65) (layer Dwgs.User))
    (feature1 (pts (xy 128 76) (xy 128 56.3)))
    (feature2 (pts (xy 184 76) (xy 184 56.3)))
    (crossbar (pts (xy 184 59) (xy 128 59)))
    (arrow1a (pts (xy 128 59) (xy 129.126504 58.413579)))
    (arrow1b (pts (xy 128 59) (xy 129.126504 59.586421)))
    (arrow2a (pts (xy 184 59) (xy 182.873496 58.413579)))
    (arrow2b (pts (xy 184 59) (xy 182.873496 59.586421)))
  )
  (dimension 57 (width 0.3) (layer Dwgs.User)
    (gr_text "57.000 mm" (at 206.35 96.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 184 125) (xy 207.7 125)))
    (feature2 (pts (xy 184 68) (xy 207.7 68)))
    (crossbar (pts (xy 205 68) (xy 205 125)))
    (arrow1a (pts (xy 205 125) (xy 204.413579 123.873496)))
    (arrow1b (pts (xy 205 125) (xy 205.586421 123.873496)))
    (arrow2a (pts (xy 205 68) (xy 204.413579 69.126504)))
    (arrow2b (pts (xy 205 68) (xy 205.586421 69.126504)))
  )
  (dimension 7 (width 0.3) (layer Dwgs.User)
    (gr_text "7.000 mm" (at 197.35 88.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 184 92) (xy 198.7 92)))
    (feature2 (pts (xy 184 85) (xy 198.7 85)))
    (crossbar (pts (xy 196 85) (xy 196 92)))
    (arrow1a (pts (xy 196 92) (xy 195.413579 90.873496)))
    (arrow1b (pts (xy 196 92) (xy 196.586421 90.873496)))
    (arrow2a (pts (xy 196 85) (xy 195.413579 86.126504)))
    (arrow2b (pts (xy 196 85) (xy 196.586421 86.126504)))
  )
  (dimension 17 (width 0.3) (layer Dwgs.User)
    (gr_text "17.000 mm" (at 197.35 76.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 184 85) (xy 198.7 85)))
    (feature2 (pts (xy 184 68) (xy 198.7 68)))
    (crossbar (pts (xy 196 68) (xy 196 85)))
    (arrow1a (pts (xy 196 85) (xy 195.413579 83.873496)))
    (arrow1b (pts (xy 196 85) (xy 196.586421 83.873496)))
    (arrow2a (pts (xy 196 68) (xy 195.413579 69.126504)))
    (arrow2b (pts (xy 196 68) (xy 196.586421 69.126504)))
  )
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "14.000 mm" (at 117.65 75 90) (layer Dwgs.User))
    (feature1 (pts (xy 132 68) (xy 116.3 68)))
    (feature2 (pts (xy 132 82) (xy 116.3 82)))
    (crossbar (pts (xy 119 82) (xy 119 68)))
    (arrow1a (pts (xy 119 68) (xy 119.586421 69.126504)))
    (arrow1b (pts (xy 119 68) (xy 118.413579 69.126504)))
    (arrow2a (pts (xy 119 82) (xy 119.586421 80.873496)))
    (arrow2b (pts (xy 119 82) (xy 118.413579 80.873496)))
  )
  (dimension 28 (width 0.3) (layer Dwgs.User)
    (gr_text "28.000 mm" (at 117.65 96 270) (layer Dwgs.User))
    (feature1 (pts (xy 132 110) (xy 116.3 110)))
    (feature2 (pts (xy 132 82) (xy 116.3 82)))
    (crossbar (pts (xy 119 82) (xy 119 110)))
    (arrow1a (pts (xy 119 110) (xy 118.413579 108.873496)))
    (arrow1b (pts (xy 119 110) (xy 119.586421 108.873496)))
    (arrow2a (pts (xy 119 82) (xy 118.413579 83.126504)))
    (arrow2b (pts (xy 119 82) (xy 119.586421 83.126504)))
  )
  (dimension 28 (width 0.3) (layer Dwgs.User)
    (gr_text "28.000 mm" (at 156 66.65) (layer Dwgs.User))
    (feature1 (pts (xy 170 76) (xy 170 65.3)))
    (feature2 (pts (xy 142 76) (xy 142 65.3)))
    (crossbar (pts (xy 142 68) (xy 170 68)))
    (arrow1a (pts (xy 170 68) (xy 168.873496 68.586421)))
    (arrow1b (pts (xy 170 68) (xy 168.873496 67.413579)))
    (arrow2a (pts (xy 142 68) (xy 143.126504 68.586421)))
    (arrow2b (pts (xy 142 68) (xy 143.126504 67.413579)))
  )
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 186.69 128.27) (xy 125.73 128.27) (xy 125.73 66.04) (xy 186.69 66.04)
      )
    )
  )
)
