(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 44)
    (zones 0)
    (modules 33)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module alexglow-footprints:hlogoTiny (layer F.Cu) (tedit 600E2129)
    (at 151.003 86.6775)
    (fp_text reference " " (at 0 0) (layer F.SilkS) hide)
    (fp_text value " " (at 0.75 0) (layer F.SilkS) hide)
  )
  (module cbot-breadboard:herz-whole-mask-neg-520 (layer B.Cu) (tedit 0)
    (at 143.51 68.707 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module cbot-breadboard:coretext-520 (layer B.Cu) (tedit 0)
    (at 151.47036 94.10192 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module cbot-breadboard:bow-smol-neg-385 (layer B.Cu) (tedit 0)
    (at 151.19096 71.5772 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 152.4 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 149.86 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 128.27 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 130.81 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 176.53 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 173.99 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 171.45 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (gr_text "Companion Bot core: designed for use with\nTeensy and Arduino Nano 33 BLE Sense.\n\nPlace a little sticky breadboard in this\nbox, with male headers along the sides.\n\nUse short wires to connect the breadboard\nGPIO pins to the nearest header pins.\n\nSolder a cut USB cable to 5V and ground." (at 151.1935 61.214) (layer F.SilkS))
  (gr_text "“MITTLER ZWISCHEN HIRN UND HANDEN MUSS DAS HERZ SEIN”" (at 152.4 99.695) (layer B.SilkS))
  (gr_text "v1\nalex glow\n@glowascii" (at 151.13 84.963) (layer B.SilkS))
  (gr_text "<-----                                  \nNeed to use one of those pins with power?\nUse the pads on the back to bridge over\nto one of the GPIO lines over here. --->" (at 151.13 74.295) (layer F.SilkS))
  (gr_text "5 volts" (at 173.99 83.185 90) (layer F.SilkS))
  (gr_text gpio (at 171.45 83.185 90) (layer F.SilkS))
  (gr_text ground (at 176.53 83.185 90) (layer F.SilkS))
  (gr_line (start 176.53 101.6) (end 128.27 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.8 100.33) (end 176.53 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.27 101.6) (end 127 100.33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 52.07) (end 127 100.33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.53 50.8) (end 177.8 52.07) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.53 50.8) (end 128.27 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 52.07) (end 128.27 50.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.8 52.07) (end 177.8 100.33) (layer Edge.Cuts) (width 0.05))
)
