(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "GND")
	(net 3 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad4)")
	(net 4 "Net-(LED1-ANODEGREENEMITTER)")
	(net 5 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad2)")
	(net 6 "Net-(LED2-ANODEGREENEMITTER)")
	(net 7 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad2)")
	(net 8 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad4)")
	(net 9 "Net-(R4-Pad2)")
	(net 10 "Net-(R2-Pad2)")
	(net 11 "unconnected-(U1-Pad2)")
	(net 12 "unconnected-(U2-Pad2)")
	(net 13 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad4)")
	(net 14 "Net-(LED3-ANODEGREENEMITTER)")
	(net 15 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad2)")
	(net 16 "Net-(R6-Pad2)")
	(net 17 "unconnected-(U3-Pad2)")
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 238.033686 95.33019 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R10"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(LED3-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 254.5 95.5 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R11"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 189.5 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R1"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(LED1-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 230 108 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R7"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 234 108 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R9"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(LED2-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 214 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R4"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 -3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(R4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 194 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R3"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -3.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 179.5 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R2"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 230 108 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R7"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 250.5 95.5 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R12"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CHIP_1GF1A_SVI"
		(layer "F.Cu")
		(at 224.5 109 -90)
		(tags "CUD1GF1A ")
		(property "Reference" "U3"
			(at -2.899192 1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CUD1GF1A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "CUD1GF1A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CHIP_1GF1A_SVI")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.375 0 270)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(R4-Pad2)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1.2954 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(U3-Pad2)")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 1.375 0 270)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 226.2018 108.3015) (xy 226.2018 107.904399) (xy 222.7982 107.904399) (xy 222.7982 108.3015)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 226.2018 110.095601) (xy 226.2018 109.6985) (xy 222.7982 109.6985) (xy 222.7982 110.095601)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 217.993255 108.360418 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R8"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 189.5 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R1"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(LED1-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 214 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R4"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 -3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(R4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CHIP_1GF1A_SVI"
		(layer "F.Cu")
		(at 204.5872 94.500126 90)
		(tags "CUD1GF1A ")
		(property "Reference" "U2"
			(at 1.500126 -3.0872 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CUD1GF1A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "CUD1GF1A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CHIP_1GF1A_SVI")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.375 0 90)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(R6-Pad2)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0 0 90)
			(size 1.2954 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(U2-Pad2)")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 1.375 0 90)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 202.8854 93.404525) (xy 202.8854 93.801626) (xy 206.289 93.801626) (xy 206.289 93.404525)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 202.8854 95.198626) (xy 202.8854 95.595727) (xy 206.289 95.595727) (xy 206.289 95.198626)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 194 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R3"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -3.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 217.993255 108.360418 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R8"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 179.5 95.65 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R2"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SMD8_2p4x2p4_SFH7018A_OSM"
		(layer "F.Cu")
		(at 224.5 94)
		(tags "SFH 7018A ")
		(property "Reference" "LED2"
			(at 3.5 -1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SFH 7018A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SFH 7018A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SMD8_2p4x2p4_SFH7018A_OSM")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.0872 -0.500126 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.0872 -0.500126 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.900001 -0.8536)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.204801 0)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -0.900001 0.8036)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEIREMITTER")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 1.0242 90)
			(size 1.1684 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(LED2-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.900001 0.8036)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEREDEMITTER")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.211659 0)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(LED2-ANODEGREENEMITTER)")
			(pinfunction "ANODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 0.900001 -0.8536)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 0 -0.774192 90)
			(size 1.65 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:SMD8_2p4x2p4_SFH7018A_OSM"
		(layer "F.Cu")
		(at 204.5 109 180)
		(tags "SFH 7018A ")
		(property "Reference" "LED1"
			(at 3.5 1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SFH 7018A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SFH 7018A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SMD8_2p4x2p4_SFH7018A_OSM")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.0872 -0.500126 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.0872 -0.500126 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.900001 -0.8536 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.204801 0 180)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -0.900001 0.8036 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEIREMITTER")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 1.0242 270)
			(size 1.1684 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.900001 0.8036 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEREDEMITTER")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.211659 0 180)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(LED1-ANODEGREENEMITTER)")
			(pinfunction "ANODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 0.900001 -0.8536 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 0 -0.774192 270)
			(size 1.65 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 210 95.7 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R5"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 250.5 95.5 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R12"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 198.25339 108.384639 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R6"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(R6-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CHIP_1GF1A_SVI"
		(layer "F.Cu")
		(at 184.5 109 -90)
		(tags "CUD1GF1A ")
		(property "Reference" "U1"
			(at -0.225808 -3.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CUD1GF1A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "CUD1GF1A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CHIP_1GF1A_SVI")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.375 0 270)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(R2-Pad2)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1.2954 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(U1-Pad2)")
			(pinfunction "2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" smd rect
			(at 1.375 0 270)
			(size 0.4572 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 186.2018 108.3015) (xy 186.2018 107.904399) (xy 182.7982 107.904399) (xy 182.7982 108.3015)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 186.2018 110.095601) (xy 186.2018 109.6985) (xy 182.7982 109.6985) (xy 182.7982 110.095601)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 198.25339 108.384639 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R6"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(R6-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 234 108 90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R9"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(LED2-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 254.5 95.5 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R11"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SMD8_2p4x2p4_SFH7018A_OSM"
		(layer "F.Cu")
		(at 244.5 109 180)
		(tags "SFH 7018A ")
		(property "Reference" "LED3"
			(at 2.5 2.899192 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SFH 7018A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SFH 7018A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SMD8_2p4x2p4_SFH7018A_OSM")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.0872 -0.500126 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.0872 -0.500126 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.900001 -0.8536 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.204801 0 180)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -0.900001 0.8036 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEIREMITTER")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 1.0242 270)
			(size 1.1684 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(LED3-ANODEIR{slash}REDEMMITERS-Pad4)")
			(pinfunction "ANODEIR/REDEMMITERS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.900001 0.8036 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEREDEMITTER")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.211659 0 180)
			(size 0.7874 0.508)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(LED3-ANODEGREENEMITTER)")
			(pinfunction "ANODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at 0.900001 -0.8536 180)
			(size 0.3556 0.4572)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 0 -0.774192 270)
			(size 1.65 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CATHODEGREENEMITTER")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 41.4 101.974192)
		(descr "Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole angled socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at -4.38 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at -4.38 5.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.775 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 210 95.7 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R5"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 -2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(LED1-ANODEIR{slash}REDEMMITERS-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 238.033686 95.33019 -90)
		(descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
		(property "Reference" "R10"
			(at 6.35 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 6.35 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "meterstick.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(LED3-ANODEGREENEMITTER)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 262.5 91.5)
		(mid 263.207107 91.792893)
		(end 263.5 92.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 30.5 92.5)
		(mid 30.792893 91.792893)
		(end 31.5 91.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 263.5 110.774192)
		(mid 263.207107 111.481299)
		(end 262.5 111.774192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 30.5 92.5)
		(end 30.5 110.774192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 262.5 111.774192)
		(end 31.5 111.774192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 31.5 91.5)
		(end 262.5 91.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 31.5 111.774192)
		(mid 30.792893 111.481299)
		(end 30.5 110.774192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 263.5 92.5)
		(end 263.5 110.774192)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
