(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Platform Board Attempt 1")
    (date "2023-12-28")
    (rev "0")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./fab/")
    )
  )
  (net 0 "")
  (net 1 "Net-(J39-Pin_1)")
  (net 2 "Net-(J37-Pin_1)")
  (net 3 "Net-(U3-VO)")
  (net 4 "+9V")
  (net 5 "Net-(J1-Pin_1)")
  (net 6 "Net-(J5-Pin_1)")
  (net 7 "Net-(J6-Pin_1)")
  (net 8 "Net-(J11-Pin_1)")
  (net 9 "Net-(J10-Pin_1)")
  (net 10 "Net-(J13-Pin_1)")
  (net 11 "Net-(J15-Pin_1)")
  (net 12 "Net-(J17-Pin_1)")
  (net 13 "Net-(J19-Pin_1)")
  (net 14 "Net-(J21-Pin_1)")
  (net 15 "Net-(J22-Pin_1)")
  (net 16 "Net-(J25-Pin_1)")
  (net 17 "Net-(J26-Pin_1)")
  (net 18 "Net-(J29-Pin_1)")
  (net 19 "Net-(J30-Pin_1)")
  (net 20 "Net-(J38-Pin_1)")
  (net 21 "Net-(J40-Pin_1)")
  (net 22 "Net-(R1-Pad1)")
  (net 23 "Net-(U5-D3)")
  (net 24 "Net-(R2-Pad1)")
  (net 25 "Net-(U5-D4)")
  (net 26 "Net-(R3-Pad1)")
  (net 27 "Net-(U5-D5)")
  (net 28 "Net-(R4-Pad1)")
  (net 29 "Net-(U5-D6)")
  (net 30 "Net-(R5-Pad1)")
  (net 31 "Net-(U5-D7)")
  (net 32 "Net-(R6-Pad1)")
  (net 33 "Net-(U5-D8)")
  (net 34 "Net-(R7-Pad1)")
  (net 35 "Net-(U5-D9)")
  (net 36 "Net-(U5-MISO)")
  (net 37 "Net-(R8-Pad2)")
  (net 38 "Net-(U5-MOSI)")
  (net 39 "Net-(R9-Pad2)")
  (net 40 "Net-(U5-D10)")
  (net 41 "Net-(R12-Pad1)")
  (net 42 "Net-(J4-Pin_1)")
  (net 43 "unconnected-(U5-TXO_2-PadJP7_12)")
  (net 44 "unconnected-(U5-RXI_2-PadJP7_11)")
  (net 45 "unconnected-(U5-RST_2-PadJP7_10)")
  (net 46 "unconnected-(U5-A0-PadJP6_8)")
  (net 47 "unconnected-(U5-A1-PadJP6_7)")
  (net 48 "unconnected-(U5-A2-PadJP6_6)")
  (net 49 "unconnected-(U5-A3-PadJP6_5)")
  (net 50 "unconnected-(U5-VCC_1-PadJP6_4)")
  (net 51 "unconnected-(U5-RST_1-PadJP6_3)")
  (net 52 "unconnected-(U5-RAW-PadJP6_1)")
  (net 53 "unconnected-(U5-A6-PadJP3_1)")
  (net 54 "unconnected-(U5-A7-PadJP3_2)")
  (net 55 "unconnected-(U5-A5-PadJP2_2)")
  (net 56 "unconnected-(U5-A4-PadJP2_1)")
  (net 57 "unconnected-(U5-RXI-PadJP1_3)")
  (net 58 "unconnected-(U5-TXO-PadJP1_2)")
  (net 59 "unconnected-(U5-DTR-PadJP1_1)")
  (net 60 "Earth")
  (net 61 "Net-(U4-VO)")
  (net 62 "unconnected-(U5-GND_2-PadJP7_9)")
  (net 63 "unconnected-(U5-GND_1-PadJP6_2)")
  (net 64 "Net-(U5-D2)")
  (net 65 "Net-(D2-K)")
  (net 66 "Net-(J43-Pin_1)")
  (net 67 "Net-(J35-Pin_1)")
  (net 68 "Net-(J41-Pin_1)")
  (net 69 "Net-(J45-Pin_1)")
  (net 70 "Net-(J41-Pin_2)")
  (net 71 "Net-(J45-Pin_2)")
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 28 91)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J16" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 132 131.85)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J42" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 70 "Net-(J41-Pin_2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 65.5 46.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.5 21.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 99.36 38.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(U5-D2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 159.42 23.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Positive")
    (attr through_hole)
    (fp_text reference "U4" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "+9V") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(U4-VO)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 44.58 119)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J24" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 88.44 134.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J29" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J29-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 74.56 125.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J28" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 37.5 111)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T6" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J22-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 49.5 132.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J21" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J21-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 76.5 46.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 122.5 120.945)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Positive")
    (attr through_hole)
    (fp_text reference "U2" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(J41-Pin_1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J37-Pin_1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 116.71 72)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Positive")
    (attr through_hole)
    (fp_text reference "U1" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(J45-Pin_1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J39-Pin_1)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 68.42 31.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T2" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J4-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 92.5 21.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J5-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 57.86 68.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U5-D6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 158 102)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J37" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J37-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 62.56 125.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J26" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J26-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 91.36 117.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T8" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J30-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 150.92 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U5-MISO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 38 80)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J14" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 92.42 31.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T1" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(J5-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 36.36 20.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U5-D4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 118.25 111)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "Net-(J41-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 21 23)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 56 96.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J20" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J17-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 154.5 40.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J33" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 122 42)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U3-VO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 121 23.1)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J43" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 66 "Net-(J43-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(J35-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 90.5 47.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J6-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 109.25 46)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(J43-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D2.0mm_W4.8mm_H2.5mm_FlatTop" (layer "F.Cu")
    (at 116.5 100.5)
    (descr "LED, Round, FlatTop,  Rectangular size 4.8x2.5mm^2 diameter 2.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-13GD(Ver.11B).pdf")
    (tags "LED Round FlatTop  Rectangular size 4.8x2.5mm^2 diameter 2.0mm 2 pins")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -2.31) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.31) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D2.0mm_W4.8mm_H2.5mm_FlatTop.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 99.44 134.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J32" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(J29-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 38.5 102)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U5-D7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 65.5 21.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 74.42 38.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U5-D3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 39.5 132.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J23" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(J21-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 182.8 134)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 62.56 134.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J25" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J25-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 149.75 116.5)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J37-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 75.5 21.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 28 80)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J15-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 99.44 125.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J31" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 29.92 71)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T4" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J15-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 29.92 62)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-D5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 66 96.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J17" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J17-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 132.36 96.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(U5-MOSI)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 24 40)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J10" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J10-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 150.75 31.5)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(U4-VO)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 167.25 32.25)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 2.25 -3.42) (layer "F.SilkS"))
    (fp_text value "C" (at 2.25 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.25 -0.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "+9V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 99.5 47.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J6-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 88.44 125.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J30" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(J30-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 158 76)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T9" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(R8-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J40-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 130.65 83.1)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J46" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 71 "Net-(J45-Pin_2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 36.42 29.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T3" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J10-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:MODULE_ARDUINO_PRO_MINI" (layer "F.Cu")
    (at 89.12 76.58)
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/Arduino%20Pro%20Mini/Arduino/view-part/?ref=eda")
    (property "Description" "\nThis board was developed for applications and installations where space is premium and projects are made as permanent set ups. Small, available in 3.3 V and 5 V versions, powered by ATmega328P.\n")
    (property "MANUFACTURER" "SparkFun Electronics")
    (property "MAXIMUM_PACKAGE_HEIGHT" "N/A")
    (property "MF" "Arduino")
    (property "MP" "Arduino Pro Mini")
    (property "PARTREV" "N/A")
    (property "Package" "None")
    (property "Price" "None")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/Arduino%20Pro%20Mini/Arduino/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "U5" (at -5.825 -17.635) (layer "F.SilkS"))
    (fp_text value "ARDUINO_PRO_MINI" (at 5.605 17.865) (layer "F.Fab"))
    (pad "JP1_1" thru_hole circle (at 6.35 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(U5-DTR-PadJP1_1)") (pinfunction "DTR") (pintype "input") (solder_mask_margin 0.102))
    (pad "JP1_2" thru_hole circle (at 3.81 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(U5-TXO-PadJP1_2)") (pinfunction "TXO") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP1_3" thru_hole circle (at 1.27 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(U5-RXI-PadJP1_3)") (pinfunction "RXI") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP1_4" thru_hole circle (at -1.27 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U3-VO)") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP1_5" thru_hole circle (at -3.81 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP1_6" thru_hole circle (at -6.35 -15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP2_1" thru_hole circle (at 4.699 -1.397) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(U5-A4-PadJP2_1)") (pinfunction "A4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP2_2" thru_hole circle (at 4.699 -3.937) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(U5-A5-PadJP2_2)") (pinfunction "A5") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP3_1" thru_hole circle (at 4.699 9.017) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U5-A6-PadJP3_1)") (pinfunction "A6") (pintype "input") (solder_mask_margin 0.102))
    (pad "JP3_2" thru_hole circle (at 4.699 6.477) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(U5-A7-PadJP3_2)") (pinfunction "A7") (pintype "input") (solder_mask_margin 0.102))
    (pad "JP6_1" thru_hole circle (at 7.62 -12.7) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U5-RAW-PadJP6_1)") (pinfunction "RAW") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP6_2" thru_hole circle (at 7.62 -10.16) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(U5-GND_1-PadJP6_2)") (pinfunction "GND_1") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP6_3" thru_hole circle (at 7.62 -7.62) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U5-RST_1-PadJP6_3)") (pinfunction "RST_1") (pintype "input") (solder_mask_margin 0.102))
    (pad "JP6_4" thru_hole circle (at 7.62 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U5-VCC_1-PadJP6_4)") (pinfunction "VCC_1") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP6_5" thru_hole circle (at 7.62 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U5-A3-PadJP6_5)") (pinfunction "A3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_6" thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(U5-A2-PadJP6_6)") (pinfunction "A2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_7" thru_hole circle (at 7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U5-A1-PadJP6_7)") (pinfunction "A1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_8" thru_hole circle (at 7.62 5.08) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U5-A0-PadJP6_8)") (pinfunction "A0") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_9" thru_hole circle (at 7.62 7.62) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(U4-VO)") (pinfunction "SCK") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_10" thru_hole circle (at 7.62 10.16) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(U5-MISO)") (pinfunction "MISO") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_11" thru_hole circle (at 7.62 12.7) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(U5-MOSI)") (pinfunction "MOSI") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP6_12" thru_hole circle (at 7.62 15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U5-D10)") (pinfunction "D10") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_1" thru_hole circle (at -7.62 15.24) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U5-D9)") (pinfunction "D9") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_2" thru_hole circle (at -7.62 12.7) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U5-D8)") (pinfunction "D8") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_3" thru_hole circle (at -7.62 10.16) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(U5-D7)") (pinfunction "D7") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_4" thru_hole circle (at -7.62 7.62) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(U5-D6)") (pinfunction "D6") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_5" thru_hole circle (at -7.62 5.08) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(U5-D5)") (pinfunction "D5") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_6" thru_hole circle (at -7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(U5-D4)") (pinfunction "D4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_7" thru_hole circle (at -7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(U5-D3)") (pinfunction "D3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_8" thru_hole circle (at -7.62 -2.54) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(U5-D2)") (pinfunction "D2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_9" thru_hole circle (at -7.62 -5.08) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(U5-GND_2-PadJP7_9)") (pinfunction "GND_2") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "JP7_10" thru_hole circle (at -7.62 -7.62) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U5-RST_2-PadJP7_10)") (pinfunction "RST_2") (pintype "input") (solder_mask_margin 0.102))
    (pad "JP7_11" thru_hole circle (at -7.62 -10.16) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U5-RXI_2-PadJP7_11)") (pinfunction "RXI_2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "JP7_12" thru_hole circle (at -7.62 -12.7) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U5-TXO_2-PadJP7_12)") (pinfunction "TXO_2") (pintype "bidirectional") (solder_mask_margin 0.102))
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 138.96 110.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T10" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(R9-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J38-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 38 91)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J13" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J13-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 114.5 61)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 1.2 -1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(J45-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 65.48 117.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T7" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(J26-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 114.35 83.1)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J45" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 69 "Net-(J45-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 71 "Net-(J45-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal" (layer "F.Cu")
    (at 141.25 75)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 3.75 -2.67) (layer "F.SilkS"))
    (fp_text value "C" (at 3.75 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J39-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P7.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 148 102)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J38" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(J38-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 92.36 108.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(U5-D9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 169.5 40.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J34" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "+9V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 56 85.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J19" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J19-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 120 131.85)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J41" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 68 "Net-(J41-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(J41-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 114.46 35)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Positive")
    (attr through_hole)
    (fp_text reference "U3" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(J43-Pin_1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U3-VO)") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 101.42 100.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(U5-D10)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 66 85.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J18" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at -0.24 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 74.56 134.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J27" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(J25-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (at 57.46 77.5)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Availability" "In Stock")
    (property "Check_prices" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=eda")
    (property "Description" "\nBipolar (BJT) Transistor NPN - Darlington 100 V 5 A - 2 W Through Hole TO-220\n")
    (property "MF" "onsemi")
    (property "MP" "TIP122")
    (property "Package" "TO-220-3 ON Semiconductor")
    (property "Price" "None")
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=6587647&manufacturer=onsemi&part_name=TIP122&search_term=tip122")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/TIP122/Onsemi/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "T5" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "TIP122" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(J19-Pin_1)") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 24 51)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 34.58 119)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J22" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(J22-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical" (layer "F.Cu")
    (at 66.42 108.5)
    (descr "Resistor, Axial_DIN0309 series, Axial, Vertical, pin pitch=5.08mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Vertical pin pitch 5.08mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 2.54 -2.72) (layer "F.SilkS"))
    (fp_text value "R_US" (at 2.54 2.72) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.72) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(U5-D8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 34 40)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J12" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 143 56)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J40" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(J40-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 182.8 23)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 21 134)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 135 56)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J39" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J39-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal" (layer "F.Cu")
    (at 135 22.85)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J35" (at 1 -2.55) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Socket" (at 1 7.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 2.5) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.2083333333)
      (net 67 "Net-(J35-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 60 "Earth") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 34 51)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (property "Sheetfile" "PlatformBoard.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J11" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Pin" (at 0 2.77) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J11-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 13 15) (end 190.8 142)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Alpert Kazemba\nLibben McKown\nWilder Swanson" (at 148 55) (layer "F.SilkS"))
  (gr_text "SPEED" (at 147 50) (layer "F.SilkS"))
  (zone (net 60) (net_name "Earth") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 21 99)
        (xy 21 101)
        (xy 23 101)
        (xy 23 99)
      )
    )
  )
  (zone (net 60) (net_name "Earth") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 183 54.5)
        (xy 186 54.5)
        (xy 186 56.5)
        (xy 183 56.5)
      )
    )
  )
)
