(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 32)
    (no_connects 0)
    (area 58.809667 76.940999 240.030001 157.480001)
    (thickness 1.6)
    (drawings 10)
    (tracks 168)
    (zones 0)
    (modules 5)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.3302)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER_files/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(TD1-Pad3)")
  (net 4 "Net-(TD1-PadRST)")
  (net 5 "Net-(TD1-Pad3V3)")
  (net 6 "Net-(TD1-Pad5V)")
  (net 7 "Net-(TD1-Pad9)")
  (net 8 "Net-(TD1-Pad10)")
  (net 9 "Net-(TD1-Pad11)")
  (net 10 "Net-(TD1-Pad12)")
  (net 11 "Net-(TD1-Pad13)")
  (net 12 "Net-(TD1-PadAREF)")
  (net 13 "Net-(TD2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(TD1-Pad10)")
    (add_net "Net-(TD1-Pad11)")
    (add_net "Net-(TD1-Pad12)")
    (add_net "Net-(TD1-Pad13)")
    (add_net "Net-(TD1-Pad3)")
    (add_net "Net-(TD1-Pad3V3)")
    (add_net "Net-(TD1-Pad5V)")
    (add_net "Net-(TD1-Pad9)")
    (add_net "Net-(TD1-PadAREF)")
    (add_net "Net-(TD1-PadRST)")
    (add_net "Net-(TD2-Pad7)")
  )
  (module MJC:Arduino_UNO_R3_WithMountingHoles (layer F.Cu) (tedit 5B6F9E43)
    (at 121.92 111.76 270)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (fp_text reference TD3 (at -26.67 48.26 360) (layer F.SilkS))
    (fp_text value TDisplay (at 0 22.86 270) (layer F.Fab))
    (fp_text user %R (at 0 20.32 450) (layer F.Fab))
    (pad SCL thru_hole oval (at -9.14 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad SDA thru_hole oval (at -6.6 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 30.48 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad IORF thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 27.94 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(TD1-Pad3)"))
    (pad RST thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(TD1-PadRST)"))
    (pad 4 thru_hole oval (at 25.4 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3V3 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(TD1-Pad3V3)"))
    (pad 5 thru_hole oval (at 22.86 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5V thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(TD1-Pad5V)"))
    (pad 6 thru_hole oval (at 20.32 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 17.78 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 13.72 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad VIN thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 11.18 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(TD1-Pad9)"))
    (pad AD0 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 8.64 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(TD2-Pad7)"))
    (pad AD1 thru_hole oval (at 25.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 6.1 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(TD1-Pad11)"))
    (pad AD2 thru_hole oval (at 27.94 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 3.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(TD1-Pad12)"))
    (pad AD3 thru_hole oval (at 30.48 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 1.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(TD1-Pad13)"))
    (pad AD4 thru_hole oval (at 33.02 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at -1.52 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad AD5 thru_hole oval (at 35.56 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad AREF thru_hole oval (at -4.06 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(TD1-PadAREF)"))
    (pad 0 thru_hole oval (at 35.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 33.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -13.97 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12.7 48.26) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 33.02) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
  )
  (module MJC:2pin (layer F.Cu) (tedit 5B6F9D65)
    (at 63.5 134.62)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 1.1938 -3.048) (layer F.SilkS))
    (fp_text value MonoJack-2pin (at 1.397 2.9972) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad GND thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MJC:2pin (layer F.Cu) (tedit 5B6F9D6C)
    (at 63.5 144.78)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J2 (at 1.1938 -3.048) (layer F.SilkS))
    (fp_text value MonoJack-2pin (at 1.397 2.9972) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad GND thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MJC:Arduino_UNO_R3_WithMountingHoles (layer F.Cu) (tedit 5B6F9E35)
    (at 233.68 111.76 270)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (fp_text reference TD1 (at -26.67 48.26 360) (layer F.SilkS))
    (fp_text value TDisplay (at 0 22.86 270) (layer F.Fab))
    (fp_text user %R (at 0 20.32 450) (layer F.Fab))
    (pad SCL thru_hole oval (at -9.14 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad SDA thru_hole oval (at -6.6 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 30.48 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad IORF thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 27.94 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(TD1-Pad3)"))
    (pad RST thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(TD1-PadRST)"))
    (pad 4 thru_hole oval (at 25.4 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3V3 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(TD1-Pad3V3)"))
    (pad 5 thru_hole oval (at 22.86 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5V thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(TD1-Pad5V)"))
    (pad 6 thru_hole oval (at 20.32 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 17.78 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 13.72 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad VIN thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 11.18 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(TD1-Pad9)"))
    (pad AD0 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 8.64 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(TD1-Pad10)"))
    (pad AD1 thru_hole oval (at 25.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 6.1 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(TD1-Pad11)"))
    (pad AD2 thru_hole oval (at 27.94 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 3.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(TD1-Pad12)"))
    (pad AD3 thru_hole oval (at 30.48 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 1.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(TD1-Pad13)"))
    (pad AD4 thru_hole oval (at 33.02 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at -1.52 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad AD5 thru_hole oval (at 35.56 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad AREF thru_hole oval (at -4.06 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(TD1-PadAREF)"))
    (pad 0 thru_hole oval (at 35.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 33.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -13.97 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12.7 48.26) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 33.02) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
  )
  (module MJC:Arduino_UNO_R3_WithMountingHoles (layer F.Cu) (tedit 5B6F9E3C)
    (at 177.8 111.76 270)
    (descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino UNO R3")
    (fp_text reference TD2 (at -26.67 48.26 360) (layer F.SilkS))
    (fp_text value TDisplay (at 0 22.86 270) (layer F.Fab))
    (fp_text user %R (at 0 20.32 450) (layer F.Fab))
    (pad SCL thru_hole oval (at -9.14 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad SDA thru_hole oval (at -6.6 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad NC thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 30.48 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad IORF thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 27.94 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(TD1-Pad3)"))
    (pad RST thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(TD1-PadRST)"))
    (pad 4 thru_hole oval (at 25.4 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3V3 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(TD1-Pad3V3)"))
    (pad 5 thru_hole oval (at 22.86 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5V thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(TD1-Pad5V)"))
    (pad 6 thru_hole oval (at 20.32 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(TD1-Pad10)"))
    (pad GND thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 17.78 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(TD2-Pad7)"))
    (pad GND thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 13.72 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad VIN thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 11.18 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(TD1-Pad9)"))
    (pad AD0 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 8.64 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad AD1 thru_hole oval (at 25.4 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 6.1 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(TD1-Pad11)"))
    (pad AD2 thru_hole oval (at 27.94 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 3.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(TD1-Pad12)"))
    (pad AD3 thru_hole oval (at 30.48 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 1.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(TD1-Pad13)"))
    (pad AD4 thru_hole oval (at 33.02 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at -1.52 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad AD5 thru_hole oval (at 35.56 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad AREF thru_hole oval (at -4.06 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(TD1-PadAREF)"))
    (pad 0 thru_hole oval (at 35.56 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 1 thru_hole oval (at 33.02 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -13.97 0) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12.7 48.26) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 33.02) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 38.1 5.08) (size 1.78 1.78) (drill 1.78) (layers *.Cu *.Mask))
  )
  (gr_line (start 60.96 81.28) (end 60.96 157.48) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.76 81.28) (end 60.96 81.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.76 157.48) (end 238.76 81.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.96 157.48) (end 238.76 157.48) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "GND\nCIV" (at 64.77 140.97 270) (layer B.SilkS))
  (gr_text "GND\nCIV" (at 64.77 130.81 270) (layer B.SilkS))
  (gr_text "Display side (sockets)\n[ FRONT ]" (at 66.04 97.79 270) (layer B.SilkS))
  (gr_text "Arduino side (pins)\n[ BACK ]" (at 66.04 97.79 270) (layer F.SilkS))
  (gr_text "Large Print Radio Display V2 by Mark (KD5RXT) - desgined and built for Anthony (KG5JPU) following Field Day 2018" (at 149.86 154.94) (layer B.SilkS))
  (gr_text "Large Print Radio Display V2 by Mark (KD5RXT) - desgined and built for Anthony (KG5JPU) following Field Day 2018" (at 149.86 154.94) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.76 157.48) (xy 60.96 157.48) (xy 60.96 81.28) (xy 238.76 81.28)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.76 157.48) (xy 60.96 157.48) (xy 60.96 81.28) (xy 238.76 81.28)
      )
    )
  )
)
