(kicad_pcb (version 20171130) (host pcbnew 5.1.4-e60b266~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 267)
    (zones 0)
    (modules 38)
    (nets 24)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 100.421 82.571)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "mix4-gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 V+)
  (net 4 V-)
  (net 5 "Net-(U$1-Pad1)")
  (net 6 "Net-(U$2-Pad1)")
  (net 7 "Net-(U$3-Pad1)")
  (net 8 "Net-(U$5-Pad1)")
  (net 9 "Net-(C1-Pad1)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(R2-Pad1)")
  (net 12 "Net-(R3-Pad1)")
  (net 13 "Net-(R4-Pad1)")
  (net 14 "Net-(C2-Pad1)")
  (net 15 "Net-(C2-Pad2)")
  (net 16 "Net-(C1-Pad2)")
  (net 17 "Net-(LOCK1-PadPOS1)")
  (net 18 "Net-(LOCK1-PadNEG1)")
  (net 19 "Net-(R13-Pad2)")
  (net 20 "Net-(R12-Pad2)")
  (net 21 "Net-(R11-Pad2)")
  (net 22 "Net-(R8-Pad2)")
  (net 23 "Net-(OUT1-PadP$1_TIP)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(LOCK1-PadNEG1)")
    (add_net "Net-(LOCK1-PadPOS1)")
    (add_net "Net-(OUT1-PadP$1_TIP)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U$1-Pad1)")
    (add_net "Net-(U$2-Pad1)")
    (add_net "Net-(U$3-Pad1)")
    (add_net "Net-(U$5-Pad1)")
    (add_net V+)
    (add_net V-)
  )
  (module Symbol:KiCad-Logo2_8mm_SilkScreen (layer Bottom) (tedit 0)
    (at 140.807 113.813 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 6.35 90) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0 -7.62 90) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_9.8x8mm_SilkScreen (layer Bottom) (tedit 0)
    (at 140.807 93.239 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0 90) (layer B.Fab) hide)
  )
  (module Package_TO_SOT_THT:TO-92 (layer Top) (tedit 5A279852)
    (at 185.814 87.8536)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference IC2 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 78Z (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 V+))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp (layer Top) (tedit 5AE50CD5)
    (at 193.131 104.923 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 1.27 -2.326371) (layer F.SilkS))
    (fp_text value D (at 1.27 3.215371) (layer F.Fab))
    (fp_text user A (at 4.34 0) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.326371) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V-))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp (layer Top) (tedit 5AE50CD5)
    (at 187.797 104.923 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 1.27 -2.326371) (layer F.SilkS))
    (fp_text value D (at 1.27 3.215371) (layer F.Fab))
    (fp_text user A (at 4.34 0) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.326371) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Bottom) (tedit 5AE50EF0)
    (at 191.861 94.001)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C8 (at 1.25 3.75) (layer B.SilkS))
    (fp_text value CP (at 1.25 -3.75) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V-))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Bottom) (tedit 5AE50EF0)
    (at 194.401 87.651 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C7 (at 1.25 3.75) (layer B.SilkS))
    (fp_text value CP (at 1.25 -3.75) (layer B.Fab))
    (fp_text user %R (at 1.25 0) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_Socket (layer Bottom) (tedit 5DA3A37E)
    (at 167.985 88.921 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference IC1 (at 3.81 -4.064) (layer B.SilkS))
    (fp_text value TL072P (at 3.81 -9.95) (layer B.Fab))
    (fp_text user %R (at 3.81 -3.81) (layer B.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V-))
    (pad 7 thru_hole oval (at 7.62 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 -5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 -7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A2EB)
    (at 163.322 108.458)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -2.1716 0.0304 90) (layer F.SilkS))
    (fp_text value 47p (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A400)
    (at 185.42 93.218)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at -2.4256 0.0304 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A2F8)
    (at 163.322 104.394)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at -2.1716 0.0304 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V-))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A384)
    (at 163.068 85.09)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C5 (at -2.1716 0.0304 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A3F7)
    (at 185.42 96.774)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5DA3A307)
    (at 163.322 119.888)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at -2.286 -0.254 90) (layer F.SilkS))
    (fp_text value 47p (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A30E)
    (at 163.322 116.078)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -2.286 0 90) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A47C)
    (at 112.789 100.554 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at -2.2556 0.0126) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R12-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A46D)
    (at 117.234 110.587 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at -2.3826 0.1396) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5AE5139B)
    (at 191.008 101.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 22R (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(LOCK1-PadNEG1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 V-))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A3EC)
    (at 185.42 101.6)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 1.016 -2.286 180) (layer F.SilkS))
    (fp_text value 22R (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(LOCK1-PadPOS1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V+))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A445)
    (at 112.789 110.587 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at -2.3826 0.0126) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A43D)
    (at 108.979 110.587 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -2.3826 0.0126) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(OUT1-PadP$1_TIP)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A315)
    (at 165.412 123.444 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 4.318 0.254 270) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A2F2)
    (at 163.322 112.268)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -2.1716 -0.2236 90) (layer F.SilkS))
    (fp_text value 100k (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A435)
    (at 104.534 110.587 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -2.3826 -0.1144) (layer F.SilkS))
    (fp_text value 100k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A477)
    (at 108.979 100.554 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -2.2556 0.0126) (layer F.SilkS))
    (fp_text value 100k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A47F)
    (at 117.234 100.554 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at -2.2556 -0.1144) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R13-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Top) (tedit 5DA3A471)
    (at 104.534 100.554 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2.2556 0.1396) (layer F.SilkS))
    (fp_text value 100k (at 1.27 2.37 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module euroslideymixer:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 175.654 90.3936 90)
    (fp_text reference U1 (at 2.5096 -4.4576 90) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(U$1-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module euroslideymixer:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 175.654 100.554 90)
    (fp_text reference U2 (at 2.7636 -4.7116 270) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(U$2-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module euroslideymixer:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 175.654 110.714 90)
    (fp_text reference U3 (at 2.5096 -4.7116 270) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(U$3-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module euroslideymixer:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 175.654 120.874 90)
    (fp_text reference U4 (at 2.7636 -4.7116 270) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(U$5-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module euroslideymixer:WQP-PJ301M-12_JACK (layer Top) (tedit 0)
    (at 111.519 120.874 90)
    (fp_text reference OUT1 (at 1.473 -4.748 270) (layer F.SilkS))
    (fp_text value THONKICONNNEW (at 0 0 90) (layer F.SilkS) hide)
    (pad P$3_SLEEVE thru_hole circle (at 0 6.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad P$2_SWITCH thru_hole circle (at 0 3.5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad P$1_TIP thru_hole circle (at 0 -5 90) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(OUT1-PadP$1_TIP)") (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (module euroslideymixer:9MM_SNAP-IN_POT (layer Top) (tedit 0)
    (at 111.519 90.3936 270)
    (descr "9mm vertical snap-in pot, Alpha / Panasonic style")
    (fp_text reference GAIN1 (at -0.7106 4.24 90) (layer F.SilkS))
    (fp_text value 1M (at -3.81 3.81 90) (layer F.Fab))
    (pad CHASSIS1 thru_hole circle (at -4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad CHASSIS2 thru_hole circle (at 4.5 0 180) (size 2.794 2.794) (drill 2.1) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -2.5 7 180) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(C1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module euroslideymixer:EURO_PWR_HEADER_LOCK (layer Bottom) (tedit 5DA3A3C2)
    (at 188.989 116.429 270)
    (descr "Eurorack Modular Synth 5 x 2 power header, fat pads and offset pins for easier soldering")
    (fp_text reference LOCK1 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value EURO_POWER_LOCK (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user RED (at -6.9546 1.5366) (layer B.SilkS))
    (fp_text user - (at -4.318231 -3.5434 180) (layer B.SilkS))
    (fp_text user + (at 5.9994 -5.0674 90) (layer B.SilkS))
    (fp_text user GND (at 2.9514 -3.2894 180) (layer B.SilkS))
    (fp_text user GND (at 0.389575 -3.2894 180) (layer B.SilkS))
    (fp_text user GND (at -2.1286 -3.2894 180) (layer B.SilkS))
    (fp_text user POWER (at 7.7774 2.2986) (layer B.SilkS))
    (pad POS1 thru_hole circle (at 5.08 1.397 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(LOCK1-PadPOS1)") (solder_mask_margin 0.1016))
    (pad GND5 thru_hole circle (at 2.54 1.143 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad GND3 thru_hole circle (at 0 1.397 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad GND1 thru_hole circle (at -2.54 1.143 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad NEG1 thru_hole circle (at -5.08 1.397 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(LOCK1-PadNEG1)") (solder_mask_margin 0.1016))
    (pad POS2 thru_hole circle (at 5.08 -1.143 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(LOCK1-PadPOS1)") (solder_mask_margin 0.1016))
    (pad GND6 thru_hole circle (at 2.54 -1.397 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad GND4 thru_hole circle (at 0 -1.143 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad GND2 thru_hole circle (at -2.54 -1.397 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad NEG2 thru_hole circle (at -5.08 -1.143 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(LOCK1-PadNEG1)") (solder_mask_margin 0.1016))
  )
  (module euroslideymixer:ALPHA_ILL_FADER_20MM (layer Top) (tedit 0)
    (at 141.364 90.3936 180)
    (descr "Alpha LED fader, 20mm")
    (fp_text reference U$1 (at -12.42 -2) (layer F.SilkS))
    (fp_text value 50k (at -12.92 3) (layer F.Fab))
    (pad 3 thru_hole rect (at 15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad B thru_hole rect (at 15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.1016))
    (pad E thru_hole rect (at -15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R13-Pad2)") (solder_mask_margin 0.1016))
    (pad L thru_hole rect (at -15.24 1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U$1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole rect (at -15.24 -3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module euroslideymixer:ALPHA_ILL_FADER_20MM (layer Top) (tedit 0)
    (at 141.364 100.554 180)
    (descr "Alpha LED fader, 20mm")
    (fp_text reference U$2 (at -12.42 -2) (layer F.SilkS))
    (fp_text value 50k (at -12.92 3) (layer F.Fab))
    (pad 3 thru_hole rect (at 15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad B thru_hole rect (at 15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.1016))
    (pad E thru_hole rect (at -15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R12-Pad2)") (solder_mask_margin 0.1016))
    (pad L thru_hole rect (at -15.24 1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(U$2-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole rect (at -15.24 -3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module euroslideymixer:ALPHA_ILL_FADER_20MM (layer Top) (tedit 0)
    (at 141.364 110.714 180)
    (descr "Alpha LED fader, 20mm")
    (fp_text reference U$3 (at -12.42 -2) (layer F.SilkS))
    (fp_text value 50k (at -12.92 3) (layer F.Fab))
    (pad 3 thru_hole rect (at 15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad B thru_hole rect (at 15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.1016))
    (pad E thru_hole rect (at -15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R11-Pad2)") (solder_mask_margin 0.1016))
    (pad L thru_hole rect (at -15.24 1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U$3-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole rect (at -15.24 -3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad1)") (solder_mask_margin 0.1016))
  )
  (module euroslideymixer:ALPHA_ILL_FADER_20MM (layer Top) (tedit 0)
    (at 141.364 120.874 180)
    (descr "Alpha LED fader, 20mm")
    (fp_text reference U$5 (at -12.42 -2) (layer F.SilkS))
    (fp_text value 50k (at -12.92 3) (layer F.Fab))
    (pad 3 thru_hole rect (at 15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad B thru_hole rect (at 15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.1016))
    (pad E thru_hole rect (at -15.24 3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R8-Pad2)") (solder_mask_margin 0.1016))
    (pad L thru_hole rect (at -15.24 1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole rect (at -15.24 -1.27 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U$5-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole rect (at -15.24 -3.81 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(R4-Pad1)") (solder_mask_margin 0.1016))
  )
  (gr_text "York Modular::MIX4" (at 148.844 106.172 270) (layer B.SilkS))
  (gr_line (start 196.2786 125.9536) (end 196.2786 84.0536) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 195.0086 84.0536) (end 196.2786 84.0536) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195.0086 82.7836) (end 101.9936 82.7836) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.9936 84.0536) (end 101.9936 82.7836) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100.7236 84.0536) (end 100.7236 125.9536) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.9936 125.9536) (end 100.7236 125.9536) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.9936 127.2236) (end 195.0086 127.2236) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 195.0086 125.9536) (end 195.0086 127.2236) (angle -90) (layer Edge.Cuts) (width 0.05))
)
