(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(A1-Pin_1)")
  (net 3 "Net-(Dy8-Pin_1)")
  (net 4 "Net-(Dy9-Pin_1)")
  (net 5 "Net-(Dy10-Pin_1)")
  (net 6 "Net-(Dy11-Pin_1)")
  (net 7 "Net-(Dy12-Pin_1)")
  (net 8 "Net-(Dy1-Pin_1)")
  (net 9 "Net-(Dy2-Pin_1)")
  (net 10 "Net-(Dy3-Pin_1)")
  (net 11 "Net-(Dy4-Pin_1)")
  (net 12 "Net-(Dy5-Pin_1)")
  (net 13 "Net-(Dy6-Pin_1)")
  (net 14 "Net-(Dy7-Pin_1)")
  (net 15 "Net-(HVIN1-Pin_1)")
  (net 16 "unconnected-(IC1-Pin_1-Pad1)")
  (net 17 "unconnected-(IC2-Pin_1-Pad1)")
  (net 18 "unconnected-(IC3-Pin_1-Pad1)")
  (net 19 "unconnected-(IC4-Pin_1-Pad1)")
  (net 20 "unconnected-(IC5-Pin_1-Pad1)")
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 114.741 95.21)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "K1" (at 1.049 -2.22 unlocked) (layer "F.SilkS"))
    (fp_text value "K" (at -1.621 2.5 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(HVIN1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 102.13 89.31 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "1.5R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "Net-(Dy1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 9 "Net-(Dy2-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 127.28 115.75)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 84.5 100)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "IC3" (at -4.14 -0.03 unlocked) (layer "F.SilkS"))
    (fp_text value "IC" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(IC3-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 100 115.5)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy11" (at 0.07 2.44 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy11" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Dy11-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 87.46 90.889)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy8" (at -2.81 -2.409 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy8" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(Dy8-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 115.5 100)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy1" (at 3.56 -0.03 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy1" (at 3.5 -0.09 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Dy1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 119.3 90.63)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "HVGND1" (at -0.03 -2.9 unlocked) (layer "F.SilkS"))
    (fp_text value "HV GND" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 100.22 111.96)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 3.4 0.09) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "Net-(Dy10-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 6 "Net-(Dy11-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 104.79 114.741)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy9" (at 1.73 2.159 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy9" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Dy9-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 104.79 85.259)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Gate1" (at 1.51 -2.779 unlocked) (layer "F.SilkS"))
    (fp_text value "G" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Dy1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 85.259 95.21)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy10" (at -3.999 -1.22 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy10" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Dy10-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 92.61 90.07 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -1.02 1.69) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 12 "Net-(Dy5-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(Dy6-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 100.21 109.85)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 3.18 0.08) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "Net-(Dy10-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 6 "Net-(Dy11-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 72.72 115.75)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 111.45 96.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "4R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 15 "Net-(HVIN1-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "Net-(Dy1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 90.65 101.05 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at -3.15 0.06) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "Net-(Dy8-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Net-(Dy9-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 99.69 92.09 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -0.49 -1.89) (layer "F.SilkS"))
    (fp_text value "2R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 9 "Net-(Dy2-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "Net-(Dy3-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 100 68.5)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 112.54 90.889)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "IC5" (at 3.07 -1.319 unlocked) (layer "F.SilkS"))
    (fp_text value "IC" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(IC5-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 95.21 114.741)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "A1" (at -1.22 1.899 unlocked) (layer "F.SilkS"))
    (fp_text value "A" (at -23.9914 9.2468 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(A1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 94.87 111.86 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 3.13 -0.17) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 6 "Net-(Dy11-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 7 "Net-(Dy12-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 94.83 109.73 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 3.5 0.08) (layer "F.SilkS"))
    (fp_text value "1.5R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 6 "Net-(Dy11-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "Net-(Dy12-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 109.111 112.54)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy7" (at 2.469 3.11 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy7" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Dy7-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 89.86 93.59 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0.35 -1.68) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "Net-(Dy7-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(Dy8-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 100 84.5)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy2" (at 0 -2.75 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy2" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Dy2-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 95.72 92.71 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 11 "Net-(Dy4-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 12 "Net-(Dy5-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 91.56 104.06 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -3.71 0.02) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 4 "Net-(Dy9-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "Net-(Dy10-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_8.4mm_M8" (layer "F.Cu")
    (at 100 100)
    (descr "Mounting Hole 8.4mm, no annular, M8")
    (tags "mounting hole 8.4mm no annular m8")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -9.4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 9.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 8.4 8.4) (drill 8.4) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 93.26 96.21 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.83 -0.76) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(Dy6-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "Net-(Dy7-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 91.56 106.06 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at -2.87 -0.13) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "Net-(Dy9-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "Net-(Dy10-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 87.46 109.111)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "IC1" (at -2.39 3.009 unlocked) (layer "F.SilkS"))
    (fp_text value "IC" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(IC1-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 112.54 109.111)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy5" (at 3.21 1.629 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy5" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Dy5-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 90.889 87.46)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy6" (at -2.429 -2.55 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy6" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Dy6-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 107.38 119.66)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "SGND1" (at 3.99 -0.39 unlocked) (layer "F.SilkS"))
    (fp_text value "SIG GND" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 85.259 104.79)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "IC2" (at -2.789 2.19 unlocked) (layer "F.SilkS"))
    (fp_text value "IC" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(IC2-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 95.21 85.259)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy4" (at -1.1 -2.729 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy4" (at 0.01 2.521 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Dy4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 90.72 98.75 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -3.02 -0.12) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(Dy8-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 4 "Net-(Dy9-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (at 90.25 119.47 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at -0.09 1.69 90) (layer "F.SilkS"))
    (fp_text value "C" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 7 "Net-(Dy12-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 109.111 87.46)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "IC4" (at 3.539 -1.52 unlocked) (layer "F.SilkS"))
    (fp_text value "IC" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(IC4-Pin_1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 92.75 119.49 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 1.0575 -1.93 90) (layer "F.SilkS"))
    (fp_text value "1.5R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "Net-(Dy12-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 98.26 121.68 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "RL1" (at 0.12 1.96 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "Net-(A1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 120.28 94.84)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "HVIN1" (at 0.46 2.47 unlocked) (layer "F.SilkS"))
    (fp_text value "HV IN" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(HVIN1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 97.45 88.62 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -0.29 1.83) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "Net-(Dy3-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 11 "Net-(Dy4-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 114.741 104.79)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy3" (at 3.949 0.68 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy3" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Dy3-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 90.889 112.54)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "Dy12" (at -1.679 3.58 unlocked) (layer "F.SilkS"))
    (fp_text value "Dy12" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Dy12-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Custom parts:PMT pin" (layer "F.Cu")
    (at 102.6 120.36)
    (property "Sheetfile" "R11410 base v1.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "SOUT1" (at 2.08 2.05 unlocked) (layer "F.SilkS"))
    (fp_text value "Out" (at -0.08 7.52 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.57) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(A1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (gr_circle (center 100.04 99.99) (end 104.04 99.99)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 126.331216 111.705139) (mid 125.238586 110.413053) (end 125.21919 108.721029)
    (layer "Edge.Cuts"))
  (gr_line (start 97.04 68.49) (end 97.04 71.36357)
    (layer "Edge.Cuts"))
  (gr_arc (start 70.345136 116.556987) (mid 70.095385 114.659939) (end 71.2602 113.141924)
    (layer "Edge.Cuts"))
  (gr_arc (start 105.068302 73.818667) (mid 123.119577 86.665) (end 125.21919 108.721029)
    (layer "Edge.Cuts"))
  (gr_arc (start 105.068302 73.818667) (mid 103.612664 72.955857) (end 103.04 71.36357)
    (layer "Edge.Cuts"))
  (gr_circle (center 127.3198 115.74) (end 128.8198 115.74)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 97.04 71.36357) (mid 96.467336 72.955857) (end 95.011698 73.818667)
    (layer "Edge.Cuts"))
  (gr_line (start 100.54 65.99) (end 99.54 65.99)
    (layer "Edge.Cuts"))
  (gr_line (start 73.748784 111.705139) (end 71.2602 113.141924)
    (layer "Edge.Cuts"))
  (gr_arc (start 100.54 65.99) (mid 102.307767 66.722233) (end 103.04 68.49)
    (layer "Edge.Cuts"))
  (gr_arc (start 120.190888 117.430304) (mid 100.04 126.64) (end 79.889112 117.430304)
    (layer "Edge.Cuts"))
  (gr_arc (start 76.748784 116.901291) (mid 78.414078 116.60109) (end 79.889112 117.430304)
    (layer "Edge.Cuts"))
  (gr_line (start 74.2602 118.338076) (end 76.748784 116.901291)
    (layer "Edge.Cuts"))
  (gr_line (start 128.8198 113.141924) (end 126.331216 111.705139)
    (layer "Edge.Cuts"))
  (gr_arc (start 120.190888 117.430304) (mid 121.665921 116.601114) (end 123.331216 116.901291)
    (layer "Edge.Cuts"))
  (gr_line (start 129.234864 117.423013) (end 129.734864 116.556987)
    (layer "Edge.Cuts"))
  (gr_arc (start 74.2602 118.338076) (mid 72.363152 118.587827) (end 70.845136 117.423013)
    (layer "Edge.Cuts"))
  (gr_line (start 123.331216 116.901291) (end 125.8198 118.338076)
    (layer "Edge.Cuts"))
  (gr_arc (start 74.86081 108.721029) (mid 76.960423 86.665) (end 95.011698 73.818667)
    (layer "Edge.Cuts"))
  (gr_arc (start 128.8198 113.141924) (mid 129.984616 114.65994) (end 129.734864 116.556987)
    (layer "Edge.Cuts"))
  (gr_circle (center 72.7602 115.74) (end 74.2602 115.74)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 103.04 71.36357) (end 103.04 68.49)
    (layer "Edge.Cuts"))
  (gr_arc (start 74.86081 108.721029) (mid 74.841413 110.413054) (end 73.748784 111.705139)
    (layer "Edge.Cuts"))
  (gr_circle (center 100.04 68.49) (end 101.54 68.49)
    (fill none) (layer "Edge.Cuts"))
  (gr_arc (start 97.04 68.49) (mid 97.772233 66.722233) (end 99.54 65.99)
    (layer "Edge.Cuts"))
  (gr_line (start 70.345136 116.556987) (end 70.845136 117.423013)
    (layer "Edge.Cuts"))
  (gr_arc (start 129.234864 117.423013) (mid 127.716847 118.587822) (end 125.8198 118.338076)
    (layer "Edge.Cuts"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125 100)
        (xy 124.980235 99.006087)
        (xy 124.920971 98.013746)
        (xy 124.822302 97.024545)
        (xy 124.684384 96.040049)
        (xy 124.507434 95.061815)
        (xy 124.291734 94.091389)
        (xy 124.037623 93.130306)
        (xy 123.745503 92.180085)
        (xy 123.415837 91.242229)
        (xy 123.049146 90.318221)
        (xy 122.64601 89.409521)
        (xy 122.207065 88.517568)
        (xy 121.733007 87.64377)
        (xy 121.224584 86.789511)
        (xy 120.682601 85.956139)
        (xy 120.107914 85.144974)
        (xy 119.501433 84.357298)
        (xy 118.864116 83.594356)
        (xy 118.19697 82.857355)
        (xy 117.501052 82.14746)
        (xy 116.777461 81.465793)
        (xy 116.027341 80.813433)
        (xy 115.251879 80.191411)
        (xy 114.4523 79.60071)
        (xy 113.629869 79.042265)
        (xy 112.785887 78.516958)
        (xy 111.921688 78.02562)
        (xy 111.038637 77.569028)
        (xy 110.138133 77.147905)
        (xy 109.221598 76.762915)
        (xy 108.290482 76.414668)
        (xy 107.346257 76.103713)
        (xy 106.390416 75.830544)
        (xy 105.42447 75.595592)
        (xy 104.449947 75.399228)
        (xy 103.468388 75.241763)
        (xy 102.481345 75.123446)
        (xy 101.490378 75.044464)
        (xy 100.497055 75.004942)
        (xy 99.502945 75.004942)
        (xy 98.509622 75.044464)
        (xy 97.518655 75.123446)
        (xy 96.531612 75.241763)
        (xy 95.550053 75.399228)
        (xy 94.57553 75.595592)
        (xy 93.609584 75.830544)
        (xy 92.653743 76.103713)
        (xy 91.709518 76.414668)
        (xy 90.778402 76.762915)
        (xy 89.861867 77.147905)
        (xy 88.961363 77.569028)
        (xy 88.078312 78.02562)
        (xy 87.214113 78.516958)
        (xy 86.370131 79.042265)
        (xy 85.5477 79.60071)
        (xy 84.748121 80.191411)
        (xy 83.972659 80.813433)
        (xy 83.222539 81.465793)
        (xy 82.498948 82.14746)
        (xy 81.80303 82.857355)
        (xy 81.135884 83.594356)
        (xy 80.498567 84.357298)
        (xy 79.892086 85.144974)
        (xy 79.317399 85.956139)
        (xy 78.775416 86.789511)
        (xy 78.266993 87.64377)
        (xy 77.792935 88.517568)
        (xy 77.35399 89.409521)
        (xy 76.950854 90.318221)
        (xy 76.584163 91.242229)
        (xy 76.254497 92.180085)
        (xy 75.962377 93.130306)
        (xy 75.708266 94.091389)
        (xy 75.492566 95.061815)
        (xy 75.315616 96.040049)
        (xy 75.177698 97.024545)
        (xy 75.079029 98.013746)
        (xy 75.019765 99.006087)
        (xy 75 100)
        (xy 75.019765 100.993913)
        (xy 75.079029 101.986254)
        (xy 75.177698 102.975455)
        (xy 75.315616 103.959951)
        (xy 75.492566 104.938185)
        (xy 75.708266 105.908611)
        (xy 75.962377 106.869694)
        (xy 76.254497 107.819915)
        (xy 76.584163 108.757771)
        (xy 76.950854 109.681779)
        (xy 77.35399 110.590479)
        (xy 77.792935 111.482432)
        (xy 78.266993 112.35623)
        (xy 78.775416 113.210489)
        (xy 79.317399 114.043861)
        (xy 79.892086 114.855026)
        (xy 80.498567 115.642702)
        (xy 81.135884 116.405644)
        (xy 81.80303 117.142645)
        (xy 82.498948 117.85254)
        (xy 83.222539 118.534207)
        (xy 83.972659 119.186567)
        (xy 84.748121 119.808589)
        (xy 85.5477 120.39929)
        (xy 86.370131 120.957735)
        (xy 87.214113 121.483042)
        (xy 88.078312 121.97438)
        (xy 88.961363 122.430972)
        (xy 89.861867 122.852095)
        (xy 90.778402 123.237085)
        (xy 91.709518 123.585332)
        (xy 92.653743 123.896287)
        (xy 93.609584 124.169456)
        (xy 94.57553 124.404408)
        (xy 95.550053 124.600772)
        (xy 96.531612 124.758237)
        (xy 97.518655 124.876554)
        (xy 98.509622 124.955536)
        (xy 99.502945 124.995058)
        (xy 100.497055 124.995058)
        (xy 101.490378 124.955536)
        (xy 102.481345 124.876554)
        (xy 103.468388 124.758237)
        (xy 104.449947 124.600772)
        (xy 105.42447 124.404408)
        (xy 106.390416 124.169456)
        (xy 107.346257 123.896287)
        (xy 108.290482 123.585332)
        (xy 109.221598 123.237085)
        (xy 110.138133 122.852095)
        (xy 111.038637 122.430972)
        (xy 111.921688 121.97438)
        (xy 112.785887 121.483042)
        (xy 113.629869 120.957735)
        (xy 114.4523 120.39929)
        (xy 115.251879 119.808589)
        (xy 116.027341 119.186567)
        (xy 116.777461 118.534207)
        (xy 117.501052 117.85254)
        (xy 118.19697 117.142645)
        (xy 118.864116 116.405644)
        (xy 119.501433 115.642702)
        (xy 120.107914 114.855026)
        (xy 120.682601 114.043861)
        (xy 121.224584 113.210489)
        (xy 121.733007 112.35623)
        (xy 122.207065 111.482432)
        (xy 122.64601 110.590479)
        (xy 123.049146 109.681779)
        (xy 123.415837 108.757771)
        (xy 123.745503 107.819915)
        (xy 124.037623 106.869694)
        (xy 124.291734 105.908611)
        (xy 124.507434 104.938185)
        (xy 124.684384 103.959951)
        (xy 124.822302 102.975455)
        (xy 124.920971 101.986254)
        (xy 124.980235 100.993913)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 126.665 100)
        (xy 126.644947 98.966055)
        (xy 126.584817 97.933665)
        (xy 126.484701 96.904382)
        (xy 126.344749 95.879756)
        (xy 126.165173 94.861328)
        (xy 125.946241 93.850628)
        (xy 125.688284 92.849177)
        (xy 125.39169 91.858482)
        (xy 125.056904 90.880033)
        (xy 124.68443 89.915301)
        (xy 124.274828 88.965737)
        (xy 123.828714 88.03277)
        (xy 123.34676 87.117803)
        (xy 122.82969 86.222211)
        (xy 122.278282 85.347343)
        (xy 121.693366 84.494514)
        (xy 121.075821 83.665006)
        (xy 120.426575 82.860068)
        (xy 119.746606 82.08091)
        (xy 119.036936 81.328704)
        (xy 118.298633 80.604582)
        (xy 117.532807 79.909632)
        (xy 116.74061 79.2449)
        (xy 115.923234 78.611385)
        (xy 115.081907 78.010041)
        (xy 114.217896 77.441772)
        (xy 113.3325 76.907433)
        (xy 112.42705 76.407827)
        (xy 111.502909 75.943706)
        (xy 110.561467 75.515768)
        (xy 109.604139 75.124656)
        (xy 108.632366 74.770959)
        (xy 107.647608 74.45521)
        (xy 106.651348 74.177882)
        (xy 105.645084 73.939393)
        (xy 104.630329 73.740101)
        (xy 103.608609 73.580307)
        (xy 102.581462 73.460251)
        (xy 101.550432 73.380113)
        (xy 100.51707 73.340014)
        (xy 99.48293 73.340014)
        (xy 98.449568 73.380113)
        (xy 97.418538 73.460251)
        (xy 96.391391 73.580307)
        (xy 95.369671 73.740101)
        (xy 94.354916 73.939393)
        (xy 93.348652 74.177882)
        (xy 92.352392 74.45521)
        (xy 91.367634 74.770959)
        (xy 90.395861 75.124656)
        (xy 89.438533 75.515768)
        (xy 88.497091 75.943706)
        (xy 87.57295 76.407827)
        (xy 86.6675 76.907433)
        (xy 85.782104 77.441772)
        (xy 84.918093 78.010041)
        (xy 84.076766 78.611385)
        (xy 83.25939 79.2449)
        (xy 82.467193 79.909632)
        (xy 81.701367 80.604582)
        (xy 80.963064 81.328704)
        (xy 80.253394 82.08091)
        (xy 79.573425 82.860068)
        (xy 78.924179 83.665006)
        (xy 78.306634 84.494514)
        (xy 77.721718 85.347343)
        (xy 77.17031 86.222211)
        (xy 76.65324 87.117803)
        (xy 76.171286 88.03277)
        (xy 75.725172 88.965737)
        (xy 75.31557 89.915301)
        (xy 74.943096 90.880033)
        (xy 74.60831 91.858482)
        (xy 74.311716 92.849177)
        (xy 74.053759 93.850628)
        (xy 73.834827 94.861328)
        (xy 73.655251 95.879756)
        (xy 73.515299 96.904382)
        (xy 73.415183 97.933665)
        (xy 73.355053 98.966055)
        (xy 73.335 100)
        (xy 73.355053 101.033945)
        (xy 73.415183 102.066335)
        (xy 73.515299 103.095618)
        (xy 73.655251 104.120244)
        (xy 73.834827 105.138672)
        (xy 74.053759 106.149372)
        (xy 74.311716 107.150823)
        (xy 74.60831 108.141518)
        (xy 74.943096 109.119967)
        (xy 75.31557 110.084699)
        (xy 75.725172 111.034263)
        (xy 76.171286 111.96723)
        (xy 76.65324 112.882197)
        (xy 77.17031 113.777789)
        (xy 77.721718 114.652657)
        (xy 78.306634 115.505486)
        (xy 78.924179 116.334994)
        (xy 79.573425 117.139932)
        (xy 80.253394 117.91909)
        (xy 80.963064 118.671296)
        (xy 81.701367 119.395418)
        (xy 82.467193 120.090368)
        (xy 83.25939 120.7551)
        (xy 84.076766 121.388615)
        (xy 84.918093 121.989959)
        (xy 85.782104 122.558228)
        (xy 86.6675 123.092567)
        (xy 87.57295 123.592173)
        (xy 88.497091 124.056294)
        (xy 89.438533 124.484232)
        (xy 90.395861 124.875344)
        (xy 91.367634 125.229041)
        (xy 92.352392 125.54479)
        (xy 93.348652 125.822118)
        (xy 94.354916 126.060607)
        (xy 95.369671 126.259899)
        (xy 96.391391 126.419693)
        (xy 97.418538 126.539749)
        (xy 98.449568 126.619887)
        (xy 99.48293 126.659986)
        (xy 100.51707 126.659986)
        (xy 101.550432 126.619887)
        (xy 102.581462 126.539749)
        (xy 103.608609 126.419693)
        (xy 104.630329 126.259899)
        (xy 105.645084 126.060607)
        (xy 106.651348 125.822118)
        (xy 107.647608 125.54479)
        (xy 108.632366 125.229041)
        (xy 109.604139 124.875344)
        (xy 110.561467 124.484232)
        (xy 111.502909 124.056294)
        (xy 112.42705 123.592173)
        (xy 113.3325 123.092567)
        (xy 114.217896 122.558228)
        (xy 115.081907 121.989959)
        (xy 115.923234 121.388615)
        (xy 116.74061 120.7551)
        (xy 117.532807 120.090368)
        (xy 118.298633 119.395418)
        (xy 119.036936 118.671296)
        (xy 119.746606 117.91909)
        (xy 120.426575 117.139932)
        (xy 121.075821 116.334994)
        (xy 121.693366 115.505486)
        (xy 122.278282 114.652657)
        (xy 122.82969 113.777789)
        (xy 123.34676 112.882197)
        (xy 123.828714 111.96723)
        (xy 124.274828 111.034263)
        (xy 124.68443 110.084699)
        (xy 125.056904 109.119967)
        (xy 125.39169 108.141518)
        (xy 125.688284 107.150823)
        (xy 125.946241 106.149372)
        (xy 126.165173 105.138672)
        (xy 126.344749 104.120244)
        (xy 126.484701 103.095618)
        (xy 126.584817 102.066335)
        (xy 126.644947 101.033945)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 104 100)
        (xy 103.980739 99.607931)
        (xy 103.923141 99.219639)
        (xy 103.827761 98.838861)
        (xy 103.695518 98.469266)
        (xy 103.527685 98.114413)
        (xy 103.325878 97.777719)
        (xy 103.092042 97.462427)
        (xy 102.828427 97.171573)
        (xy 102.537573 96.907958)
        (xy 102.222281 96.674122)
        (xy 101.885587 96.472315)
        (xy 101.530734 96.304482)
        (xy 101.161139 96.172239)
        (xy 100.780361 96.076859)
        (xy 100.392069 96.019261)
        (xy 100 96)
        (xy 99.607931 96.019261)
        (xy 99.219639 96.076859)
        (xy 98.838861 96.172239)
        (xy 98.469266 96.304482)
        (xy 98.114413 96.472315)
        (xy 97.777719 96.674122)
        (xy 97.462427 96.907958)
        (xy 97.171573 97.171573)
        (xy 96.907958 97.462427)
        (xy 96.674122 97.777719)
        (xy 96.472315 98.114413)
        (xy 96.304482 98.469266)
        (xy 96.172239 98.838861)
        (xy 96.076859 99.219639)
        (xy 96.019261 99.607931)
        (xy 96 100)
        (xy 96.019261 100.392069)
        (xy 96.076859 100.780361)
        (xy 96.172239 101.161139)
        (xy 96.304482 101.530734)
        (xy 96.472315 101.885587)
        (xy 96.674122 102.222281)
        (xy 96.907958 102.537573)
        (xy 97.171573 102.828427)
        (xy 97.462427 103.092042)
        (xy 97.777719 103.325878)
        (xy 98.114413 103.527685)
        (xy 98.469266 103.695518)
        (xy 98.838861 103.827761)
        (xy 99.219639 103.923141)
        (xy 99.607931 103.980739)
        (xy 100 104)
        (xy 100.392069 103.980739)
        (xy 100.780361 103.923141)
        (xy 101.161139 103.827761)
        (xy 101.530734 103.695518)
        (xy 101.885587 103.527685)
        (xy 102.222281 103.325878)
        (xy 102.537573 103.092042)
        (xy 102.828427 102.828427)
        (xy 103.092042 102.537573)
        (xy 103.325878 102.222281)
        (xy 103.527685 101.885587)
        (xy 103.695518 101.530734)
        (xy 103.827761 101.161139)
        (xy 103.923141 100.780361)
        (xy 103.980739 100.392069)
      )
    )
  )
)
