(kicad_pcb (version 4) (host pcbnew no-vcs-found-product)
  (general
    (links 127)
    (no_connects 0)
    (area 129.464999 81.966999 162.381001 121.233001)
    (thickness 1.6)
    (drawings 9)
    (tracks 322)
    (zones 0)
    (modules 51)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.1016)
    (pad_size 0.6858 0.6858)
    (pad_drill 0.3302)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 +3.3VADC)
  (net 5 "Net-(C105-Pad2)")
  (net 6 "Net-(C107-Pad1)")
  (net 7 "Net-(C107-Pad2)")
  (net 8 "Net-(C108-Pad2)")
  (net 9 "Net-(C109-Pad2)")
  (net 10 "Net-(C115-Pad2)")
  (net 11 "Net-(J101-Pad1)")
  (net 12 "Net-(P101-Pad1)")
  (net 13 "Net-(P101-Pad2)")
  (net 14 "Net-(P101-Pad3)")
  (net 15 "Net-(P101-Pad4)")
  (net 16 "Net-(P101-Pad5)")
  (net 17 "Net-(P101-Pad6)")
  (net 18 "Net-(P101-Pad7)")
  (net 19 "Net-(P101-Pad8)")
  (net 20 "Net-(P102-Pad1)")
  (net 21 "Net-(P102-Pad2)")
  (net 22 "Net-(P102-Pad3)")
  (net 23 "Net-(P102-Pad4)")
  (net 24 "Net-(P102-Pad5)")
  (net 25 "Net-(P102-Pad6)")
  (net 26 "Net-(P102-Pad7)")
  (net 27 "Net-(P102-Pad8)")
  (net 28 "Net-(R102-Pad1)")
  (net 29 "Net-(R103-Pad1)")
  (net 30 "Net-(R104-Pad2)")
  (net 31 "Net-(R106-Pad1)")
  (net 32 "Net-(R106-Pad2)")
  (net 33 "Net-(RP101-Pad1)")
  (net 34 "Net-(RP101-Pad8)")
  (net 35 "Net-(RP101-Pad2)")
  (net 36 "Net-(RP101-Pad3)")
  (net 37 "Net-(RP101-Pad4)")
  (net 38 "Net-(RP101-Pad5)")
  (net 39 "Net-(RP101-Pad6)")
  (net 40 "Net-(RP101-Pad7)")
  (net 41 "Net-(RP102-Pad1)")
  (net 42 "Net-(RP102-Pad8)")
  (net 43 "Net-(RP102-Pad2)")
  (net 44 "Net-(RP102-Pad3)")
  (net 45 "Net-(RP102-Pad4)")
  (net 46 "Net-(RP102-Pad5)")
  (net 47 "Net-(RP102-Pad6)")
  (net 48 "Net-(RP102-Pad7)")
  (net 49 "Net-(P101-Pad11)")
  (net 50 "Net-(P101-Pad12)")
  (net 51 "Net-(P102-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C107-Pad1)")
    (add_net "Net-(C107-Pad2)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C109-Pad2)")
    (add_net "Net-(C115-Pad2)")
    (add_net "Net-(P101-Pad1)")
    (add_net "Net-(P101-Pad12)")
    (add_net "Net-(P101-Pad2)")
    (add_net "Net-(P101-Pad3)")
    (add_net "Net-(P101-Pad4)")
    (add_net "Net-(P101-Pad5)")
    (add_net "Net-(P101-Pad6)")
    (add_net "Net-(P101-Pad7)")
    (add_net "Net-(P101-Pad8)")
    (add_net "Net-(P102-Pad1)")
    (add_net "Net-(P102-Pad11)")
    (add_net "Net-(P102-Pad2)")
    (add_net "Net-(P102-Pad3)")
    (add_net "Net-(P102-Pad4)")
    (add_net "Net-(P102-Pad5)")
    (add_net "Net-(P102-Pad6)")
    (add_net "Net-(P102-Pad7)")
    (add_net "Net-(P102-Pad8)")
    (add_net "Net-(R102-Pad1)")
    (add_net "Net-(R103-Pad1)")
    (add_net "Net-(R104-Pad2)")
    (add_net "Net-(R106-Pad1)")
    (add_net "Net-(R106-Pad2)")
    (add_net "Net-(RP101-Pad1)")
    (add_net "Net-(RP101-Pad2)")
    (add_net "Net-(RP101-Pad3)")
    (add_net "Net-(RP101-Pad4)")
    (add_net "Net-(RP101-Pad5)")
    (add_net "Net-(RP101-Pad6)")
    (add_net "Net-(RP101-Pad7)")
    (add_net "Net-(RP101-Pad8)")
    (add_net "Net-(RP102-Pad1)")
    (add_net "Net-(RP102-Pad2)")
    (add_net "Net-(RP102-Pad3)")
    (add_net "Net-(RP102-Pad4)")
    (add_net "Net-(RP102-Pad5)")
    (add_net "Net-(RP102-Pad6)")
    (add_net "Net-(RP102-Pad7)")
    (add_net "Net-(RP102-Pad8)")
  )
  (net_class 50ohm ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VADC)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J101-Pad1)")
    (add_net "Net-(P101-Pad11)")
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 145.6055 116.6495)
    (fp_text reference REF**11135 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 144.3355 116.6495)
    (fp_text reference REF**11125 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 143.0655 116.6495)
    (fp_text reference REF**11115 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 145.6055 115.3795)
    (fp_text reference REF**11134 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 144.3355 115.3795)
    (fp_text reference REF**11124 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 143.0655 115.3795)
    (fp_text reference REF**11114 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 145.6055 114.1095)
    (fp_text reference REF**11133 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 144.3355 114.1095)
    (fp_text reference REF**11123 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 143.0655 114.1095)
    (fp_text reference REF**11113 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 145.6055 112.8395)
    (fp_text reference REF**11132 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 144.3355 112.8395)
    (fp_text reference REF**11122 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 143.0655 112.8395)
    (fp_text reference REF**11112 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 145.6055 111.5695)
    (fp_text reference REF**11131 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 144.3355 111.5695)
    (fp_text reference REF**11121 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5882706B)
    (at 137.7315 116.459 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at -0.1905 3.683 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5882706F)
    (at 137.795 114.173 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at -0.127 2.413 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826F4E)
    (at 140.208 101.092 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5882708A)
    (at 155.575 118.618 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at -3.048 0.127 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826FEA)
    (at 153.924 98.044 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at -2.54 -1.524 360) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C105-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5882708D)
    (at 157.2895 118.618 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C106 (at -3.556 0.0635 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826FBC)
    (at 150.368 100.076 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C107 (at 2.794 0.254 90) (layer F.SilkS))
    (fp_text value 18pf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C107-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58827001)
    (at 152.908 106.172 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C108 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C108-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58827E85)
    (at 152.908 104.14 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C109 (at -2.921 -0.0635 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C109-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58828795)
    (at 151.511 102.616)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C110 (at 3.683 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826F62)
    (at 144.272 84.074 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C111 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58827007)
    (at 150.368 105.156 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C112 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C109-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826FB1)
    (at 149.352 96.012 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C113 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5882700E)
    (at 148.59 106.934 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C114 (at -2.794 0.762 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C105-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58827018)
    (at 147.066 106.934 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C115 (at -2.794 0 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C115-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5882709A)
    (at 144.526 107.696)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C116 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1uf (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C115-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58826FA8)
    (at 147.828 96.012 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C117 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5882705F)
    (at 149.6695 118.8085 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C118 (at -0.3175 -1.3335 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58827085)
    (at 152.4635 117.7925)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference FB101 (at -0.0635 -1.2065) (layer F.SilkS))
    (fp_text value FILTER (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 58826F38)
    (at 131.318 83.82)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P101 (at 4.572 -0.254 90) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 1.27 15.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P101-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P101-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P101-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P101-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P101-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P101-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P101-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P101-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P101-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P101-Pad12)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 58826F41)
    (at 131.318 106.68)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P102 (at -0.508 -2.286) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 1.27 15.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P102-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P102-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P102-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P102-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P102-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P102-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P102-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P102-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P102-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P102-Pad11)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58826F66)
    (at 153.416 89.916)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 50 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J101-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58826FF2)
    (at 155.448 98.044 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 20 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R102-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58826FEE)
    (at 152.146 98.044 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at 2.794 -2.54 360) (layer F.SilkS))
    (fp_text value 20 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R103-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C107-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58B5F495)
    (at 143.0655 93.6625 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at -1.016 1.27 270) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R104-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58B5F491)
    (at 144.653 93.6625 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at 1.27 1.2065 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R104-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58826F9D)
    (at 146.304 95.504 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R106 (at 3.048 0.762 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R106-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R106-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-223 (layer F.Cu) (tedit 58827081)
    (at 144.4625 114.1095)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U101 (at -0.1905 -4.1275) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 4.5) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3) (zone_connect 2))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58827077)
    (at 137.287 119.38 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P103 (at 0 6.985 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P102-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module footprints:stitch_via (layer F.Cu) (tedit 58826A8E)
    (at 143.0655 111.5695)
    (fp_text reference REF**11111 (at 0 1.016) (layer F.SilkS) hide)
    (fp_text value stitch_via (at 0.0508 -0.762) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 3 +3V3) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58827128)
    (at 153.0985 112.649)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module footprints:Pulse_SMD_Balun (layer F.Cu) (tedit 58828619)
    (at 153.416 93.4085)
    (fp_text reference T101 (at -2.3495 -0.254 90) (layer F.SilkS))
    (fp_text value TRANSFO4 (at 0 -0.5) (layer F.Fab))
    (pad 5 smd rect (at -1.27 -1.5875) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.27 -1.5875) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J101-Pad1)"))
    (pad 1 smd rect (at -1.27 1.5875) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R103-Pad1)"))
    (pad 3 smd rect (at 1.27 1.5875) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R102-Pad1)"))
    (pad 2 smd rect (at 0 1.5875) (size 0.762 1.651) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C105-Pad2)"))
  )
  (module footprints:R_Array_EXB2HV (layer F.Cu) (tedit 5882A053)
    (at 140.462 105.156 180)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP101 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value 100 (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65 -1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(RP101-Pad1)"))
    (pad 16 smd rect (at 0.65 -1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P102-Pad7)"))
    (pad 8 smd rect (at -0.65 1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(RP101-Pad8)"))
    (pad 9 smd rect (at 0.65 1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P101-Pad7)"))
    (pad 2 smd rect (at -0.65 -1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(RP101-Pad2)"))
    (pad 3 smd rect (at -0.65 -0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(RP101-Pad3)"))
    (pad 4 smd rect (at -0.65 -0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(RP101-Pad4)"))
    (pad 5 smd rect (at -0.65 0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(RP101-Pad5)"))
    (pad 6 smd rect (at -0.65 0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(RP101-Pad6)"))
    (pad 7 smd rect (at -0.65 1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(RP101-Pad7)"))
    (pad 15 smd rect (at 0.65 -1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P102-Pad6)"))
    (pad 14 smd rect (at 0.65 -0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P102-Pad5)"))
    (pad 13 smd rect (at 0.65 -0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P102-Pad4)"))
    (pad 11 smd rect (at 0.65 0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P102-Pad2)"))
    (pad 12 smd rect (at 0.65 0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P102-Pad3)"))
    (pad 10 smd rect (at 0.65 1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P102-Pad1)"))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_Array_EXB2HV (layer F.Cu) (tedit 5882A05D)
    (at 140.462 97.536 180)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RP102 (at 0 2.794 180) (layer F.SilkS))
    (fp_text value 100 (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65 -1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(RP102-Pad1)"))
    (pad 16 smd rect (at 0.65 -1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P102-Pad8)"))
    (pad 8 smd rect (at -0.65 1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(RP102-Pad8)"))
    (pad 9 smd rect (at 0.65 1.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P101-Pad2)"))
    (pad 2 smd rect (at -0.65 -1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(RP102-Pad2)"))
    (pad 3 smd rect (at -0.65 -0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(RP102-Pad3)"))
    (pad 4 smd rect (at -0.65 -0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(RP102-Pad4)"))
    (pad 5 smd rect (at -0.65 0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(RP102-Pad5)"))
    (pad 6 smd rect (at -0.65 0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(RP102-Pad6)"))
    (pad 7 smd rect (at -0.65 1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(RP102-Pad7)"))
    (pad 15 smd rect (at 0.65 -1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P101-Pad8)"))
    (pad 14 smd rect (at 0.65 -0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P101-Pad5)"))
    (pad 13 smd rect (at 0.65 -0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P101-Pad6)"))
    (pad 11 smd rect (at 0.65 0.75 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P101-Pad4)"))
    (pad 12 smd rect (at 0.65 0.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P101-Pad3)"))
    (pad 10 smd rect (at 0.65 1.25 180) (size 0.5 0.33) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P101-Pad1)"))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Crystal_SMD_Abracon_ASFL1-4pin_5.0x3.2mm (layer F.Cu) (tedit 5882A2E3)
    (at 144.272 87.884 270)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3C http://www.abracon.com/Resonators/abm3c.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference U102 (at -0.0635 2.4765 270) (layer F.SilkS))
    (fp_text value ASFL1-80.000MHZ-EC-T (at 0 2.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1.27 1.1 270) (size 1.7 1.5) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.27 1.1 270) (size 1.7 1.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.27 -1.1 270) (size 1.7 1.5) (layers F.Cu F.Mask)
      (net 32 "Net-(R106-Pad2)"))
    (pad 4 smd rect (at -1.27 -1.1 270) (size 1.7 1.5) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model Crystals.3dshapes/Crystal_SMD_Abracon_ABM3C-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SMA_END (layer F.Cu) (tedit 58894D7D)
    (at 159.258 89.662)
    (fp_text reference J101 (at -3.81 -4.826) (layer F.SilkS))
    (fp_text value SMA (at 0 -0.5) (layer F.Fab))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -3.5) (size 5 4) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0) (size 5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J101-Pad1)"))
  )
  (module footprints:QFN-32-1EP_5x5mm_Pitch0.5mm_extended_pad (layer F.Cu) (tedit 588955C2)
    (at 146.05 101.346 180)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U103 (at 1.524 -3.556 180) (layer F.SilkS))
    (fp_text value ADC14C105 (at 0 3.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2.55 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at -2.55 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C109-Pad2)"))
    (pad 3 smd rect (at -2.55 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 4 smd rect (at -2.55 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -2.55 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C107-Pad1)"))
    (pad 6 smd rect (at -2.55 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C107-Pad2)"))
    (pad 7 smd rect (at -2.55 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -2.55 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 9 smd rect (at -1.75 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.25 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VADC))
    (pad 11 smd rect (at -0.75 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R106-Pad1)"))
    (pad 12 smd rect (at -0.25 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R104-Pad2)"))
    (pad 13 smd rect (at 0.25 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(RP102-Pad8)"))
    (pad 14 smd rect (at 0.75 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(RP102-Pad7)"))
    (pad 15 smd rect (at 1.25 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(RP102-Pad6)"))
    (pad 16 smd rect (at 1.75 2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(RP102-Pad5)"))
    (pad 17 smd rect (at 2.55 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(RP102-Pad4)"))
    (pad 18 smd rect (at 2.55 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(RP102-Pad3)"))
    (pad 19 smd rect (at 2.55 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(RP102-Pad2)"))
    (pad 20 smd rect (at 2.55 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 21 smd rect (at 2.55 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(RP102-Pad1)"))
    (pad 22 smd rect (at 2.55 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 2.55 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(RP101-Pad8)"))
    (pad 24 smd rect (at 2.55 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(RP101-Pad7)"))
    (pad 25 smd rect (at 1.75 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(RP101-Pad6)"))
    (pad 26 smd rect (at 1.25 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(RP101-Pad5)"))
    (pad 27 smd rect (at 0.75 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(RP101-Pad4)"))
    (pad 28 smd rect (at 0.25 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(RP101-Pad3)"))
    (pad 29 smd rect (at -0.25 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(RP101-Pad2)"))
    (pad 30 smd rect (at -0.75 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(RP101-Pad1)"))
    (pad 31 smd rect (at -1.25 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C115-Pad2)"))
    (pad 32 smd rect (at -1.75 -2.55 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C105-Pad2)"))
    (pad 33 smd rect (at 0.8625 0.8625 180) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 180) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 180) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 180) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "PMOD +5\n+5\nGND" (at 139.954 117.983 90) (layer B.SilkS))
  (gr_text "rxadc_14 v0.2\n(c) 2017\nE. Brombaugh" (at 159.0675 106.9975 90) (layer F.SilkS))
  (dimension 39.116 (width 0.3) (layer Dwgs.User)
    (gr_text "1.5400 in" (at 168.99 101.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 162.306 121.158) (xy 170.34 121.158)))
    (feature2 (pts (xy 162.306 82.042) (xy 170.34 82.042)))
    (crossbar (pts (xy 167.64 82.042) (xy 167.64 121.158)))
    (arrow1a (pts (xy 167.64 121.158) (xy 167.053579 120.031496)))
    (arrow1b (pts (xy 167.64 121.158) (xy 168.226421 120.031496)))
    (arrow2a (pts (xy 167.64 82.042) (xy 167.053579 83.168504)))
    (arrow2b (pts (xy 167.64 82.042) (xy 168.226421 83.168504)))
  )
  (dimension 32.766 (width 0.3) (layer Dwgs.User)
    (gr_text "1.2900 in" (at 145.923 75.612) (layer Dwgs.User))
    (feature1 (pts (xy 162.306 82.042) (xy 162.306 74.262)))
    (feature2 (pts (xy 129.54 82.042) (xy 129.54 74.262)))
    (crossbar (pts (xy 129.54 76.962) (xy 162.306 76.962)))
    (arrow1a (pts (xy 162.306 76.962) (xy 161.179496 77.548421)))
    (arrow1b (pts (xy 162.306 76.962) (xy 161.179496 76.375579)))
    (arrow2a (pts (xy 129.54 76.962) (xy 130.666504 77.548421)))
    (arrow2b (pts (xy 129.54 76.962) (xy 130.666504 76.375579)))
  )
  (gr_line (start 129.54 121.158) (end 129.54 82.042) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.306 121.158) (end 129.54 121.158) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.306 82.042) (end 162.306 121.158) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.54 82.042) (end 162.306 82.042) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.798 120.65) (xy 130.048 120.65) (xy 130.048 82.55) (xy 161.798 82.55) (xy 161.798 120.65)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.798 120.65) (xy 130.048 120.65) (xy 130.048 82.55) (xy 161.798 82.55) (xy 161.798 120.65)
      )
    )
  )
  (zone (net 4) (net_name +3.3VADC) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.798 120.65) (xy 146.558 120.65) (xy 146.558 82.55) (xy 161.798 82.55) (xy 161.798 120.65)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 146.05 120.65) (xy 130.048 120.65) (xy 130.048 82.55) (xy 146.05 82.55) (xy 146.05 120.65)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 148.844 117.6655) (xy 140.081 117.6655) (xy 140.081 110.49) (xy 148.844 110.49) (xy 148.844 117.6655)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 161.798 120.65) (xy 130.048 120.65) (xy 130.048 82.55) (xy 161.798 82.55) (xy 161.798 120.65)
      )
    )
  )
)
