(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 26)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 1.5)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 166.871 110.61)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Crazy_Circuits:Adafruit-Circuit-Playground-Express (layer F.Cu) (tedit 5C68996F)
    (at 102.87 54.61)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference "Circuit Playground Express" (at 32.001 32 90) (layer F.SilkS) hide)
    (fp_text value "Adafruit Circuit Playground Express" (at 30.101006 32.006807 90) (layer F.Fab) hide)
    (fp_arc (start 64.001 56) (end 67.901 56) (angle 90) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 64 8) (end 64 4.1) (angle 89.89999678) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 67.901 56) (end 67.899994 7.993193) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 0 8) (end -3.9 8) (angle 90) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 0.001 56) (end 0.001 59.9) (angle 89.89999678) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start -3.9 8) (end -3.898994 56.006807) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 64 4.1) (end 0 4.1) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 0.001 59.9) (end 64.001 59.9) (layer Edge.Cuts) (width 0.04064))
    (pad GND thru_hole circle (at 64.001 8 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A7 thru_hole circle (at 64.001 16 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A6 thru_hole circle (at 64.001 24 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 3.3V thru_hole circle (at 64.001 32 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A5 thru_hole circle (at 64.001 40 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A4 thru_hole circle (at 64.001 48 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad GND thru_hole circle (at 64.001 56 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 3.3V thru_hole circle (at 0.001 56 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A3 thru_hole circle (at 0.001 48 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A1 thru_hole circle (at 0.001 24 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A2 thru_hole circle (at 0.001 40 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad GND thru_hole circle (at 0.001 32 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad A0 thru_hole circle (at 0.001 16 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad VOUT thru_hole circle (at 0 8 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
  )
  (module AdafruitTrinketM0:CircuitPlaygroundExpress (layer F.Cu) (tedit 5C689C8B)
    (at 134.871 86.61)
    (fp_text reference " " (at 0 7) (layer F.SilkS))
    (fp_text value "Circuit Playground Express" (at 0 -8) (layer F.Fab))
    (pad 14 smd oval (at 11.303 -19.685 330) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at 17.399 -14.605 310) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at 21.336 -7.747 290) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd oval (at 22.6695 0 270) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at 21.336 7.747 250) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at 17.399 14.605 230) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at 11.303 19.685 210) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at -11.303 19.685 150) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd oval (at -17.145 14.859 130) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd oval (at -21.2725 8.001 110) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at -22.6695 0 90) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd oval (at -21.336 -7.747 70) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd oval (at -17.399 -14.5415 50) (size 5 7) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd oval (at -11.3665 -19.6215 30) (size 5 7) (layers F.Cu F.Paste F.Mask))
  )
  (gr_text "Adafruit Circuit Playground\nExpress" (at 134.871 86.61) (layer F.SilkS))
  (gr_text GND (at 162.871 62.61) (layer F.SilkS))
  (gr_text "A7\nTX" (at 162.871 70.61) (layer F.SilkS))
  (gr_text "A6\nRX" (at 162.871 78.61) (layer F.SilkS))
  (gr_text 3.3V (at 164.871 89.61) (layer F.SilkS))
  (gr_text "A5\nSDA" (at 162.871 94.61) (layer F.SilkS))
  (gr_text GND (at 162.871 110.61) (layer F.SilkS))
  (gr_text "A4\nSCL" (at 162.871 102.61) (layer F.SilkS))
  (gr_text 3.3V (at 106.871 110.61) (layer F.SilkS))
  (gr_text A3 (at 106.871 102.61) (layer F.SilkS))
  (gr_text A2 (at 106.871 94.61) (layer F.SilkS))
  (gr_text GND (at 105.871 89.61) (layer F.SilkS))
  (gr_text A1 (at 106.871 78.61) (layer F.SilkS))
  (gr_text A0 (at 106.871 70.61) (layer F.SilkS))
  (gr_text VOUT (at 106.871 62.61) (layer F.SilkS))
  (gr_text BAT (at 134.871 66.61) (layer F.SilkS))
  (gr_text USB (at 134.871 107.61) (layer F.SilkS))
)
