(kicad_pcb (version 20171130) (host pcbnew "(6.0.0-rc1-dev-465-gd3c82b0)")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 90)
    (zones 0)
    (modules 12)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu jumper hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.000152)
    (user_trace_width 0.24892)
    (user_trace_width 0.5)
    (trace_clearance 0.000152)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.000152)
    (via_size 0.000686)
    (via_drill 0.00033)
    (via_min_size 0.000686)
    (via_min_drill 0.00033)
    (user_via 0.8 0.254)
    (uvia_size 0.000686)
    (uvia_drill 0.00033)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.00129)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 DIN)
  (net 4 BIN)
  (net 5 D3)
  (net 6 D4)
  (net 7 D1)
  (net 8 D2)
  (net 9 D5)
  (net_class Default "This is the default net class."
    (clearance 0.000152)
    (trace_width 0.000152)
    (via_dia 0.000686)
    (via_drill 0.00033)
    (uvia_dia 0.000686)
    (uvia_drill 0.00033)
    (add_net BIN)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net DIN)
    (add_net GND)
    (add_net VDD)
  )
  (module LEDStrip:C_0201_0603Metric (layer F.Cu) (tedit 5B99DEC1)
    (at 84.8995 148.217)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -1.5 0) (layer F.SilkS))
    (fp_text value C (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDStrip:C_0201_0603Metric (layer F.Cu) (tedit 5B99DEC1)
    (at 77.9145 148.217)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -1.5 0) (layer F.SilkS))
    (fp_text value C (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDStrip:C_0201_0603Metric (layer F.Cu) (tedit 5B99DEC1)
    (at 70.9295 148.217)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.5 0) (layer F.SilkS))
    (fp_text value C (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDStrip:C_0201_0603Metric (layer F.Cu) (tedit 5B99DEC1)
    (at 63.881 148.217)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -1.5 0) (layer F.SilkS))
    (fp_text value C (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B99D7F3)
    (at 56.896 148.209)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.3 0) (layer F.SilkS))
    (fp_text value C (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TX1818A:TX1818A_5.0x5.0mm_Pad1.1mm (layer F.Cu) (tedit 5B97295A)
    (at 75.5 145)
    (descr http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf)
    (tags "LED RGB PLCC-6")
    (attr smd)
    (fp_text reference LED4 (at 3.81 0 90) (layer F.Fab))
    (fp_text value TX1818A (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.2 0) (layer F.SilkS))
    (pad 4 smd rect (at 2.6 1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at 2.6 0) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 2.6 -1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 D4))
    (pad 3 smd rect (at -2.6 1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 D2))
    (pad 2 smd rect (at -2.6 0) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.6 -1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 D3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Normandled_WS2813-06_5.0x5.0mm_Pitch1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TX1818A:TX1818A_5.0x5.0mm_Pad1.1mm (layer F.Cu) (tedit 5B97295A)
    (at 54.5 145.000001)
    (descr http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf)
    (tags "LED RGB PLCC-6")
    (attr smd)
    (fp_text reference LED1 (at 3.81 0 90) (layer F.Fab))
    (fp_text value TX1818A (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.2 0) (layer F.SilkS))
    (pad 4 smd rect (at 2.6 1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at 2.6 0) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 2.6 -1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 D1))
    (pad 3 smd rect (at -2.6 1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 BIN))
    (pad 2 smd rect (at -2.6 0) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.6 -1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 DIN))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Normandled_WS2813-06_5.0x5.0mm_Pitch1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TX1818A:TX1818A_5.0x5.0mm_Pad1.1mm (layer F.Cu) (tedit 5B97295A)
    (at 61.5 145)
    (descr http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf)
    (tags "LED RGB PLCC-6")
    (attr smd)
    (fp_text reference LED2 (at 3.81 0 90) (layer F.Fab))
    (fp_text value TX1818A (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.2 0) (layer F.SilkS))
    (pad 4 smd rect (at 2.6 1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at 2.6 0) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 2.6 -1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 D2))
    (pad 3 smd rect (at -2.6 1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 DIN))
    (pad 2 smd rect (at -2.6 0) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.6 -1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 D1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Normandled_WS2813-06_5.0x5.0mm_Pitch1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TX1818A:TX1818A_5.0x5.0mm_Pad1.1mm (layer F.Cu) (tedit 5B97295A)
    (at 68.499999 145)
    (descr http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf)
    (tags "LED RGB PLCC-6")
    (attr smd)
    (fp_text reference LED3 (at 3.81 0 90) (layer F.Fab))
    (fp_text value TX1818A (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.2 0) (layer F.SilkS))
    (pad 4 smd rect (at 2.6 1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at 2.6 0) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 2.6 -1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 D3))
    (pad 3 smd rect (at -2.6 1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 D1))
    (pad 2 smd rect (at -2.6 0) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.6 -1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 D2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Normandled_WS2813-06_5.0x5.0mm_Pitch1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TX1818A:TX1818A_5.0x5.0mm_Pad1.1mm (layer F.Cu) (tedit 5B97295A)
    (at 82.499999 145)
    (descr http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf)
    (tags "LED RGB PLCC-6")
    (attr smd)
    (fp_text reference LED5 (at 3.81 0 90) (layer F.Fab))
    (fp_text value TX1818A (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0.2 0) (layer F.SilkS))
    (pad 4 smd rect (at 2.6 1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at 2.6 0) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 6 smd rect (at 2.6 -1.6) (size 1.1 1) (drill (offset -0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 D5))
    (pad 3 smd rect (at -2.6 1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 D3))
    (pad 2 smd rect (at -2.6 0) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.6 -1.6) (size 1.1 1) (drill (offset 0.4 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 D4))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Normandled_WS2813-06_5.0x5.0mm_Pitch1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDStrip:LEDStrip_SolderWirePad_1x04_P9x1mm_Drill0.6mm locked (layer F.Cu) (tedit 5B99A4FB)
    (at 50.5079 148.4757 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference IN (at 3.048 1.2065 90) (layer F.SilkS) hide)
    (fp_text value LEDStrip_SolderWirePad_1x04_P9x1mm_Drill0.6mm (at 3.048 2.286 90) (layer F.Fab))
    (fp_text user %R (at 3.302 0 90) (layer F.Fab))
    (pad 4 thru_hole rect (at 6.096 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 3 thru_hole rect (at 4.064 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 DIN))
    (pad 2 thru_hole rect (at 1.9685 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 BIN))
    (pad 1 thru_hole oval (at -0.127 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module LEDStrip:LEDStrip_SolderWirePad_1x04_P9x1mm_Drill0.6mm locked (layer F.Cu) (tedit 5B99A4B9)
    (at 86.487 148.5011 90)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference OUT (at 3.048 1.2065 90) (layer F.SilkS) hide)
    (fp_text value LEDStrip_SolderWirePad_1x04_P9x1mm_Drill0.6mm (at 3.048 2.286 90) (layer F.Fab))
    (fp_text user %R (at 3.302 0 90) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.127 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 1.9685 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 D4))
    (pad 3 thru_hole rect (at 4.064 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 D5))
    (pad 4 thru_hole rect (at 6.096 0 90) (size 1.5 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 VDD))
  )
  (gr_text B (at 69.2785 146.785) (layer B.SilkS))
  (gr_text "EST\n'73" (at 65.913 146.685) (layer B.SilkS))
  (gr_text "LED Test 1.1mm Pad   Rev A" (at 68.5165 143.0655) (layer B.SilkS))
  (target plus (at 68.5292 145.51944) (size 5) (width 0.05) (layer Edge.Cuts))
  (gr_text +5 (at 85.979 142.3035) (layer B.SilkS))
  (gr_text GND (at 85.9155 148.6535) (layer B.SilkS))
  (gr_text DOUT (at 85.979 144.4625) (layer B.SilkS))
  (gr_text BOUT (at 85.979 146.558) (layer B.SilkS))
  (gr_text BIN (at 50.9905 146.4945) (layer B.SilkS))
  (gr_text DIN (at 50.9905 144.4625) (layer B.SilkS))
  (gr_text GND (at 51.054 148.6535) (layer B.SilkS))
  (gr_text +5 (at 50.9905 142.367) (layer B.SilkS))
  (gr_line (start 50 141) (end 87 141) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 150) (end 50 141) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87 150) (end 50 150) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87 141) (end 87 150) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 150) (xy 50 150) (xy 50 141) (xy 87 141)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 150) (xy 50 150) (xy 50 141) (xy 87 141)
      )
    )
  )
)
