(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.644)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.025))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.524) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.025))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 135.400508 91.26)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/Electronics/COIN project/COIN-SHITHz board/")
    )
  )
  (net 0 "")
  (net 1 "Net-(Con2-Pad1)")
  (net 2 "Net-(Con2-Pad2)")
  (net 3 "Net-(Con2-Pad3)")
  (net 4 "Net-(Con2-Pad4)")
  (net 5 "Net-(Con1-Pad5)")
  (net 6 "Net-(Con1-Pad6)")
  (net 7 "Net-(Con1-Pad7)")
  (net 8 "Net-(Con1-Pad8)")
  (net 9 "unconnected-(Con1-Pad9)")
  (net 10 "unconnected-(Con1-Pad10)")
  (net 11 "unconnected-(Con1-Pad11)")
  (net 12 "unconnected-(Con1-Pad12)")
  (net 13 "unconnected-(Con1-Pad13)")
  (net 14 "unconnected-(Con1-Pad14)")
  (net 15 "unconnected-(Con1-Pad15)")
  (net 16 "unconnected-(Con1-Pad16)")
  (net 17 "unconnected-(Con1-Pad17)")
  (net 18 "unconnected-(Con1-Pad18)")
  (net 19 "unconnected-(Con1-Pad19)")
  (net 20 "unconnected-(Con1-Pad20)")
  (net 21 "unconnected-(Con1-Pad21)")
  (net 22 "unconnected-(Con1-Pad22)")
  (net 23 "unconnected-(Con1-Pad23)")
  (net 24 "unconnected-(Con1-Pad24)")
  (net 25 "unconnected-(Con1-Pad25)")
  (net 26 "unconnected-(Con1-Pad26)")
  (net 27 "unconnected-(Con1-Pad27)")
  (net 28 "unconnected-(Con1-Pad28)")
  (net 29 "unconnected-(Con1-Pad29)")
  (net 30 "unconnected-(Con1-Pad30)")
  (net 31 "unconnected-(Con1-Pad31)")
  (net 32 "unconnected-(Con1-Pad32)")
  (net 33 "unconnected-(Con1-Pad33)")
  (net 34 "unconnected-(Con1-Pad34)")
  (net 35 "unconnected-(Con1-Pad35)")
  (net 36 "unconnected-(Con1-Pad36)")
  (net 37 "unconnected-(Con1-Pad37)")
  (net 38 "unconnected-(Con1-Pad38)")
  (net 39 "unconnected-(Con1-Pad39)")
  (net 40 "unconnected-(Con1-Pad40)")
  (net 41 "unconnected-(Con1-Pad41)")
  (net 42 "unconnected-(Con1-Pad42)")
  (net 43 "unconnected-(Con1-Pad43)")
  (net 44 "unconnected-(Con1-Pad44)")
  (net 45 "unconnected-(Con1-Pad45)")
  (net 46 "unconnected-(Con1-Pad46)")
  (net 47 "unconnected-(Con1-Pad47)")
  (net 48 "unconnected-(Con1-Pad48)")
  (net 49 "unconnected-(Con1-Pad49)")
  (net 50 "unconnected-(Con1-Pad50)")
  (net 51 "unconnected-(Con1-Pad51)")
  (net 52 "unconnected-(Con1-Pad52)")
  (net 53 "Net-(Con3-Pad1)")
  (net 54 "Net-(Con3-Pad2)")
  (net 55 "Net-(Con3-Pad3)")
  (net 56 "Net-(Con3-Pad4)")
  (net 57 "Net-(Con3-Pad5)")
  (net 58 "Net-(Con3-Pad6)")
  (net 59 "Net-(Con3-Pad7)")
  (net 60 "Net-(Con3-Pad8)")
  (footprint "Connector_Samtec_manual:SLM-102-01-X-S" (layer "F.Cu")
    (tedit 64BAF33F)
    (at 135.400508 119.26)
    (descr "LOW PROFILE .050 [1.27] SOCKET STRIP ASM.")
    (attr through_hole)
    (fp_text reference "Con5" (at -0.63502 -2.159068) (layer "F.SilkS"))
    (fp_text value "SLM-102-01-X-S" (at 1.65178 2.28708) (layer "F.Fab"))
    (fp_text user "1" (at 1.325 -2.225) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0.635 0) (size 1.0668 1.0668) (drill 0.7874) (layers *.Cu *.Mask))
    (pad "2" thru_hole circle (at -0.635 0) (size 1.0668 1.0668) (drill 0.7874) (layers *.Cu *.Mask))
  )
  (footprint "ENGdownloadedFootprint:Omron XF2M50151A" (layer "F.Cu")
    (tedit 0)
    (at 165.400508 109.26 60)
    (descr "XF2M-5015-1A")
    (tags "Connector")
    (property "Datasheet_1" "http://omronfs.omron.com/en_US/ecb/products/pdf/en-xf2m.pdf")
    (property "Footprint_1" "XF2M50151A")
    (property "Height" "3")
    (property "Manufacturer_Name" "Omron Electronics")
    (property "Manufacturer_Part_Number" "XF2M-5015-1A")
    (property "Mouser Part Number" "653-XF2M-5015-1A")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Omron-Electronics/XF2M-5015-1A?qs=9iNEzSI19qVl7hYv8histQ%3D%3D")
    (property "Reference_1" "J")
    (property "Sheetfile" "COIN.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "XF2M-5015-1A")
    (attr smd)
    (fp_text reference "Con1" (at 0 0 60) (layer "F.SilkS"))
    (fp_text value "Omron_XF2M-5015-1A" (at 0 0 60) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 60) (layer "F.Fab"))
    (pad "1" smd rect (at -12.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Con2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -11.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(Con2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -11.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Con2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -10.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(Con2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" smd rect (at -10.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Con1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" smd rect (at -9.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Con1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" smd rect (at -9.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(Con1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" smd rect (at -8.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(Con1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" smd rect (at -8.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(Con1-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" smd rect (at -7.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(Con1-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" smd rect (at -7.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(Con1-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" smd rect (at -6.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "unconnected-(Con1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" smd rect (at -6.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "unconnected-(Con1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" smd rect (at -5.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "unconnected-(Con1-Pad14)") (pinfunction "14") (pintype "passive"))
    (pad "15" smd rect (at -5.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(Con1-Pad15)") (pinfunction "15") (pintype "passive"))
    (pad "16" smd rect (at -4.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(Con1-Pad16)") (pinfunction "16") (pintype "passive"))
    (pad "17" smd rect (at -4.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(Con1-Pad17)") (pinfunction "17") (pintype "passive"))
    (pad "18" smd rect (at -3.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(Con1-Pad18)") (pinfunction "18") (pintype "passive"))
    (pad "19" smd rect (at -3.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(Con1-Pad19)") (pinfunction "19") (pintype "passive"))
    (pad "20" smd rect (at -2.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(Con1-Pad20)") (pinfunction "20") (pintype "passive"))
    (pad "21" smd rect (at -2.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(Con1-Pad21)") (pinfunction "21") (pintype "passive"))
    (pad "22" smd rect (at -1.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(Con1-Pad22)") (pinfunction "22") (pintype "passive"))
    (pad "23" smd rect (at -1.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(Con1-Pad23)") (pinfunction "23") (pintype "passive"))
    (pad "24" smd rect (at -0.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(Con1-Pad24)") (pinfunction "24") (pintype "passive"))
    (pad "25" smd rect (at -0.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(Con1-Pad25)") (pinfunction "25") (pintype "passive"))
    (pad "26" smd rect (at 0.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(Con1-Pad26)") (pinfunction "26") (pintype "passive"))
    (pad "27" smd rect (at 0.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(Con1-Pad27)") (pinfunction "27") (pintype "passive"))
    (pad "28" smd rect (at 1.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(Con1-Pad28)") (pinfunction "28") (pintype "passive"))
    (pad "29" smd rect (at 1.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(Con1-Pad29)") (pinfunction "29") (pintype "passive"))
    (pad "30" smd rect (at 2.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(Con1-Pad30)") (pinfunction "30") (pintype "passive"))
    (pad "31" smd rect (at 2.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(Con1-Pad31)") (pinfunction "31") (pintype "passive"))
    (pad "32" smd rect (at 3.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(Con1-Pad32)") (pinfunction "32") (pintype "passive"))
    (pad "33" smd rect (at 3.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(Con1-Pad33)") (pinfunction "33") (pintype "passive"))
    (pad "34" smd rect (at 4.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(Con1-Pad34)") (pinfunction "34") (pintype "passive"))
    (pad "35" smd rect (at 4.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(Con1-Pad35)") (pinfunction "35") (pintype "passive"))
    (pad "36" smd rect (at 5.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(Con1-Pad36)") (pinfunction "36") (pintype "passive"))
    (pad "37" smd rect (at 5.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(Con1-Pad37)") (pinfunction "37") (pintype "passive"))
    (pad "38" smd rect (at 6.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(Con1-Pad38)") (pinfunction "38") (pintype "passive"))
    (pad "39" smd rect (at 6.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(Con1-Pad39)") (pinfunction "39") (pintype "passive"))
    (pad "40" smd rect (at 7.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(Con1-Pad40)") (pinfunction "40") (pintype "passive"))
    (pad "41" smd rect (at 7.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(Con1-Pad41)") (pinfunction "41") (pintype "passive"))
    (pad "42" smd rect (at 8.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(Con1-Pad42)") (pinfunction "42") (pintype "passive"))
    (pad "43" smd rect (at 8.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(Con1-Pad43)") (pinfunction "43") (pintype "passive"))
    (pad "44" smd rect (at 9.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(Con1-Pad44)") (pinfunction "44") (pintype "passive"))
    (pad "45" smd rect (at 9.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "unconnected-(Con1-Pad45)") (pinfunction "45") (pintype "passive"))
    (pad "46" smd rect (at 10.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(Con1-Pad46)") (pinfunction "46") (pintype "passive"))
    (pad "47" smd rect (at 10.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "unconnected-(Con1-Pad47)") (pinfunction "47") (pintype "passive"))
    (pad "48" smd rect (at 11.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "unconnected-(Con1-Pad48)") (pinfunction "48") (pintype "passive"))
    (pad "49" smd rect (at 11.75 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "unconnected-(Con1-Pad49)") (pinfunction "49") (pintype "passive"))
    (pad "50" smd rect (at 12.25 -2.015 60) (size 0.25 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "unconnected-(Con1-Pad50)") (pinfunction "50") (pintype "passive"))
    (pad "51" smd rect (at -13.9 1.885 150) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "unconnected-(Con1-Pad51)") (pinfunction "51") (pintype "passive"))
    (pad "52" smd rect (at 13.9 1.885 150) (size 1.5 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(Con1-Pad52)") (pinfunction "52") (pintype "passive"))
    (model "XF2M-5015-1A.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ENGdownloadedFootprint:8501000810001000" (layer "F.Cu")
    (tedit 0)
    (at 125.400508 127.26 90)
    (descr "850-10-008-10-001000-4")
    (tags "Connector")
    (property "Arrow Part Number" "850-10-008-10-001000")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/850-10-008-10-001000/mill-max")
    (property "Datasheet_1" "https://www.mill-max.com/products/interconnect/machined-pin-header/850-xx-xxx-10-001000/850-10-008-10-001000?s_term=850-10-008-10-001000&s_type=Quick/Product/Part%20Number%20Search")
    (property "Footprint_1" "8501000810001000")
    (property "Height" "5.207")
    (property "Manufacturer_Name" "Mill-Max")
    (property "Manufacturer_Part_Number" "850-10-008-10-001000")
    (property "Mouser Part Number" "575-8501000810001000")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mill-Max/850-10-008-10-001000?qs=iJx90KzHWBqzImkU8uqnzw%3D%3D")
    (property "Reference_1" "J")
    (property "Sheetfile" "COIN.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "850-10-008-10-001000")
    (attr through_hole)
    (fp_text reference "Con3" (at 4.125 3.775 270) (layer "F.SilkS"))
    (fp_text value "850-10-008-10-001000" (at 4.445 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.445 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 53 "Net-(Con3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 54 "Net-(Con3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 55 "Net-(Con3-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.81 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 56 "Net-(Con3-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 5.08 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 57 "Net-(Con3-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 58 "Net-(Con3-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 7.62 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 59 "Net-(Con3-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 8.89 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 60 "Net-(Con3-Pad8)") (pinfunction "8") (pintype "passive"))
    (model "850-10-008-10-001000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ENGdownloadedFootprint:8501000810001000" (layer "F.Cu")
    (tedit 0)
    (at 105.400508 113.26 120)
    (descr "850-10-008-10-001000-4")
    (tags "Connector")
    (property "Arrow Part Number" "850-10-008-10-001000")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/850-10-008-10-001000/mill-max")
    (property "Datasheet_1" "https://www.mill-max.com/products/interconnect/machined-pin-header/850-xx-xxx-10-001000/850-10-008-10-001000?s_term=850-10-008-10-001000&s_type=Quick/Product/Part%20Number%20Search")
    (property "Footprint_1" "8501000810001000")
    (property "Height" "5.207")
    (property "Manufacturer_Name" "Mill-Max")
    (property "Manufacturer_Part_Number" "850-10-008-10-001000")
    (property "Mouser Part Number" "575-8501000810001000")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mill-Max/850-10-008-10-001000?qs=iJx90KzHWBqzImkU8uqnzw%3D%3D")
    (property "Reference_1" "J")
    (property "Sheetfile" "COIN.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "850-10-008-10-001000")
    (attr through_hole)
    (fp_text reference "Con4" (at -3.348974 0.000593 210) (layer "F.SilkS"))
    (fp_text value "850-10-008-10-001000" (at 4.445 0 120) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.445 0 120) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 53 "Net-(Con3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 54 "Net-(Con3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 55 "Net-(Con3-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.81 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 56 "Net-(Con3-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 5.08 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 57 "Net-(Con3-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 58 "Net-(Con3-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 7.62 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 59 "Net-(Con3-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 8.89 0 120) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 60 "Net-(Con3-Pad8)") (pinfunction "8") (pintype "passive"))
    (model "850-10-008-10-001000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ENGdownloadedFootprint:8501000810001000" (layer "F.Cu")
    (tedit 0)
    (at 145.400508 127.26 90)
    (descr "850-10-008-10-001000-4")
    (tags "Connector")
    (property "Arrow Part Number" "850-10-008-10-001000")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/850-10-008-10-001000/mill-max")
    (property "Datasheet_1" "https://www.mill-max.com/products/interconnect/machined-pin-header/850-xx-xxx-10-001000/850-10-008-10-001000?s_term=850-10-008-10-001000&s_type=Quick/Product/Part%20Number%20Search")
    (property "Footprint_1" "8501000810001000")
    (property "Height" "5.207")
    (property "Manufacturer_Name" "Mill-Max")
    (property "Manufacturer_Part_Number" "850-10-008-10-001000")
    (property "Mouser Part Number" "575-8501000810001000")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Mill-Max/850-10-008-10-001000?qs=iJx90KzHWBqzImkU8uqnzw%3D%3D")
    (property "Reference_1" "J")
    (property "Sheetfile" "COIN.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "850-10-008-10-001000")
    (attr through_hole)
    (fp_text reference "Con2" (at 4.325 -3.25 90) (layer "F.SilkS"))
    (fp_text value "850-10-008-10-001000" (at 4.445 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.445 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 1 "Net-(Con2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 2 "Net-(Con2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 3 "Net-(Con2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.81 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 4 "Net-(Con2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 5.08 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 5 "Net-(Con1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 6 "Net-(Con1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 7.62 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 7 "Net-(Con1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 8.89 0 90) (size 1.07 1.07) (drill 0.606) (layers *.Cu *.Mask)
      (net 8 "Net-(Con1-Pad8)") (pinfunction "8") (pintype "passive"))
    (model "850-10-008-10-001000.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 104.699031 65.225) (end 91.048554 88.2943) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 179.744792 88.210684) (mid 179.849508 91.26) (end 179.744792 94.309316) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 140.479508 131.9) (end 140.479508 135.41876) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 160.212935 128.139484) (end 179.744792 94.309316) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 139.209508 130.63) (mid 140.107534 131.001974) (end 140.479508 131.9) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 154.449508 110.31) (end 155.973508 110.31) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_line (start 130.319508 131.9) (end 130.319508 135.41876) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 104.699031 65.225) (end 166.474001 65.225) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 91.054224 94.309316) (mid 90.949528 91.301904) (end 91.048554 88.2943) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 131.589508 130.63) (end 139.209508 130.63) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 160.212935 128.139484) (mid 150.78298 132.963133) (end 140.479508 135.41876) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 135.399508 91.26) (end 159.402508 91.26) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_arc (start 130.319508 131.9) (mid 130.691482 131.001974) (end 131.589508 130.63) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 116.349508 72.21) (end 117.873508 72.21) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_arc (start 130.319508 135.41876) (mid 120.016036 132.963133) (end 110.586081 128.139484) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 116.349508 110.31) (end 117.873508 110.31) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_line (start 91.054224 94.309316) (end 110.586081 128.139484) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 179.744792 88.210684) (end 166.474001 65.225) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 154.449508 72.21) (end 155.973508 72.21) (layer "Edge.Cuts") (width 0.2) (fill none))
)
