<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="14.605" y2="0" width="0" layer="20"/>
<wire x1="14.605" y1="0" x2="14.605" y2="6.35" width="0" layer="20"/>
<wire x1="14.605" y1="6.35" x2="0" y2="6.35" width="0" layer="20"/>
<wire x1="0" y1="6.35" x2="0" y2="0" width="0" layer="20"/>
<text>Pyxida</text>
<text>Program</text>
<text>THIS ^ SIDE ^ EDGE</text>
</plain>
<libraries>
<library name="Teensy_DIY_v1.0">
<packages>
<package name="QFN50P300X300X100-17N">
</package>
</packages>
</library>
<library name="custom">
<packages>
<package name="4-0.49&quot;">
</package>
<package name="4.5X4.5_TACT_SWITCH">
</package>
</packages>
</library>
<library name="Preferred Parts">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MKL02" library="Teensy_DIY_v1.0" package="QFN50P300X300X100-17N" value="CURRENT_BOOTLOADER3X3MM"/>
<element name="U$1" library="custom" package="4-0.49&quot;" value="4-PINHEADER"/>
<element name="U$2" library="custom" package="4-0.49&quot;" value="4-PINHEADER"/>
<element name="C1" library="Preferred Parts" package="0402-CAP" value="0.1uF"/>
<element name="S1" library="custom" package="4.5X4.5_TACT_SWITCH" value="TACT_SWITCHESWITCH_TL3305"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="MKL02" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="MKL02" pad="2"/>
<contactref element="MKL02" pad="17"/>
<contactref element="C1" pad="2"/>
<contactref element="S1" pad="P$2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="PTA2">
<contactref element="MKL02" pad="9"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="PTA1">
<contactref element="MKL02" pad="6"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="PTA3">
<contactref element="MKL02" pad="7"/>
<contactref element="U$2" pad="P$4"/>
</signal>
<signal name="PROGRAM">
<contactref element="MKL02" pad="10"/>
<contactref element="S1" pad="P$3"/>
</signal>
<signal name="PTA0">
<contactref element="MKL02" pad="8"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="RST">
<contactref element="MKL02" pad="4"/>
<contactref element="MKL02" pad="13"/>
<contactref element="U$1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
