(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 65)
    (zones 0)
    (modules 17)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.635)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.27 0.635)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.56 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +15V)
  (net 2 /Prox_Out)
  (net 3 /UPDI)
  (net 4 /VIN)
  (net 5 /GND)
  (net 6 /Probe_Out)
  (net 7 /TxD)
  (net 8 /RxD)
  (net 9 /Ena_Prox)
  (net 10 /Probe_In)
  (net 11 /Spare)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net +15V)
    (add_net /Ena_Prox)
    (add_net /GND)
    (add_net /Probe_In)
    (add_net /Probe_Out)
    (add_net /Prox_Out)
    (add_net /RxD)
    (add_net /Spare)
    (add_net /TxD)
    (add_net /UPDI)
    (add_net /VIN)
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J6-Pad5)")
  )
  (net_class Minimum ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class Power ""
    (clearance 0.635)
    (trace_width 0.635)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.635)
    (diff_pair_gap 0.635)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 139.065 98.425 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J6 (at -2.54 3.81) (layer B.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 -7.41) (layer B.Fab))
    (fp_text user %R (at 1.27 -2.54 270) (layer B.Fab))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /UPDI))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 152.4 101.6)
    (fp_text reference TP9 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value PB3 (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 11 /Spare))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 149.86 97.155)
    (fp_text reference TP8 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value Probe_In (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 10 /Probe_In))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 154.94 97.155)
    (fp_text reference TP7 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value ENA_PROX (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 9 /Ena_Prox))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 157.48 101.6)
    (fp_text reference TP6 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value RxD (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 8 /RxD))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 147.32 101.6)
    (fp_text reference TP5 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value TxD (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 7 /TxD))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 154.94 106.045)
    (fp_text reference TP4 (at 2.54 -1.905) (layer F.SilkS))
    (fp_text value UPDI (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 3 /UPDI))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Boeing_6652:P70-2200045 (layer F.Cu) (tedit 5E9886D3)
    (at 149.86 106.045)
    (fp_text reference TP3 (at -3.175 -1.27) (layer F.SilkS))
    (fp_text value Probe_Out (at -0.1 3.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.25) (layers *.Cu *.Mask)
      (net 6 /Probe_Out))
    (model ${KIPRJMOD}/p70-2200045.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 146.05 113.665 270)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J5 (at -2.54 3.81 270) (layer B.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 1.27 -15.03 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -6.35) (layer B.Fab))
    (pad 12 thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Spare))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RxD))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TxD))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /UPDI))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Probe_Out))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Probe_In))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Ena_Prox))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GND))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /Prox_Out))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9E0C39)
    (at 155.575 85.725)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J4 (at 3.175 0) (layer F.SilkS))
    (fp_text value GND (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 /GND))
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9E0C39)
    (at 149.225 85.725)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J3 (at -3.175 0) (layer F.SilkS))
    (fp_text value Prox_Out (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 /Prox_Out))
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9E0C39)
    (at 149.225 92.075)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J2 (at -3.175 0) (layer F.SilkS))
    (fp_text value V_Prox (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 +15V))
  )
  (module Boeing_6652:1946_or_S70-332 locked (layer F.Cu) (tedit 5E9E0C39)
    (at 155.575 92.075)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference J1 (at 3.175 0) (layer F.SilkS))
    (fp_text value VBATT (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 /VIN))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 167.005 93.98)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 138.43 114.3)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 167.132 109.22)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad locked (layer F.Cu) (tedit 56D1B4CB)
    (at 138.43 88.9)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "M2 Screw" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text J2 (at 146.05 92.075) (layer B.SilkS))
  (gr_text J3 (at 149.225 82.55) (layer B.SilkS))
  (gr_text J4 (at 155.575 82.55) (layer B.SilkS))
  (gr_text J1 (at 158.75 92.075) (layer B.SilkS))
  (gr_text TP7 (at 157.48 95.25) (layer B.SilkS))
  (gr_text TP8 (at 147.32 95.25) (layer B.SilkS))
  (gr_text TP9 (at 149.86 99.695) (layer B.SilkS))
  (gr_text TP5 (at 144.78 99.695) (layer B.SilkS))
  (gr_text TP3 (at 146.685 104.775) (layer B.SilkS))
  (gr_text TP4 (at 157.48 104.14) (layer B.SilkS))
  (gr_text TP6 (at 160.02 99.695) (layer B.SilkS))
  (gr_text NC (at 158.75 119.276905 90) (layer B.SilkS))
  (gr_text RxD (at 156.21 119.657857 90) (layer B.SilkS))
  (gr_text UPDI (at 153.67 120.015 90) (layer B.SilkS))
  (gr_text PRBI (at 151.13 119.99119 90) (layer B.SilkS))
  (gr_text PB3 (at 158.75 110.37881 90) (layer B.SilkS))
  (gr_text TxD (at 156.21 110.569286 90) (layer B.SilkS))
  (gr_text PRBO (at 153.67 109.831191 90) (layer B.SilkS))
  (gr_text ENA (at 151.13 110.450238 90) (layer B.SilkS))
  (gr_text PRXO (at 148.59 109.855 90) (layer B.SilkS))
  (gr_text GND (at 148.59 119.776905 90) (layer B.SilkS))
  (gr_text PRXV (at 146.05 120.157857 90) (layer B.SilkS))
  (gr_text VIN (at 146.05 110.664524 90) (layer B.SilkS))
  (gr_text 2 (at 143.51 116.205 90) (layer B.SilkS))
  (gr_text 1 (at 143.51 113.665 90) (layer B.SilkS))
  (gr_text 2 (at 136.525 95.885) (layer B.SilkS))
  (gr_text 1 (at 139.065 95.885) (layer B.SilkS))
  (gr_text GND (at 132.715 103.505) (layer B.SilkS))
  (gr_text UPDI (at 132.715 98.425) (layer B.SilkS))
  (gr_text VIN (at 142.24 98.425) (layer B.SilkS))
  (gr_text "PRGMR A\nCriterion MS\n6652 2020 04" (at 159.004 88.392) (layer B.SilkS))
  (gr_circle (center 152.4 101.6) (end 174.625 101.6) (layer Edge.Cuts) (width 0.254))
)
