<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="12.5" x2="0" y2="2.5" width="0" layer="20"/>
<wire x1="0" y1="2.5" x2="2.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.5" y1="0" x2="25.5" y2="0" width="0" layer="20"/>
<wire x1="25.5" y1="0" x2="28" y2="2.5" width="0" layer="20" curve="90"/>
<wire x1="28" y1="2.5" x2="28" y2="12.5" width="0" layer="20"/>
<wire x1="28" y1="12.5" x2="25.5" y2="15" width="0" layer="20" curve="90"/>
<wire x1="25.5" y1="15" x2="2.5" y2="15" width="0" layer="20"/>
<wire x1="2.5" y1="15" x2="0" y2="12.5" width="0" layer="20" curve="90"/>
<text>VOUT</text>
<text>GND</text>
<text>VOUT</text>
<text>LBO</text>
<text>GND</text>
<text>GND</text>
<text>EN</text>
<text>LBI</text>
<text>GND</text>
<text>VCC</text>
<text>Power Converter
TPS61092
Vcc 1.8-5.5V
Vout 5.0V
Iout Max 2A</text>
</plain>
<libraries>
<library name="lucky-resistor">
<packages>
<package name="CPOL-2312-AVX-TAJ-C">
<description>&lt;p&gt;Footprint for the AVX TAJ capacitors with the size "C" 2312&lt;/p&gt;</description>
</package>
<package name="CAPACITOR-0805-VISHAY">
</package>
<package name="S-PVQFN-N16">
<description>&lt;p&gt;The recommended package for Texas Instruments chips with the die on the bottom side for optimal
heat dissipation.&lt;/p&gt;
&lt;p&gt;Longer pads as recommended for hand soldering. The recommended length over the chip size is just 0.4mm which is too short to heat it using a solder iron. Therefore a 0.8mm is used in this package design.&lt;/p&gt;</description>
</package>
<package name="CON-SOLDER-POINT2">
</package>
<package name="L-PCC-M0530M-LP">
<description>&lt;p&gt;Recommended landing pattern for the coil series PCC-M0530M-LP from Panasonic.&lt;/p&gt;
&lt;p&gt;Product numbers: ETQP3M???KVP&lt;/p&gt;</description>
</package>
<package name="RESISTOR-0805-KOA-RK73-2A">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="JUMPER-SMD-ON">
<description>&lt;h3&gt;SMD Jumper Connected&lt;/h3&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="lucky-resistor" package="CPOL-2312-AVX-TAJ-C" value="100µF">
<attribute name="NAME"/>
</element>
<element name="C1" library="lucky-resistor" package="CAPACITOR-0805-VISHAY" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="lucky-resistor" package="CAPACITOR-0805-VISHAY" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="lucky-resistor" package="CAPACITOR-0805-VISHAY" value="2.2µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="lucky-resistor" package="S-PVQFN-N16" value="TPS61092">
<attribute name="NAME"/>
</element>
<element name="J4" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J1" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J2" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J3" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J5" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="L1" library="lucky-resistor" package="L-PCC-M0530M-LP" value="6.8µH">
<attribute name="NAME"/>
</element>
<element name="R1" library="lucky-resistor" package="RESISTOR-0805-KOA-RK73-2A" value="330kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="lucky-resistor" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="lucky-resistor" package="RESISTOR-0805-KOA-RK73-2A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="lucky-resistor" package="JUMPER-SMD-ON" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J7" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J8" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J9" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
<element name="J10" library="lucky-resistor" package="CON-SOLDER-POINT2" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="5" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="6" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="7" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="GND@1" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="GND@2" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="GND@3" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="GND@4" route="any" routetag="G$1.PGND"/>
<contactref element="IC1" pad="GND@5" route="any" routetag="G$1.PGND"/>
<contactref element="J5" pad="1"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="13"/>
<contactref element="J3" pad="1"/>
<contactref element="C4" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP1" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="16"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="A"/>
<contactref element="J4" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="EN">
<contactref element="IC1" pad="11"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SW">
<contactref element="L1" pad="1"/>
<contactref element="IC1" pad="3" route="any" routetag="G$1.SW"/>
<contactref element="IC1" pad="4" route="any" routetag="G$1.SW"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="LBI">
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="LBO">
<contactref element="IC1" pad="12"/>
<contactref element="J8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
