<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<circle x="41.91" y="53.975" radius="2.55" width="0.05" layer="20"/>
<wire x1="55.5625" y1="101.6" x2="33.02" y2="101.6" width="0" layer="20"/>
<wire x1="33.02" y1="101.6" x2="31.115" y2="99.695" width="0" layer="20"/>
<wire x1="31.115" y1="99.695" x2="31.115" y2="95.885" width="0" layer="20"/>
<wire x1="31.115" y1="95.885" x2="31.115" y2="68.58" width="0" layer="20" curve="137.896229"/>
<wire x1="31.115" y1="68.58" x2="31.115" y2="64.135" width="0" layer="20"/>
<wire x1="31.115" y1="64.135" x2="32.385" y2="62.865" width="0" layer="20"/>
<wire x1="32.385" y1="62.865" x2="44.45" y2="62.865" width="0" layer="20"/>
<wire x1="44.45" y1="62.865" x2="48.26" y2="59.055" width="0" layer="20"/>
<wire x1="48.26" y1="59.055" x2="55.5625" y2="59.055" width="0" layer="20"/>
<wire x1="55.5625" y1="59.055" x2="56.8325" y2="60.325" width="0" layer="20"/>
<wire x1="56.8325" y1="60.325" x2="56.8325" y2="62.70625" width="0" layer="20"/>
<wire x1="56.8325" y1="66.04" x2="56.8325" y2="87.63" width="0" layer="20"/>
<wire x1="56.8325" y1="90.96375" x2="56.8325" y2="100.33" width="0" layer="20"/>
<wire x1="56.8325" y1="100.33" x2="55.5625" y2="101.6" width="0" layer="20"/>
<circle x="34.29" y="82.55" radius="5.0038" width="0.05" layer="20"/>
<circle x="34.29" y="53.975" radius="2.55" width="0.05" layer="20"/>
<circle x="29.21" y="48.26" radius="2.55" width="0.05" layer="20"/>
<circle x="30.48" y="40.64" radius="2.55" width="0.05" layer="20"/>
<circle x="38.1" y="36.5125" radius="2.55" width="0.05" layer="20"/>
<circle x="45.72" y="40.64" radius="2.55" width="0.05" layer="20"/>
<circle x="46.99" y="48.26" radius="2.55" width="0.05" layer="20"/>
<circle x="46.99" y="24.765" radius="2.55" width="0.05" layer="20"/>
<circle x="39.37" y="24.765" radius="2.55" width="0.05" layer="20"/>
<circle x="34.29" y="19.05" radius="2.55" width="0.05" layer="20"/>
<circle x="35.56" y="11.43" radius="2.55" width="0.05" layer="20"/>
<circle x="43.18" y="7.3025" radius="2.55" width="0.05" layer="20"/>
<circle x="50.8" y="11.43" radius="2.55" width="0.05" layer="20"/>
<circle x="52.07" y="19.05" radius="2.55" width="0.05" layer="20"/>
<wire x1="59.69" y1="10.16" x2="67.31" y2="2.54" width="0" layer="20" curve="73.739795"/>
<wire x1="67.31" y1="2.54" x2="113.03" y2="2.54" width="0" layer="20"/>
<wire x1="113.03" y1="2.54" x2="120.65" y2="10.16" width="0" layer="20" curve="73.739795"/>
<wire x1="120.65" y1="10.16" x2="120.65" y2="95.25" width="0" layer="20"/>
<wire x1="59.69" y1="95.25" x2="59.69" y2="90.96375" width="0" layer="20"/>
<wire x1="59.69" y1="87.63" x2="59.69" y2="66.04" width="0" layer="20"/>
<wire x1="59.69" y1="62.70625" x2="59.69" y2="47.625" width="0" layer="20"/>
<wire x1="59.69" y1="43.815" x2="59.69" y2="18.415" width="0" layer="20"/>
<wire x1="59.69" y1="14.605" x2="59.69" y2="10.16" width="0" layer="20"/>
<wire x1="59.69" y1="95.25" x2="66.04" y2="101.6" width="0" layer="20" curve="-45.23973"/>
<wire x1="66.04" y1="101.6" x2="114.3" y2="101.6" width="0" layer="20"/>
<wire x1="114.3" y1="101.6" x2="120.65" y2="95.25" width="0" layer="20" curve="-45.23973"/>
<text>POWER</text>
<text>ULN2804</text>
<text>ULN2804</text>
<text>ATMEGA328</text>
<text>GND-VCC-A0-A1-A2-A3</text>
<text>ON</text>
<text>OFF</text>
<text>SDA-SCL-GND-VCC</text>
<text>SCL-SDA-VCC-GND</text>
<text>RESET
SCK
MISO</text>
<text>GND
MOSI
VCC</text>
<wire x1="56.515" y1="14.605" x2="56.515" y2="18.415" width="0" layer="20" curve="-343.754474"/>
<wire x1="56.515" y1="18.415" x2="59.69" y2="18.415" width="0" layer="20"/>
<wire x1="56.515" y1="14.605" x2="59.69" y2="14.605" width="0" layer="20"/>
<hole x="56.8325" y="17.93875" drill="0.5"/>
<hole x="56.99125" y="16.98625" drill="0.5"/>
<hole x="56.8325" y="15.08125" drill="0.5"/>
<hole x="56.99125" y="15.875" drill="0.5"/>
<hole x="59.3725" y="17.93875" drill="0.5"/>
<hole x="59.3725" y="17.145" drill="0.5"/>
<hole x="59.3725" y="16.51" drill="0.5"/>
<hole x="59.3725" y="15.71625" drill="0.5"/>
<hole x="59.3725" y="15.08125" drill="0.5"/>
<wire x1="52.07" y1="47.625" x2="52.07" y2="43.815" width="0" layer="20" curve="344.485903"/>
<wire x1="52.07" y1="43.815" x2="59.69" y2="43.815" width="0" layer="20"/>
<wire x1="52.07" y1="47.625" x2="59.69" y2="47.625" width="0" layer="20"/>
<hole x="52.54625" y="47.14875" drill="0.5"/>
<hole x="52.54625" y="46.355" drill="0.5"/>
<hole x="52.54625" y="45.72" drill="0.5"/>
<hole x="52.54625" y="45.085" drill="0.5"/>
<hole x="52.54625" y="44.29125" drill="0.5"/>
<hole x="59.3725" y="47.14875" drill="0.5"/>
<hole x="59.3725" y="46.355" drill="0.5"/>
<hole x="59.3725" y="45.72" drill="0.5"/>
<hole x="59.3725" y="45.085" drill="0.5"/>
<hole x="59.3725" y="44.29125" drill="0.5"/>
<wire x1="56.8325" y1="90.96375" x2="59.69" y2="90.96375" width="0" layer="20"/>
<hole x="57.15" y="90.4875" drill="0.5"/>
<hole x="57.15" y="89.69375" drill="0.5"/>
<hole x="57.15" y="88.9" drill="0.5"/>
<hole x="57.15" y="88.10625" drill="0.5"/>
<hole x="59.3725" y="90.4875" drill="0.5"/>
<hole x="59.3725" y="89.69375" drill="0.5"/>
<hole x="59.3725" y="88.9" drill="0.5"/>
<hole x="59.3725" y="88.10625" drill="0.5"/>
<hole x="57.15" y="65.56375" drill="0.5"/>
<hole x="57.15" y="64.77" drill="0.5"/>
<hole x="57.15" y="63.97625" drill="0.5"/>
<hole x="57.15" y="63.1825" drill="0.5"/>
<hole x="59.3725" y="65.56375" drill="0.5"/>
<hole x="59.3725" y="64.77" drill="0.5"/>
<hole x="59.3725" y="63.97625" drill="0.5"/>
<hole x="59.3725" y="63.1825" drill="0.5"/>
<wire x1="59.69" y1="66.04" x2="56.8325" y2="66.04" width="0" layer="20"/>
<wire x1="56.8325" y1="62.70625" x2="59.69" y2="62.70625" width="0" layer="20"/>
<wire x1="56.8325" y1="87.63" x2="59.69" y2="87.63" width="0" layer="20"/>
<text>RESET</text>
<text>BOBRICIUS</text>
<text>SLOVAKIA</text>
<text>PD0-PD7</text>
<text>PB7-PB0</text>
<text>A1</text>
<text>A2</text>
<text>A0</text>
<text>A3</text>
</plain>
<libraries>
<library name="avr">
<packages>
<package name="DIL28/3">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="rcl-ez">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_3.0_PLATED_SQUAREVIAS">
</package>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="MOUNTINGHOLE_3.0_PLATED_VIAS">
</package>
</packages>
</library>
<library name="uln-udn">
<description>&lt;b&gt;Driver Arrays&lt;/b&gt;&lt;p&gt;
ULN and UDN Series&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X16_LOCK">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-NS">
</package>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTERY-AA-KIT">
<description>&lt;h3&gt;AA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AA battery&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="avr" package="DIL28/3" value="ATMEGA168P"/>
<element name="R1" library="rcl-ez" package="R0603" value="10K"/>
<element name="R7" library="rcl" package="R0603" value="4k7"/>
<element name="I2C1" library="SparkFun" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="rc-master-smd" package="C0603" value="100n"/>
<element name="C9" library="rc-master-smd" package="C0603" value="100n"/>
<element name="R2" library="rcl" package="R0603" value="4k7"/>
<element name="I2C4" library="SparkFun" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="uln-udn" package="DIL18" value="">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="microbuilder" package="MOUNTINGHOLE_3.0_PLATED_SQUAREVIAS" value="MOUNTINGHOLE3.0SQUARE">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$5" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$7" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$8" library="microbuilder" package="MOUNTINGHOLE_3.0_PLATED_VIAS" value="MOUNTINGHOLE">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$9" library="microbuilder" package="MOUNTINGHOLE_3.0_PLATED_VIAS" value="MOUNTINGHOLE">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="JP4" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="BT1" library="SparkFun-Batteries" package="BATTERY-AA-KIT" value="">
<attribute name="SF_SKU" value="PRT-07949"/>
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="VALUE"/>
</element>
<element name="BT2" library="SparkFun-Batteries" package="BATTERY-AA-KIT" value="">
<attribute name="SF_SKU" value="PRT-07949"/>
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="uln-udn" package="DIL18" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X16_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="R3" library="rcl" package="0309/12" value="10R"/>
<element name="R4" library="rcl" package="0309/12" value="10R"/>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="1k"/>
<element name="C7" library="rcl" package="E2,5-7" value="10uF"/>
<element name="C1" library="rcl" package="E2,5-7" value="10uF"/>
<element name="C2" library="rcl" package="E2,5-7" value="10uF"/>
<element name="JP2" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$2" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$3" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$10" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$11" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$12" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$13" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$14" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$15" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$16" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$17" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="C3" library="rcl" package="E2,5-7" value="10uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="22"/>
<contactref element="I2C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="I2C4" pad="2"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC3" pad="9"/>
<contactref element="JP1" pad="6"/>
<contactref element="S4" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="S3" pad="3"/>
<contactref element="BT2" pad="GND@1"/>
<contactref element="LED1" pad="K"/>
<contactref element="C1" pad="-"/>
<contactref element="C7" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="J4" pad="1"/>
<contactref element="S5" pad="3"/>
<contactref element="C3" pad="-"/>
</signal>
<signal name="PB6">
<contactref element="IC1" pad="9"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="PB3">
<contactref element="IC1" pad="17"/>
<contactref element="IC3" pad="5"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="PB4">
<contactref element="IC1" pad="18"/>
<contactref element="IC3" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="23"/>
<contactref element="S4" pad="1"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="24"/>
<contactref element="S2" pad="1"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="25"/>
<contactref element="S1" pad="1"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="26"/>
<contactref element="S3" pad="1"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="PD1">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="PD0">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="21"/>
</signal>
<signal name="PB2">
<contactref element="IC1" pad="16"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="PB1">
<contactref element="IC1" pad="15"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="PB0">
<contactref element="IC1" pad="14"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="PD7">
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="PD6">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="PD5">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="PD4">
<contactref element="IC1" pad="6"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="PD3">
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="PD2">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="20"/>
<contactref element="I2C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="I2C4" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP4" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP2" pad="5"/>
<contactref element="J4" pad="2"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="S5" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="I2C1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="I2C4" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="I2C1" pad="4"/>
<contactref element="R7" pad="2"/>
<contactref element="I2C4" pad="3"/>
</signal>
<signal name="PB7">
<contactref element="IC1" pad="10"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="L8">
<contactref element="J1" pad="16"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="L6">
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="L7">
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="L5">
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="L4">
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="L3">
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="L1">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="L2">
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="BAT">
<contactref element="JP4" pad="4"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="BT1" pad="PWR@1"/>
</signal>
<signal name="PB5">
<contactref element="IC1" pad="19"/>
<contactref element="IC3" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="OL1">
<contactref element="J2" pad="16"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="OL2">
<contactref element="J2" pad="14"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="OL3">
<contactref element="J2" pad="12"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="OL4">
<contactref element="J2" pad="10"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="OL5">
<contactref element="J2" pad="8"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="OL6">
<contactref element="J2" pad="6"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="OL7">
<contactref element="J2" pad="4"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="OL8">
<contactref element="J2" pad="2"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="15"/>
<contactref element="J3" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="13"/>
<contactref element="J3" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="11"/>
<contactref element="J3" pad="12"/>
</signal>
<signal name="N$5">
<contactref element="J2" pad="9"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="N$6">
<contactref element="J2" pad="7"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="J6" pad="15"/>
<contactref element="J7" pad="16"/>
</signal>
<signal name="N$20">
<contactref element="J6" pad="13"/>
<contactref element="J7" pad="14"/>
</signal>
<signal name="N$21">
<contactref element="J6" pad="11"/>
<contactref element="J7" pad="12"/>
</signal>
<signal name="N$22">
<contactref element="J6" pad="9"/>
<contactref element="J7" pad="10"/>
</signal>
<signal name="N$23">
<contactref element="J6" pad="7"/>
<contactref element="J7" pad="8"/>
</signal>
<signal name="N$24">
<contactref element="J6" pad="5"/>
<contactref element="J7" pad="6"/>
</signal>
<signal name="N$25">
<contactref element="J6" pad="3"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="N$26">
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="OR1">
<contactref element="J6" pad="16"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="OR2">
<contactref element="J6" pad="14"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="OR3">
<contactref element="J6" pad="12"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="OR4">
<contactref element="J6" pad="10"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="OR5">
<contactref element="J6" pad="8"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="OR6">
<contactref element="J6" pad="6"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="OR7">
<contactref element="J6" pad="4"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="OR8">
<contactref element="J6" pad="2"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="N$11">
<contactref element="BT2" pad="PWR@1"/>
<contactref element="BT1" pad="GND@1"/>
</signal>
<signal name="VIN1">
<contactref element="IC2" pad="10"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="15"/>
<contactref element="J3" pad="13"/>
<contactref element="J3" pad="11"/>
<contactref element="J3" pad="9"/>
<contactref element="J3" pad="7"/>
<contactref element="J3" pad="5"/>
<contactref element="J3" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="VIN2">
<contactref element="IC3" pad="10"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="15"/>
<contactref element="J7" pad="13"/>
<contactref element="J7" pad="11"/>
<contactref element="J7" pad="9"/>
<contactref element="J7" pad="7"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C7" pad="+"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
