(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 63)
    (tracks 374)
    (zones 0)
    (modules 14)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6604)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6604)
    (user_trace_width 0.9652)
    (trace_clearance 0.2)
    (zone_clearance 0.635)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (user_via 0.381 0.254)
    (user_via 0.508 0.381)
    (user_via 0.762 0.4064)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 /sw1)
  (net 4 /led1)
  (net 5 "Net-(D1-Pad1)")
  (net 6 /led2)
  (net 7 /p20)
  (net 8 /p19)
  (net 9 /p18)
  (net 10 /p17)
  (net 11 /p16)
  (net 12 /p15)
  (net 13 /p14)
  (net 14 /p13)
  (net 15 /P12)
  (net 16 /P11)
  (net 17 /P10)
  (net 18 /P9)
  (net 19 /p8)
  (net 20 /p7)
  (net 21 /p6)
  (net 22 /p5)
  (net 23 /p4)
  (net 24 /p3)
  (net 25 /p2)
  (net 26 /p1)
  (net 27 /p40)
  (net 28 /p39)
  (net 29 /p38)
  (net 30 /p37)
  (net 31 /p36)
  (net 32 /p35)
  (net 33 /p34)
  (net 34 /p33)
  (net 35 /p32)
  (net 36 /P31)
  (net 37 /p30)
  (net 38 /p29)
  (net 39 /p28)
  (net 40 /p27)
  (net 41 /p26)
  (net 42 /p25)
  (net 43 /p24)
  (net 44 /p23)
  (net 45 /p22)
  (net 46 /p21)
  (net 47 "Net-(R4-Pad2)")
  (net 48 "Net-(U1-Pad86)")
  (net 49 "Net-(U1-Pad85)")
  (net 50 "Net-(U1-Pad84)")
  (net 51 "Net-(U1-Pad70)")
  (net 52 "Net-(U1-Pad69)")
  (net 53 "Net-(U1-Pad57)")
  (net 54 "Net-(U1-Pad58)")
  (net 55 "Net-(U1-Pad60)")
  (net 56 "Net-(U1-Pad48)")
  (net 57 "Net-(U1-Pad47)")
  (net 58 "Net-(U1-Pad46)")
  (net 59 "Net-(U1-Pad44)")
  (net 60 "Net-(U1-Pad43)")
  (net 61 "Net-(U1-Pad42)")
  (net 62 "Net-(U1-Pad53)")
  (net 63 "Net-(U1-Pad52)")
  (net 64 "Net-(U1-Pad51)")
  (net 65 "Net-(U1-Pad55)")
  (net 66 "Net-(U1-Pad56)")
  (net 67 "Net-(U1-Pad54)")
  (net 68 "Net-(U1-Pad50)")
  (net 69 "Net-(U1-Pad40)")
  (net 70 "Net-(U1-Pad37)")
  (net 71 "Net-(U1-Pad39)")
  (net 72 "Net-(U1-Pad38)")
  (net 73 "Net-(U1-Pad36)")
  (net 74 "Net-(U1-Pad34)")
  (net 75 "Net-(U1-Pad32)")
  (net 76 "Net-(U1-Pad30)")
  (net 77 "Net-(U1-Pad28)")
  (net 78 "Net-(U1-Pad27)")
  (net 79 "Net-(U1-Pad8)")
  (net 80 "Net-(U1-Pad4)")
  (net 81 "Net-(U1-Pad3)")
  (net 82 "Net-(U1-Pad2)")
  (net 83 "Net-(U1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /P10)
    (add_net /P11)
    (add_net /P12)
    (add_net /P31)
    (add_net /P9)
    (add_net /led1)
    (add_net /led2)
    (add_net /p1)
    (add_net /p13)
    (add_net /p14)
    (add_net /p15)
    (add_net /p16)
    (add_net /p17)
    (add_net /p18)
    (add_net /p19)
    (add_net /p2)
    (add_net /p20)
    (add_net /p21)
    (add_net /p22)
    (add_net /p23)
    (add_net /p24)
    (add_net /p25)
    (add_net /p26)
    (add_net /p27)
    (add_net /p28)
    (add_net /p29)
    (add_net /p3)
    (add_net /p30)
    (add_net /p32)
    (add_net /p33)
    (add_net /p34)
    (add_net /p35)
    (add_net /p36)
    (add_net /p37)
    (add_net /p38)
    (add_net /p39)
    (add_net /p4)
    (add_net /p40)
    (add_net /p5)
    (add_net /p6)
    (add_net /p7)
    (add_net /p8)
    (add_net /sw1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad57)")
    (add_net "Net-(U1-Pad58)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad69)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 153.2509 91.5797 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 1K (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(R4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 156.7561 86.7791 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.6002 2.3241) (layer F.SilkS))
    (fp_text value 430 (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 158.0134 91.5924 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 10K (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /sw1))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 87.8586 78.5622 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27) (layer F.Fab))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 87.884 111.7346 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27) (layer F.Fab))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Erics_Footprints:Arduino_MEGA_2560_Shield (layer F.Cu) (tedit 60864B4A)
    (at 68.7432 122.0414)
    (fp_text reference U1 (at 41.021 -31.496) (layer F.SilkS))
    (fp_text value Arduino_Mega_2560 (at 41.529 -33.528) (layer F.Fab))
    (fp_text user pin (at 5.842 -6.731) (layer Dwgs.User))
    (fp_text user "taller than" (at 5.969 -8.763) (layer Dwgs.User))
    (fp_text user "Power jack" (at 5.715 -10.668) (layer Dwgs.User))
    (fp_text user headers (at 6.096 -4.953) (layer Dwgs.User))
    (fp_text user headers (at 4.699 -35.306) (layer Dwgs.User))
    (fp_text user pin (at 4.445 -37.084) (layer Dwgs.User))
    (fp_text user "taller than" (at 4.572 -39.116) (layer Dwgs.User))
    (fp_text user USB (at 4.318 -41.021) (layer Dwgs.User))
    (pad 86 thru_hole circle (at 18.796 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad86)"))
    (pad 85 thru_hole circle (at 21.336 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad85)"))
    (pad 82 thru_hole circle (at 28.956 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /p40))
    (pad 84 thru_hole circle (at 23.876 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad84)"))
    (pad 79 thru_hole circle (at 36.576 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /p37))
    (pad 78 thru_hole circle (at 39.116 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /p36))
    (pad 80 thru_hole circle (at 34.036 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /p38))
    (pad 81 thru_hole circle (at 31.496 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /p39))
    (pad 77 thru_hole circle (at 41.656 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /p35))
    (pad 83 thru_hole circle (at 26.416 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 70 thru_hole circle (at 60.96 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad70)"))
    (pad 69 thru_hole circle (at 63.5 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad69)"))
    (pad 74 thru_hole circle (at 50.8 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /p32))
    (pad 73 thru_hole circle (at 53.34 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /P31))
    (pad 72 thru_hole circle (at 55.88 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /p30))
    (pad 71 thru_hole circle (at 58.42 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /p29))
    (pad 76 thru_hole circle (at 45.72 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /p34))
    (pad 75 thru_hole circle (at 48.26 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /p33))
    (pad 68 thru_hole circle (at 68.58 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /p28))
    (pad 67 thru_hole circle (at 71.12 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /p27))
    (pad 66 thru_hole circle (at 73.66 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /p26))
    (pad 65 thru_hole circle (at 76.2 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /p25))
    (pad 64 thru_hole circle (at 78.74 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /p24))
    (pad 63 thru_hole circle (at 81.28 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /p23))
    (pad 62 thru_hole circle (at 83.82 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /p22))
    (pad 61 thru_hole circle (at 86.36 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /p21))
    (pad 57 thru_hole circle (at 93.98 -48.26) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "Net-(U1-Pad57)"))
    (pad 59 thru_hole circle (at 93.98 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 58 thru_hole circle (at 96.52 -48.26) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "Net-(U1-Pad58)"))
    (pad 60 thru_hole circle (at 96.52 -50.8) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(U1-Pad60)"))
    (pad 48 thru_hole circle (at 96.52 -35.56) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(U1-Pad48)"))
    (pad 45 thru_hole circle (at 93.98 -33.02) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /led1))
    (pad 47 thru_hole circle (at 93.98 -35.56) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(U1-Pad47)"))
    (pad 46 thru_hole circle (at 96.52 -33.02) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(U1-Pad46)"))
    (pad 44 thru_hole circle (at 96.52 -30.48) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "Net-(U1-Pad44)"))
    (pad 43 thru_hole circle (at 93.98 -30.48) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "Net-(U1-Pad43)"))
    (pad 42 thru_hole circle (at 96.52 -27.94) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "Net-(U1-Pad42)"))
    (pad 41 thru_hole circle (at 93.98 -27.94) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /sw1))
    (pad 53 thru_hole circle (at 93.98 -43.18) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad53)"))
    (pad 52 thru_hole circle (at 96.52 -40.64) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad52)"))
    (pad 51 thru_hole circle (at 93.98 -40.64) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(U1-Pad51)"))
    (pad 49 thru_hole circle (at 93.98 -38.1) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /led2))
    (pad 55 thru_hole circle (at 93.98 -45.72) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(U1-Pad55)"))
    (pad 56 thru_hole circle (at 96.52 -45.72) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(U1-Pad56)"))
    (pad 54 thru_hole circle (at 96.52 -43.18) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "Net-(U1-Pad54)"))
    (pad 50 thru_hole circle (at 96.52 -38.1) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 "Net-(U1-Pad50)"))
    (pad 40 thru_hole circle (at 96.52 -25.4) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "Net-(U1-Pad40)"))
    (pad 37 thru_hole circle (at 93.98 -22.86) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(U1-Pad37)"))
    (pad 39 thru_hole circle (at 93.98 -25.4) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "Net-(U1-Pad39)"))
    (pad 38 thru_hole circle (at 96.52 -22.86) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "Net-(U1-Pad38)"))
    (pad 36 thru_hole circle (at 96.52 -20.32) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(U1-Pad36)"))
    (pad 35 thru_hole circle (at 93.98 -20.32) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /p20))
    (pad 34 thru_hole circle (at 96.52 -17.78) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "Net-(U1-Pad34)"))
    (pad 33 thru_hole circle (at 93.98 -17.78) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /p19))
    (pad 32 thru_hole circle (at 96.52 -15.24) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad32)"))
    (pad 31 thru_hole circle (at 93.98 -15.24) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /p18))
    (pad 30 thru_hole circle (at 96.52 -12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad30)"))
    (pad 29 thru_hole circle (at 93.98 -12.7) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /p17))
    (pad 28 thru_hole circle (at 96.52 -10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "Net-(U1-Pad28)"))
    (pad 27 thru_hole circle (at 93.98 -10.16) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "Net-(U1-Pad27)"))
    (pad 26 thru_hole circle (at 96.52 -7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 25 thru_hole circle (at 93.98 -7.62) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 91.44 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /p16))
    (pad 23 thru_hole circle (at 88.9 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /p15))
    (pad 22 thru_hole circle (at 86.36 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /p14))
    (pad 21 thru_hole circle (at 83.82 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /p13))
    (pad 20 thru_hole circle (at 81.28 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /P12))
    (pad 19 thru_hole circle (at 78.74 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /P11))
    (pad 18 thru_hole circle (at 76.2 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /P10))
    (pad 17 thru_hole circle (at 73.66 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /P9))
    (pad 16 thru_hole circle (at 68.58 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /p8))
    (pad 15 thru_hole circle (at 66.04 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /p7))
    (pad 14 thru_hole circle (at 63.5 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /p6))
    (pad 13 thru_hole circle (at 60.96 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /p5))
    (pad 12 thru_hole circle (at 58.42 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /p4))
    (pad 11 thru_hole circle (at 55.88 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /p3))
    (pad 10 thru_hole circle (at 53.34 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /p2))
    (pad 9 thru_hole circle (at 50.8 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /p1))
    (pad 8 thru_hole circle (at 45.72 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at 43.18 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 40.64 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 38.1 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 thru_hole circle (at 35.56 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 30.48 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "Net-(U1-Pad2)"))
    (pad 1 thru_hole circle (at 27.94 -2.54) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad1)"))
  )
  (module Erics_Footprints:SW_PUSH_6.5mm_H4.5mm (layer F.Cu) (tedit 6087A1A5)
    (at 153.2382 105.3338 90)
    (descr "tactile push button, 6.5mm x 4.5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 90) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 7 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(R4-Pad2)"))
    (pad 2 thru_hole circle (at 7 4.7 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 /sw1))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(R4-Pad2)"))
    (pad 2 thru_hole circle (at 0 4.7 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 /sw1))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 97.9551 80.2005 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x20 (at 0 50.59 90) (layer F.Fab))
    (fp_text user %R (at 0 24.13) (layer F.Fab))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /p21))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /p22))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /p23))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /p24))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /p25))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /p26))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /p27))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /p28))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /p29))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /p30))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /P31))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /p32))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /p33))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /p34))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /p35))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /p36))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /p37))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /p38))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /p39))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /p40))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Erics_Footprints:ZIF_240-3345_40pin (layer F.Cu) (tedit 60879BFE)
    (at 150.1902 104.8512 90)
    (fp_text reference J4 (at 11.0744 -63.1952 90) (layer F.SilkS))
    (fp_text value Conn_02x20_Counter_Clockwise (at 13.1064 -66.7512 90) (layer F.Fab))
    (pad 40 thru_hole circle (at 18.802 -55.26024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /p40))
    (pad 1 thru_hole circle (at 3.302 -55.26024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /p1))
    (pad 39 thru_hole circle (at 18.802 -52.72024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /p39))
    (pad 2 thru_hole circle (at 3.302 -52.72024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /p2))
    (pad 38 thru_hole circle (at 18.802 -50.18024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /p38))
    (pad 3 thru_hole circle (at 3.302 -50.18024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /p3))
    (pad 37 thru_hole circle (at 18.802 -47.64024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /p37))
    (pad 4 thru_hole circle (at 3.302 -47.64024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /p4))
    (pad 36 thru_hole circle (at 18.802 -45.10024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /p36))
    (pad 5 thru_hole circle (at 3.302 -45.10024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /p5))
    (pad 35 thru_hole circle (at 18.802 -42.56024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /p35))
    (pad 6 thru_hole circle (at 3.302 -42.56024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /p6))
    (pad 34 thru_hole circle (at 18.802 -40.02024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /p34))
    (pad 7 thru_hole circle (at 3.302 -40.02024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /p7))
    (pad 33 thru_hole circle (at 18.802 -37.48024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /p33))
    (pad 8 thru_hole circle (at 3.302 -37.48024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /p8))
    (pad 32 thru_hole circle (at 18.802 -34.94024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /p32))
    (pad 9 thru_hole circle (at 3.302 -34.94024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /P9))
    (pad 31 thru_hole circle (at 18.802 -32.40024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /P31))
    (pad 10 thru_hole circle (at 3.302 -32.40024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 /P10))
    (pad 30 thru_hole circle (at 18.802 -29.86024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /p30))
    (pad 11 thru_hole circle (at 3.302 -29.86024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /P11))
    (pad 29 thru_hole circle (at 18.802 -27.32024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 /p29))
    (pad 12 thru_hole circle (at 3.302 -27.32024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 /P12))
    (pad 28 thru_hole circle (at 18.802 -24.78024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 /p28))
    (pad 13 thru_hole circle (at 3.302 -24.78024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /p13))
    (pad 27 thru_hole circle (at 18.802 -22.24024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 /p27))
    (pad 14 thru_hole circle (at 3.302 -22.24024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /p14))
    (pad 26 thru_hole circle (at 18.802 -19.70024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /p26))
    (pad 15 thru_hole circle (at 3.302 -19.70024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /p15))
    (pad 25 thru_hole circle (at 18.802 -17.16024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /p25))
    (pad 16 thru_hole circle (at 3.302 -17.16024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /p16))
    (pad 24 thru_hole circle (at 18.802 -14.62024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /p24))
    (pad 17 thru_hole circle (at 3.302 -14.62024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /p17))
    (pad 23 thru_hole circle (at 18.802 -12.08024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 /p23))
    (pad 18 thru_hole circle (at 3.302 -12.08024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /p18))
    (pad 22 thru_hole circle (at 18.802 -9.54024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 /p22))
    (pad 19 thru_hole circle (at 3.302 -9.54024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /p19))
    (pad 21 thru_hole circle (at 18.802 -7.00024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /p21))
    (pad 20 thru_hole circle (at 3.302 -7.00024 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /p20))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 97.9424 108.3564 90)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x20 (at 0 50.59 90) (layer F.Fab))
    (fp_text user %R (at 0 24.13) (layer F.Fab))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /p20))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /p19))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /p18))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /p17))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /p16))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /p15))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /p14))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /p13))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /P12))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /P11))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P10))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P9))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /p8))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /p7))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /p6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /p5))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /p4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /p3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /p2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /p1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 154.3558 80.2132)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /led1))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 157.9607 111.9378 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.55) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.55) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /sw1))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 88.7095 116.3828)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C2 (at 1.1938 2.3622) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.55) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 95.6818 113.284 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (fp_text reference C1 (at 1.1811 -2.3114 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 2.55 90) (layer F.Fab))
    (fp_text user %R (at 1.4332 0.1524 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 53.4162 (width 0.15) (layer Dwgs.User)
    (gr_text "2.1030 in" (at 172.8897 95.3643 270) (layer Dwgs.User))
    (feature1 (pts (xy 168.4274 122.0724) (xy 172.176121 122.0724)))
    (feature2 (pts (xy 168.4274 68.6562) (xy 172.176121 68.6562)))
    (crossbar (pts (xy 171.5897 68.6562) (xy 171.5897 122.0724)))
    (arrow1a (pts (xy 171.5897 122.0724) (xy 171.003279 120.945896)))
    (arrow1b (pts (xy 171.5897 122.0724) (xy 172.176121 120.945896)))
    (arrow2a (pts (xy 171.5897 68.6562) (xy 171.003279 69.782704)))
    (arrow2b (pts (xy 171.5897 68.6562) (xy 172.176121 69.782704)))
  )
  (dimension 85.217 (width 0.15) (layer Dwgs.User)
    (gr_text "3.3550 in" (at 125.2982 127.9063) (layer Dwgs.User))
    (feature1 (pts (xy 167.9067 122.5423) (xy 167.9067 127.192721)))
    (feature2 (pts (xy 82.6897 122.5423) (xy 82.6897 127.192721)))
    (crossbar (pts (xy 82.6897 126.6063) (xy 167.9067 126.6063)))
    (arrow1a (pts (xy 167.9067 126.6063) (xy 166.780196 127.192721)))
    (arrow1b (pts (xy 167.9067 126.6063) (xy 166.780196 126.019879)))
    (arrow2a (pts (xy 82.6897 126.6063) (xy 83.816204 127.192721)))
    (arrow2b (pts (xy 82.6897 126.6063) (xy 83.816204 126.019879)))
  )
  (gr_text GND (at 93.2942 77.2922 90) (layer F.SilkS))
  (gr_text +5V (at 93.345 110.8837 90) (layer F.SilkS))
  (gr_text "Rev. 1 (04/29/2021)" (at 122.6058 115.6843) (layer F.SilkS))
  (gr_text "Eric Ljungquist" (at 105.9307 115.6843) (layer F.SilkS))
  (gr_text "ZIF Socket Shield for MEGA 2560" (at 115.4684 113.6523) (layer F.SilkS))
  (gr_text 21 (at 146.2278 76.4794 90) (layer F.SilkS))
  (gr_text 22 (at 143.6878 76.4794 90) (layer F.SilkS))
  (gr_text 23 (at 141.1478 76.4794 90) (layer F.SilkS))
  (gr_text 24 (at 138.6078 76.4794 90) (layer F.SilkS))
  (gr_text 25|17 (at 136.0678 76.2 90) (layer F.SilkS))
  (gr_text 26|18 (at 133.5151 76.2127 90) (layer F.SilkS))
  (gr_text 27|19|15 (at 130.9878 78.6638 90) (layer F.SilkS))
  (gr_text 28|20|16 (at 128.4478 78.6638 90) (layer F.SilkS))
  (gr_text 29|21|17 (at 125.9078 78.6638 90) (layer F.SilkS))
  (gr_text 30|22|18 (at 123.3678 78.6638 90) (layer F.SilkS))
  (gr_text 31|23|19 (at 120.8278 78.6638 90) (layer F.SilkS))
  (gr_text 32|24|20 (at 118.2878 78.6638 90) (layer F.SilkS))
  (gr_text 33|25|21 (at 115.7478 78.6638 90) (layer F.SilkS))
  (gr_text 34|26|22 (at 113.2078 78.6638 90) (layer F.SilkS))
  (gr_text 35|27|23 (at 110.6678 78.6638 90) (layer F.SilkS))
  (gr_text 36|28|24 (at 108.1278 78.6638 90) (layer F.SilkS))
  (gr_text 37|29|25 (at 105.5878 78.6638 90) (layer F.SilkS))
  (gr_text 38|30|26 (at 103.0478 78.6638 90) (layer F.SilkS))
  (gr_text 39|31|27 (at 100.5078 78.6638 90) (layer F.SilkS))
  (gr_text 20 (at 146.2024 111.4044 90) (layer F.SilkS))
  (gr_text 19 (at 143.6624 111.4044 90) (layer F.SilkS))
  (gr_text 18 (at 141.1224 111.4044 90) (layer F.SilkS))
  (gr_text 17 (at 138.5824 111.4044 90) (layer F.SilkS))
  (gr_text 16 (at 136.0424 111.4044 90) (layer F.SilkS))
  (gr_text 15 (at 133.5024 111.4044 90) (layer F.SilkS))
  (gr_text 14 (at 130.9624 111.4044 90) (layer F.SilkS))
  (gr_text 13 (at 128.4224 111.4044 90) (layer F.SilkS))
  (gr_text 12 (at 125.8824 111.4044 90) (layer F.SilkS))
  (gr_text 11 (at 123.3424 111.4044 90) (layer F.SilkS))
  (gr_text 10 (at 120.8024 111.4044 90) (layer F.SilkS))
  (gr_text 9 (at 118.2624 111.4044 90) (layer F.SilkS))
  (gr_text 8 (at 115.7224 111.4044 90) (layer F.SilkS))
  (gr_text 7 (at 113.1824 111.4044 90) (layer F.SilkS))
  (gr_text 6 (at 110.6424 111.4044 90) (layer F.SilkS))
  (gr_text 5 (at 108.1024 111.4044 90) (layer F.SilkS))
  (gr_text 4 (at 105.5624 111.4044 90) (layer F.SilkS))
  (gr_text 3 (at 103.0224 111.4044 90) (layer F.SilkS))
  (gr_text 2 (at 100.4824 111.4044 90) (layer F.SilkS))
  (gr_line (start 167.8051 122.047) (end 167.8051 122.0343) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.7024 122.047) (end 167.8051 122.047) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.8051 68.707) (end 167.8051 122.0343) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.7024 68.707) (end 167.8051 68.707) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.7024 122.047) (end 82.7024 68.707) (layer Edge.Cuts) (width 0.05))
  (gr_text 40|32|28 (at 97.9678 78.6638 90) (layer F.SilkS))
  (gr_text 1 (at 97.9424 111.4044 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.8051 122.0343) (xy 82.6897 122.0343) (xy 82.6897 68.707) (xy 167.8051 68.707)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.635))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.7543 122.050872) (xy 82.6389 122.050872) (xy 82.6389 68.723572) (xy 167.7543 68.723572)
      )
    )
  )
)
