(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 20)
    (zones 0)
    (modules 25)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.2032)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 1.016 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.101)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad7)")
  (net 2 "Net-(U1-Pad8)")
  (net 3 "Net-(U1-Pad11)")
  (net 4 /-Vin)
  (net 5 /+Vin)
  (net 6 Earth)
  (net 7 /+V)
  (net 8 /-V)
  (net 9 "Net-(C9-Pad1)")
  (net 10 /SG)
  (net 11 /CNT)
  (net 12 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.3048)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /+V)
    (add_net /+Vin)
    (add_net /-V)
    (add_net /-Vin)
    (add_net /CNT)
    (add_net /SG)
    (add_net Earth)
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 34.4 -20.4)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -46 18)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 11 /CNT))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -46 7)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 10 /SG))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -23 -18)
    (fp_text reference J13 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 4 /-Vin))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -16 18)
    (fp_text reference J12 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 5 /+Vin))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 20 -18)
    (fp_text reference J11 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 8 /-V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 10 18)
    (fp_text reference J10 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 7 /+V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 9 -18)
    (fp_text reference J9 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 8 /-V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 32 18)
    (fp_text reference J8 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 7 /+V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -2 -18)
    (fp_text reference J7 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 8 /-V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at 21 18)
    (fp_text reference J6 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 7 /+V))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -34 -18)
    (fp_text reference J5 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 4 /-Vin))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:WP_SMBU_M4 (layer F.Cu) (tedit 5EF0DE05)
    (at -27 18)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.5 8.5) (drill 5.2) (layers *.Cu F.Mask)
      (net 5 /+Vin))
    (model "C:/Users/staffeld/Documents/kicad/kicadLibrary/Download_STP_7466004R (rev1).stp"
      (offset (xyz 0 0 -1.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (module myFootprints:PV36X_trim (layer F.Cu) (tedit 5EED39B8)
    (at 44.5 -18.5)
    (fp_text reference VR1 (at 0 0.5) (layer F.SilkS))
    (fp_text value 10k (at 0 -0.5) (layer F.Fab))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 /+V))
    (pad 1 thru_hole circle (at -2.5 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad11)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 /+V))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 47.5 -23 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value 43k (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /-V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 28 -23 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 2.5 -2.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 30.5 3.75 90)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C8 (at 3.75 -9.25 90) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 9.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /+V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 10 3.75 90)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C7 (at 3.75 -9.25 90) (layer F.SilkS))
    (fp_text value 1000uF (at 3.75 9.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /+V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 46.5 0)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C6 (at 1.25 -3.75) (layer F.SilkS))
    (fp_text value 2.2uF (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /+V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 44 -5)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C5 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value 0.022uF (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 49 5 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -2.5) (layer F.SilkS))
    (fp_text value 0.022uF (at 2.5 2.5) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /+V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.5mm_W5.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at -46 -21 270)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C3 (at 3.75 -3.75 90) (layer F.SilkS))
    (fp_text value 330pF (at 3.75 3.75 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 /-Vin))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 Earth))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D7.5mm_W5.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at -46 -1 90)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=7.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 7.5mm width 5.0mm Capacitor")
    (fp_text reference C2 (at 3.75 -3.75 90) (layer F.SilkS))
    (fp_text value 330pF (at 3.75 3.75 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /+Vin))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W5.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D16.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at -31 4 90)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=16mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 16mm Electrolytic Capacitor")
    (fp_text reference C1 (at 3.75 -9.25 90) (layer F.SilkS))
    (fp_text value 22uF (at 3.75 9.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /-Vin))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /+Vin))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootprints:PAF600F280 (layer F.Cu) (tedit 5EED04C6)
    (at 0 0)
    (fp_text reference U1 (at 0 0.5) (layer F.SilkS))
    (fp_text value PAF600F280 (at 0 -0.5) (layer F.Fab))
    (pad G thru_hole circle (at -53.35 -25.4) (size 6.8 6.8) (drill 3.4) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad G thru_hole circle (at -53.35 25.4) (size 6.8 6.8) (drill 3.4) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad G thru_hole circle (at 53.35 25.4) (size 6.8 6.8) (drill 3.4) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad G thru_hole circle (at 53.35 -25.4) (size 6.8 6.8) (drill 3.4) (layers *.Cu *.Mask)
      (net 6 Earth))
    (pad 7 thru_hole circle (at 26.7 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 30.51 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 34.32 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 10 thru_hole circle (at 38.13 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 11 thru_hole circle (at 41.94 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 45.75 -26.67) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 6 thru_hole circle (at 53.35 17.78) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 7 /+V))
    (pad 6 thru_hole circle (at 53.35 11.43) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 7 /+V))
    (pad 6 thru_hole circle (at 53.35 5.08) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 7 /+V))
    (pad 5 thru_hole circle (at 53.33 -5.08) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 5 thru_hole circle (at 53.35 -11.43) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 5 thru_hole circle (at 53.35 -17.78) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 8 /-V))
    (pad 4 thru_hole circle (at -53.35 11.43) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /CNT))
    (pad 3 thru_hole circle (at -53.35 7.62) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /SG))
    (pad 2 thru_hole circle (at -53.35 -2.54) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 5 /+Vin))
    (pad 1 thru_hole circle (at -53.35 -12.7) (size 4.2 4.2) (drill 2.1) (layers *.Cu *.Mask)
      (net 4 /-Vin))
    (model "D:/Repository/hunter/050. hardware information/TDK/paf-f_out_step/paf-f_outline.STEP"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 180))
    )
  )
  (gr_text CES (at 43.8 -20.75) (layer B.SilkS))
  (gr_text PC (at 34.5 -13.5) (layer F.SilkS))
  (gr_text CNT (at -38 21.5) (layer F.SilkS))
  (gr_text SG (at -38.5 10.5) (layer F.SilkS))
  (gr_text +V (at 18 26.5) (layer F.SilkS))
  (gr_text -V (at 6 -26.5) (layer F.SilkS))
  (gr_text "+Vin\n" (at -22.5 26) (layer F.SilkS))
  (gr_text -Vin (at -31.5 -26.5) (layer F.SilkS))
  (gr_line (start -58.4 30.5) (end 58.4 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -58.4 -30.5) (end -58.4 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.4 -30.5) (end -58.4 -30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 58.4 30.5) (end 58.4 -30.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 58.4 30.5) (xy -58.4 30.4) (xy -58.4 -30.5) (xy 58.4 -30.4)
      )
    )
  )
  (zone (net 8) (net_name /-V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 58.5 -0.5) (xy -10 -0.5) (xy -10 -30.5) (xy 58.5 -30.5)
      )
    )
  )
  (zone (net 7) (net_name /+V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 58.5 30.5) (xy 0 30.5) (xy 0 0.5) (xy 58.5 0.5)
      )
    )
  )
  (zone (net 5) (net_name /+Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy -35.5 0.5) (xy -1 0.5) (xy -1 30.5) (xy -58.5 30.5) (xy -58.5 -7)
        (xy -35.5 -7)
      )
    )
  )
  (zone (net 4) (net_name /-Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy -11 -0.5) (xy -34.5 -0.5) (xy -34.5 -8) (xy -58.5 -8) (xy -58.5 -30.5)
        (xy -11 -30.5)
      )
    )
  )
)
