<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="64.77" width="0.4064" layer="20"/>
<wire x1="0" y1="64.77" x2="93.98" y2="64.77" width="0.4064" layer="20"/>
<wire x1="93.98" y1="64.77" x2="93.98" y2="11.43" width="0.4064" layer="20"/>
<wire x1="93.98" y1="11.43" x2="82.55" y2="0" width="0.4064" layer="20"/>
<wire x1="82.55" y1="0" x2="0" y2="0" width="0.4064" layer="20"/>
<text>SCL
5v
GND</text>
<text>SDA
5V
GND</text>
<text>JACKSONVILLE STATE ROBOTICS TEAM</text>
<text>TWIZ
TECH</text>
<text>TWIZ
TECH</text>
<text>RJ45 BREAKOUT 
BOARD 2016</text>
<text>TWIZ
TECH</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X16">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Aaron Spark Fun Edit">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B25V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Beckman Helitrim 25</description>
</package>
</packages>
</library>
<library name="Aaron Arduino Edit">
<packages>
<package name="ARDUINO_MEGA2560">
<description>Footprint for representing an Arduino Mega board in an EAGLE schematic. Created by Dave Young for Element14. More EAGLE documentation at: http://www.element14.com/community/community/knode/cadsoft_eagle</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCB1" library="Aaron Arduino Edit" package="ARDUINO_MEGA2560" value="ARDUINO_MEGA2560"/>
<element name="DRIVE_RIGHT" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="DRIVE_LEFT" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="AUX1/ARM" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="AUX2/GRIP" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="AR7000" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="AUX3" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="AUX4" library="Aaron Spark Fun Edit" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD" library="pinhead" package="1X16" value=""/>
<element name="LINE" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POT1" library="pot" package="B25V" value="10K"/>
</elements>
<signals>
<signal name="DIR_DRIVE_LEFT">
<contactref element="DRIVE_LEFT" pad="2"/>
<contactref element="PCB1" pad="26"/>
</signal>
<signal name="ELEV">
<contactref element="PCB1" pad="48"/>
<contactref element="AR7000" pad="3"/>
</signal>
<signal name="PWM_DRIVE_RIGHT">
<contactref element="DRIVE_RIGHT" pad="3"/>
<contactref element="PCB1" pad="5"/>
</signal>
<signal name="FF2_DRIVE_LEFT">
<contactref element="DRIVE_LEFT" pad="6"/>
<contactref element="PCB1" pad="28"/>
</signal>
<signal name="FF2_AUX2_GRIP">
<contactref element="AUX2/GRIP" pad="6"/>
<contactref element="PCB1" pad="36"/>
</signal>
<signal name="RESET'">
<contactref element="DRIVE_RIGHT" pad="4"/>
<contactref element="DRIVE_LEFT" pad="4"/>
<contactref element="AUX2/GRIP" pad="4"/>
<contactref element="AUX1/ARM" pad="4"/>
<contactref element="AUX3" pad="4"/>
<contactref element="AUX4" pad="4"/>
<contactref element="PCB1" pad="RESET"/>
</signal>
<signal name="FF2_AUX3">
<contactref element="AUX3" pad="6"/>
<contactref element="PCB1" pad="40"/>
</signal>
<signal name="FF2">
<contactref element="AUX4" pad="6"/>
<contactref element="PCB1" pad="44"/>
</signal>
<signal name="FF1_AUX4">
<contactref element="AUX4" pad="5"/>
<contactref element="PCB1" pad="43"/>
</signal>
<signal name="THRO">
<contactref element="PCB1" pad="46"/>
<contactref element="AR7000" pad="1"/>
</signal>
<signal name="DIR_AUX4">
<contactref element="AUX4" pad="2"/>
<contactref element="PCB1" pad="42"/>
</signal>
<signal name="AILE">
<contactref element="AR7000" pad="2"/>
<contactref element="PCB1" pad="47"/>
</signal>
<signal name="N$16">
<contactref element="AUX4" pad="7"/>
<contactref element="PCB1" pad="45"/>
</signal>
<signal name="5V_AUX2_GRIP">
<contactref element="AUX2/GRIP" pad="7"/>
<contactref element="PCB1" pad="37"/>
</signal>
<signal name="FF1_AUX2_GRIP">
<contactref element="AUX2/GRIP" pad="5"/>
<contactref element="PCB1" pad="35"/>
</signal>
<signal name="DIR_AUX2_GRIP">
<contactref element="AUX2/GRIP" pad="2"/>
<contactref element="PCB1" pad="34"/>
</signal>
<signal name="5V_AUX_ARM">
<contactref element="AUX1/ARM" pad="7"/>
<contactref element="PCB1" pad="33"/>
</signal>
<signal name="DIR_AUX_ARM">
<contactref element="AUX1/ARM" pad="2"/>
<contactref element="PCB1" pad="30"/>
</signal>
<signal name="FF1_DRIVE_LEFT">
<contactref element="DRIVE_LEFT" pad="5"/>
<contactref element="PCB1" pad="27"/>
</signal>
<signal name="5V_DRIVE_RIGHT">
<contactref element="DRIVE_RIGHT" pad="7"/>
<contactref element="PCB1" pad="25"/>
</signal>
<signal name="FF2_DRIVE_RIGHT">
<contactref element="DRIVE_RIGHT" pad="6"/>
<contactref element="PCB1" pad="24"/>
</signal>
<signal name="FF1_DRIVE_RIGHT">
<contactref element="DRIVE_RIGHT" pad="5"/>
<contactref element="PCB1" pad="23"/>
</signal>
<signal name="5V_DRIVE_LEFT">
<contactref element="DRIVE_LEFT" pad="7"/>
<contactref element="PCB1" pad="29"/>
</signal>
<signal name="FF1_AUX_ARM">
<contactref element="AUX1/ARM" pad="5"/>
<contactref element="PCB1" pad="31"/>
</signal>
<signal name="FF2_AUX_ARM">
<contactref element="PCB1" pad="32"/>
<contactref element="AUX1/ARM" pad="6"/>
</signal>
<signal name="PWM_AUX4">
<contactref element="AUX4" pad="3"/>
<contactref element="PCB1" pad="0"/>
</signal>
<signal name="PWM_AUX3">
<contactref element="PCB1" pad="1"/>
<contactref element="AUX3" pad="3"/>
</signal>
<signal name="PWM_AUX2_GRIP">
<contactref element="PCB1" pad="2"/>
<contactref element="AUX2/GRIP" pad="3"/>
</signal>
<signal name="PWM_DRIVE_LEFT">
<contactref element="DRIVE_LEFT" pad="3"/>
<contactref element="PCB1" pad="4"/>
</signal>
<signal name="H/L_ENABLE">
<contactref element="PCB1" pad="A1"/>
<contactref element="LCD" pad="6"/>
</signal>
<signal name="LCD4">
<contactref element="PCB1" pad="A5"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="LCD3">
<contactref element="LCD" pad="13"/>
<contactref element="PCB1" pad="A4"/>
</signal>
<signal name="LCD2">
<contactref element="LCD" pad="12"/>
<contactref element="PCB1" pad="A3"/>
</signal>
<signal name="LCD1">
<contactref element="LCD" pad="11"/>
<contactref element="PCB1" pad="A2"/>
</signal>
<signal name="PWM_AUX_ARM">
<contactref element="AUX1/ARM" pad="3"/>
<contactref element="PCB1" pad="3"/>
</signal>
<signal name="DIR_DRIVE_RIGHT">
<contactref element="PCB1" pad="22"/>
<contactref element="DRIVE_RIGHT" pad="2"/>
</signal>
<signal name="DIR_AUX3">
<contactref element="AUX3" pad="2"/>
<contactref element="PCB1" pad="38"/>
</signal>
<signal name="FF1_AUX3">
<contactref element="AUX3" pad="5"/>
<contactref element="PCB1" pad="39"/>
</signal>
<signal name="5V_AUX3">
<contactref element="AUX3" pad="7"/>
<contactref element="PCB1" pad="41"/>
</signal>
<signal name="AUX1">
<contactref element="AR7000" pad="6"/>
<contactref element="PCB1" pad="51"/>
</signal>
<signal name="RUDD">
<contactref element="AR7000" pad="4"/>
<contactref element="PCB1" pad="49"/>
</signal>
<signal name="GEAR">
<contactref element="PCB1" pad="50"/>
<contactref element="AR7000" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="LINE" pad="1"/>
<contactref element="PCB1" pad="20"/>
</signal>
<signal name="SCL">
<contactref element="LINE" pad="2"/>
<contactref element="PCB1" pad="21"/>
</signal>
<signal name="5V">
<contactref element="LINE" pad="3"/>
<contactref element="LINE" pad="4"/>
<contactref element="AR7000" pad="7"/>
<contactref element="PCB1" pad="5V"/>
<contactref element="LCD" pad="15"/>
<contactref element="POT1" pad="E"/>
<contactref element="LCD" pad="2"/>
</signal>
<signal name="REG_SELECT">
<contactref element="PCB1" pad="A0"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="CONTRAST">
<contactref element="POT1" pad="S"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="GND">
<contactref element="POT1" pad="A"/>
<contactref element="AUX1/ARM" pad="1"/>
<contactref element="DRIVE_LEFT" pad="1"/>
<contactref element="DRIVE_RIGHT" pad="1"/>
<contactref element="AUX2/GRIP" pad="1"/>
<contactref element="AUX3" pad="1"/>
<contactref element="AUX4" pad="1"/>
<contactref element="LCD" pad="16"/>
<contactref element="LCD" pad="1"/>
<contactref element="LCD" pad="5"/>
<contactref element="PCB1" pad="GND.."/>
<contactref element="AR7000" pad="8"/>
<contactref element="AR7000" pad="P$1"/>
<contactref element="AR7000" pad="P$2"/>
<contactref element="LINE" pad="6"/>
<contactref element="LINE" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
