(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 175)
    (zones 0)
    (modules 19)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 206 114.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad19)")
  (net 3 "Net-(J1-Pad17)")
  (net 4 "Net-(J1-Pad15)")
  (net 5 /ARM_TDO)
  (net 6 /ARM_RTCK)
  (net 7 /ARM_TCK)
  (net 8 /ARM_TMS)
  (net 9 /ARM_TDI)
  (net 10 /ARM_TRST)
  (net 11 "Net-(J1-Pad2)")
  (net 12 +3V3)
  (net 13 /RX)
  (net 14 /TX)
  (net 15 "Net-(J3-Pad12)")
  (net 16 /SCL)
  (net 17 /SDA)
  (net 18 +5V)
  (net 19 "Net-(J2-Pad6)")
  (net 20 "Net-(J2-Pad3)")
  (net 21 "Net-(J2-Pad2)")
  (net 22 "Net-(J3-Pad37)")
  (net 23 "Net-(J3-Pad34)")
  (net 24 "Net-(J3-Pad30)")
  (net 25 "Net-(J3-Pad22)")
  (net 26 "Net-(J3-Pad20)")
  (net 27 "Net-(J3-Pad18)")
  (net 28 "Net-(J3-Pad17)")
  (net 29 "Net-(J3-Pad15)")
  (net 30 "Net-(J3-Pad14)")
  (net 31 "Net-(J3-Pad13)")
  (net 32 "Net-(J3-Pad10)")
  (net 33 "Net-(J3-Pad9)")
  (net 34 "Net-(J3-Pad8)")
  (net 35 "Net-(J3-Pad5)")
  (net 36 /GPIO18)
  (net 37 /GPIO19)
  (net 38 /GPIO20)
  (net 39 /GPIO21)
  (net 40 "Net-(D1-Pad1)")
  (net 41 "Net-(D2-Pad1)")
  (net 42 "Net-(D3-Pad1)")
  (net 43 "Net-(D4-Pad1)")
  (net 44 "Net-(J6-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ARM_RTCK)
    (add_net /ARM_TCK)
    (add_net /ARM_TDI)
    (add_net /ARM_TDO)
    (add_net /ARM_TMS)
    (add_net /ARM_TRST)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad17)")
    (add_net "Net-(J3-Pad18)")
    (add_net "Net-(J3-Pad20)")
    (add_net "Net-(J3-Pad22)")
    (add_net "Net-(J3-Pad30)")
    (add_net "Net-(J3-Pad34)")
    (add_net "Net-(J3-Pad37)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J6-Pad7)")
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 190.76 85.925)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 614A2817)
    (at 206 114.5)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 0 26.9) (layer B.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at 0 -26.9) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 40 thru_hole oval (at -1.27 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 39 thru_hole oval (at 1.27 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 38 thru_hole oval (at -1.27 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SDA))
    (pad 37 thru_hole oval (at 1.27 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad37)"))
    (pad 36 thru_hole oval (at -1.27 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SCL))
    (pad 35 thru_hole oval (at 1.27 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 34 thru_hole oval (at -1.27 -16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad34)"))
    (pad 33 thru_hole oval (at 1.27 -16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /TX))
    (pad 32 thru_hole oval (at -1.27 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 1.27 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RX))
    (pad 30 thru_hole oval (at -1.27 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad30)"))
    (pad 29 thru_hole oval (at 1.27 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /GPIO18))
    (pad 28 thru_hole oval (at -1.27 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ARM_TMS))
    (pad 27 thru_hole oval (at 1.27 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at -1.27 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ARM_TRST))
    (pad 25 thru_hole oval (at 1.27 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ARM_RTCK))
    (pad 24 thru_hole oval (at -1.27 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 23 thru_hole oval (at 1.27 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ARM_TDO))
    (pad 22 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad22)"))
    (pad 21 thru_hole oval (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad20)"))
    (pad 19 thru_hole oval (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /ARM_TCK))
    (pad 18 thru_hole oval (at -1.27 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad18)"))
    (pad 17 thru_hole oval (at 1.27 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad17)"))
    (pad 16 thru_hole oval (at -1.27 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 1.27 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad15)"))
    (pad 14 thru_hole oval (at -1.27 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad14)"))
    (pad 13 thru_hole oval (at 1.27 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad13)"))
    (pad 12 thru_hole oval (at -1.27 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J3-Pad12)"))
    (pad 11 thru_hole oval (at 1.27 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at -1.27 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad10)"))
    (pad 9 thru_hole oval (at 1.27 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad9)"))
    (pad 8 thru_hole oval (at -1.27 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 1.27 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -1.27 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GPIO19))
    (pad 5 thru_hole oval (at 1.27 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at -1.27 21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ARM_TDI))
    (pad 3 thru_hole oval (at 1.27 21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /GPIO20))
    (pad 2 thru_hole oval (at -1.27 24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 1.27 24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /GPIO21))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (offset (xyz 1.27 24.13 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 5EAC9A07)
    (at 198.5 125.93 180)
    (descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 -6.1) (layer F.SilkS) hide)
    (fp_text value Conn_ARM_JTAG_SWD_20 (at 1.27 28.96) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 20 thru_hole circle (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 19 thru_hole circle (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad19)"))
    (pad 17 thru_hole circle (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad17)"))
    (pad 15 thru_hole circle (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad15)"))
    (pad 13 thru_hole circle (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ARM_TDO))
    (pad 11 thru_hole circle (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /ARM_RTCK))
    (pad 9 thru_hole circle (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /ARM_TCK))
    (pad 7 thru_hole circle (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ARM_TMS))
    (pad 5 thru_hole circle (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ARM_TDI))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ARM_TRST))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 183.5 143.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 183.5 85.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 187.5 129 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37 90) (layer F.SilkS) hide)
    (fp_text value R_Small (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 190.5 129 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37 90) (layer F.SilkS) hide)
    (fp_text value R_Small (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 184.5 129 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37 90) (layer F.SilkS) hide)
    (fp_text value R_Small (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 181.5 129 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37 90) (layer F.SilkS) hide)
    (fp_text value R_Small (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 186 111 180)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J6 (at 0 -4.235) (layer F.SilkS) hide)
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0 4.235) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 10 smd rect (at 1.95 2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 10 /ARM_TRST))
    (pad 9 smd rect (at -1.95 2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.95 1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 9 /ARM_TDI))
    (pad 7 smd rect (at -1.95 1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J6-Pad7)"))
    (pad 6 smd rect (at 1.95 0 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 /ARM_TDO))
    (pad 5 smd rect (at -1.95 0 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.95 -1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 /ARM_TCK))
    (pad 3 smd rect (at -1.95 -1.27 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.95 -2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 /ARM_TMS))
    (pad 1 smd rect (at -1.95 -2.54 180) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 201 140 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 /GPIO21))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 198 135.5 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 /GPIO20))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 195 140 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 /GPIO19))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 192 135.5 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96) (layer F.SilkS) hide)
    (fp_text value LED_Small (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 /GPIO18))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 200.158 145.742 270)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 4.385 -2.27 270) (layer F.SilkS))
    (fp_text value Conn_01x05_Male (at 4.385 12.43 270) (layer F.Fab))
    (fp_text user %R (at 2.77 5.08 180) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /GPIO18))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GPIO19))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /GPIO20))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /GPIO21))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 198.5 85.5 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J4 (at 0 -3.98) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 3.98) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /SCL))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /SDA))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 206 85.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 206 143.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 181.5 102.5 180)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 4.385 -2.27) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /TX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /RX))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "In config.txt:\nenable_jtag_gpio = 1\ngpio=22-27=np" (at 187.8136 104.4924 270) (layer B.SilkS))
  (gr_text ckd.tech/pi-developer/v1 (at 193.1095 114.5635 270) (layer B.SilkS))
  (gr_text "LED Resistors\n(1k)" (at 186 131.5) (layer F.SilkS))
  (gr_text "3mm LEDs" (at 187.0135 139.3285) (layer F.SilkS))
  (gr_text "\"SWD\"" (at 186 106.5) (layer F.SilkS))
  (gr_text JTAG (at 197 95.831) (layer F.SilkS))
  (gr_text "Stemma QT" (at 196.856 89.4175) (layer F.SilkS))
  (gr_text GND (at 184.5 102.5) (layer F.SilkS))
  (gr_text RX (at 184.5 95) (layer F.SilkS))
  (gr_text TX (at 184.5 92.5) (layer F.SilkS))
  (gr_text UART (at 187.1405 96.212 -90) (layer F.SilkS))
  (gr_text GND (at 200.158 143.202) (layer F.SilkS))
  (dimension 29 (width 0.05) (layer F.CrtYd)
    (gr_text "29.000 mm" (at 232.2 100 270) (layer F.CrtYd))
    (feature1 (pts (xy 206 114.5) (xy 231.586421 114.5)))
    (feature2 (pts (xy 206 85.5) (xy 231.586421 85.5)))
    (crossbar (pts (xy 231 85.5) (xy 231 114.5)))
    (arrow1a (pts (xy 231 114.5) (xy 230.413579 113.373496)))
    (arrow1b (pts (xy 231 114.5) (xy 231.586421 113.373496)))
    (arrow2a (pts (xy 231 85.5) (xy 230.413579 86.626504)))
    (arrow2b (pts (xy 231 85.5) (xy 231.586421 86.626504)))
  )
  (dimension 65 (width 0.05) (layer F.CrtYd)
    (gr_text "65.000 mm" (at 224.2 114.5 90) (layer F.CrtYd))
    (feature1 (pts (xy 210 82) (xy 223.586421 82)))
    (feature2 (pts (xy 210 147) (xy 223.586421 147)))
    (crossbar (pts (xy 223 147) (xy 223 82)))
    (arrow1a (pts (xy 223 82) (xy 223.586421 83.126504)))
    (arrow1b (pts (xy 223 82) (xy 222.413579 83.126504)))
    (arrow2a (pts (xy 223 147) (xy 223.586421 145.873496)))
    (arrow2b (pts (xy 223 147) (xy 222.413579 145.873496)))
  )
  (dimension 30 (width 0.05) (layer F.CrtYd)
    (gr_text "30.000 mm" (at 195 69.8) (layer F.CrtYd))
    (feature1 (pts (xy 210 84.5) (xy 210 70.413579)))
    (feature2 (pts (xy 180 84.5) (xy 180 70.413579)))
    (crossbar (pts (xy 180 71) (xy 210 71)))
    (arrow1a (pts (xy 210 71) (xy 208.873496 71.586421)))
    (arrow1b (pts (xy 210 71) (xy 208.873496 70.413579)))
    (arrow2a (pts (xy 180 71) (xy 181.126504 71.586421)))
    (arrow2b (pts (xy 180 71) (xy 181.126504 70.413579)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 181.75 77.8) (layer F.CrtYd))
    (feature1 (pts (xy 180 85.5) (xy 180 78.413579)))
    (feature2 (pts (xy 183.5 85.5) (xy 183.5 78.413579)))
    (crossbar (pts (xy 183.5 79) (xy 180 79)))
    (arrow1a (pts (xy 180 79) (xy 181.126504 78.413579)))
    (arrow1b (pts (xy 180 79) (xy 181.126504 79.586421)))
    (arrow2a (pts (xy 183.5 79) (xy 182.373496 78.413579)))
    (arrow2b (pts (xy 183.5 79) (xy 182.373496 79.586421)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 174.3 83.75 90) (layer F.CrtYd))
    (feature1 (pts (xy 183.5 82) (xy 174.913579 82)))
    (feature2 (pts (xy 183.5 85.5) (xy 174.913579 85.5)))
    (crossbar (pts (xy 175.5 85.5) (xy 175.5 82)))
    (arrow1a (pts (xy 175.5 82) (xy 176.086421 83.126504)))
    (arrow1b (pts (xy 175.5 82) (xy 174.913579 83.126504)))
    (arrow2a (pts (xy 175.5 85.5) (xy 176.086421 84.373496)))
    (arrow2b (pts (xy 175.5 85.5) (xy 174.913579 84.373496)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 181.75 151.2) (layer F.CrtYd))
    (feature1 (pts (xy 180 143.5) (xy 180 150.586421)))
    (feature2 (pts (xy 183.5 143.5) (xy 183.5 150.586421)))
    (crossbar (pts (xy 183.5 150) (xy 180 150)))
    (arrow1a (pts (xy 180 150) (xy 181.126504 149.413579)))
    (arrow1b (pts (xy 180 150) (xy 181.126504 150.586421)))
    (arrow2a (pts (xy 183.5 150) (xy 182.373496 149.413579)))
    (arrow2b (pts (xy 183.5 150) (xy 182.373496 150.586421)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 175.3 145.25 270) (layer F.CrtYd))
    (feature1 (pts (xy 183.5 147) (xy 175.913579 147)))
    (feature2 (pts (xy 183.5 143.5) (xy 175.913579 143.5)))
    (crossbar (pts (xy 176.5 143.5) (xy 176.5 147)))
    (arrow1a (pts (xy 176.5 147) (xy 175.913579 145.873496)))
    (arrow1b (pts (xy 176.5 147) (xy 177.086421 145.873496)))
    (arrow2a (pts (xy 176.5 143.5) (xy 175.913579 144.626504)))
    (arrow2b (pts (xy 176.5 143.5) (xy 177.086421 144.626504)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 214.7 145.25 270) (layer F.CrtYd))
    (feature1 (pts (xy 206 147) (xy 214.086421 147)))
    (feature2 (pts (xy 206 143.5) (xy 214.086421 143.5)))
    (crossbar (pts (xy 213.5 143.5) (xy 213.5 147)))
    (arrow1a (pts (xy 213.5 147) (xy 212.913579 145.873496)))
    (arrow1b (pts (xy 213.5 147) (xy 214.086421 145.873496)))
    (arrow2a (pts (xy 213.5 143.5) (xy 212.913579 144.626504)))
    (arrow2b (pts (xy 213.5 143.5) (xy 214.086421 144.626504)))
  )
  (dimension 4 (width 0.05) (layer F.CrtYd)
    (gr_text "4.000 mm" (at 208 151.7) (layer F.CrtYd))
    (feature1 (pts (xy 210 143.5) (xy 210 151.086421)))
    (feature2 (pts (xy 206 143.5) (xy 206 151.086421)))
    (crossbar (pts (xy 206 150.5) (xy 210 150.5)))
    (arrow1a (pts (xy 210 150.5) (xy 208.873496 151.086421)))
    (arrow1b (pts (xy 210 150.5) (xy 208.873496 149.913579)))
    (arrow2a (pts (xy 206 150.5) (xy 207.126504 151.086421)))
    (arrow2b (pts (xy 206 150.5) (xy 207.126504 149.913579)))
  )
  (dimension 4 (width 0.05) (layer F.CrtYd)
    (gr_text "4.000 mm" (at 208 75.8) (layer F.CrtYd))
    (feature1 (pts (xy 210 85.5) (xy 210 76.413579)))
    (feature2 (pts (xy 206 85.5) (xy 206 76.413579)))
    (crossbar (pts (xy 206 77) (xy 210 77)))
    (arrow1a (pts (xy 210 77) (xy 208.873496 77.586421)))
    (arrow1b (pts (xy 210 77) (xy 208.873496 76.413579)))
    (arrow2a (pts (xy 206 77) (xy 207.126504 77.586421)))
    (arrow2b (pts (xy 206 77) (xy 207.126504 76.413579)))
  )
  (dimension 3.5 (width 0.05) (layer F.CrtYd)
    (gr_text "3.500 mm" (at 218.2 83.75 90) (layer F.CrtYd))
    (feature1 (pts (xy 206.5 82) (xy 217.586421 82)))
    (feature2 (pts (xy 206.5 85.5) (xy 217.586421 85.5)))
    (crossbar (pts (xy 217 85.5) (xy 217 82)))
    (arrow1a (pts (xy 217 82) (xy 217.586421 83.126504)))
    (arrow1b (pts (xy 217 82) (xy 216.413579 83.126504)))
    (arrow2a (pts (xy 217 85.5) (xy 217.586421 84.373496)))
    (arrow2b (pts (xy 217 85.5) (xy 216.413579 84.373496)))
  )
  (gr_arc (start 183 144) (end 180 144) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183 82) (end 207 82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180 85) (end 180 144) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 183 85) (end 183 82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text 21 (at 197.618 143.202) (layer F.SilkS))
  (gr_text 20 (at 195.078 143.202) (layer F.SilkS))
  (gr_text 19 (at 192.538 143.202) (layer F.SilkS))
  (gr_text 18 (at 189.998 143.202) (layer F.SilkS))
  (gr_line (start 207 147) (end 183 147) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 207 144) (end 207 147) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 207 85) (end 210 85) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 210 85) (end 210 144) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.064 147.012) (xy 179.838 147.012) (xy 179.838 81.988) (xy 210.064 81.988)
      )
    )
  )
)
