(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 56)
    (zones 0)
    (modules 6)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.75 1.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 210.82 71.12)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01010_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 SCL)
  (net 4 SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.3)
    (diff_pair_width 0.4)
    (add_net GND)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 200.914 62.23 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 SCL))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 207.01 62.15 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.968 0 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SDA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A877BBD)
    (at 197.993 62.23 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.13 0.107 -180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer F.Cu) (tedit 5B270281)
    (at 203.962 61.976 180)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (attr smd)
    (fp_text reference U1 (at 0 2.794 180) (layer F.SilkS))
    (fp_text value Si7006 (at 0 2.575 180) (layer F.Fab) hide)
    (pad 7 smd rect (at -0.425 -0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 -0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 6 smd rect (at 1.34 -0.95 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 SCL))
    (pad 5 smd rect (at 1.34 0 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 1.34 0.95 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.34 0.95 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.34 0 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.34 -0.95 180) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 SDA))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B270794)
    (at 202.321523 55.626 270)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2 270) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 270) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 5B2DA3D3)
    (at 206.131523 66.350279 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 2.33 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 -9.95 90) (layer B.Fab))
    (fp_text user %R (at 0 2.33 90) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SCL))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SDA))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_arc (start 202.311 59.182) (end 208.28 59.182) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.342 68.58) (end 196.342 59.182) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.28 68.58) (end 196.342 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.28 59.182) (end 208.28 68.58) (layer Edge.Cuts) (width 0.15))
  (gr_text Si7006 (at 202.321523 58.928) (layer B.SilkS))
  (gr_text "cperiod 2018" (at 202.321523 60.96) (layer B.SilkS))
  (gr_text VCC (at 198.511523 63.5 270) (layer B.SilkS))
  (gr_text GND (at 201.051523 63.5 270) (layer B.SilkS))
  (gr_text SCL (at 203.591523 63.5 270) (layer B.SilkS))
  (gr_text SDA (at 206.068023 63.5 270) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.671523 59.536886) (xy 208.788 69.088) (xy 195.834 69.088) (xy 195.834 48.26) (xy 195.971523 48.26)
        (xy 195.971523 44.760279) (xy 208.671523 44.760279)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.042 52.832) (xy 195.58 52.578) (xy 195.58 69.342) (xy 209.042 69.342)
      )
    )
  )
)
