<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="stm32f030x">
<packages>
<package name="TSSOP-20">
</package>
</packages>
</library>
<library name="XN297">
<packages>
<package name="XN297">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<packages>
<package name="QFN-24">
<description>Original Author: SparkFun Electronics Eagle Libraries&lt;br&gt;
Original Source: https://github.com/sparkfun/SparkFun-Eagle-Libraries&lt;br&gt;

Footprint modified by Lance for AlienWii (removed central pad)&lt;br&gt;
License: &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/" &gt;CC BY SA V4.0&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED 0603&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="XTAL_SILVER">
<packages>
<package name="XTAL_SILVER">
</package>
</packages>
</library>
<library name="ZMR330">
<packages>
<package name="ZMR330_1">
</package>
</packages>
</library>
<library name="ANTENNA">
<packages>
<package name="ANTENNA">
</package>
</packages>
</library>
<library name="CONN_SH_6PIN">
<packages>
<package name="SM06B-SRSS-TB">
</package>
</packages>
</library>
<library name="PROG_3">
<packages>
<package name="PROG_3">
</package>
</packages>
</library>
<library name="TPS62163">
<packages>
<package name="TPS62163">
</package>
</packages>
</library>
<library name="alienflight">
<packages>
<package name="NR301X">
<description>NR301X - 3X3mm Inductor&lt;hr&gt;
&lt;a href="http://datasheet.octopart.com/NR3015T2R2M-Taiyo-Yuden-datasheet-41181804.pdf" &gt;View Datasheet&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="PEDRO_CAPACITORS">
<packages>
<package name="0603">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="PEDRO_RESISTORS">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="20MMBOARD">
<packages>
<package name="20MMBOARD">
</package>
</packages>
</library>
<library name="ADC_VIN2">
<packages>
<package name="ADC_VIN2">
</package>
</packages>
</library>
<library name="FPV_5V">
<packages>
<package name="FPV_5V">
</package>
</packages>
</library>
<library name="SILVERWARE_LOGO_3">
<packages>
<package name="SILVERWARE_LOGO_3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="stm32f030x" package="TSSOP-20" value="STM32F030XTSSOP20"/>
<element name="U1" library="XN297" package="XN297" value="XN297"/>
<element name="U3" library="SparkFun-Sensors" package="QFN-24" value="MPU6050"/>
<element name="LED1" library="microbuilder" package="CHIPLED_0603" value="LED"/>
<element name="Y1" library="XTAL_SILVER" package="XTAL_SILVER" value="16MHZ"/>
<element name="Q1" library="ZMR330" package="ZMR330_1" value="V-REG"/>
<element name="AE1" library="ANTENNA" package="ANTENNA" value="AE1">
<attribute name="NAME"/>
</element>
<element name="ESC" library="CONN_SH_6PIN" package="SM06B-SRSS-TB" value="SM06B-SRSS-TB"/>
<element name="U$4" library="PROG_3" package="PROG_3" value="PROG"/>
<element name="U4" library="TPS62163" package="TPS62163" value="TPS62163"/>
<element name="L1" library="alienflight" package="NR301X" value="NR301X">
<attribute name="MPN" value="NR3015T2R2M"/>
<attribute name="MF" value="Taiyo Yuden"/>
</element>
<element name="C1" library="PEDRO_CAPACITORS" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C3" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C10" library="PEDRO_CAPACITORS" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C12" library="PEDRO_CAPACITORS" package="0603" value="4.7uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="PEDRO_CAPACITORS" package="0603" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C14" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C15" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C16" library="PEDRO_CAPACITORS" package="0603" value="2.2nF (50v)">
<attribute name="NAME"/>
</element>
<element name="C17" library="PEDRO_CAPACITORS" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="PEDRO_CAPACITORS" package="0805" value="22uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="PEDRO_CAPACITORS" package="0603" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C5" library="PEDRO_CAPACITORS" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="PEDRO_CAPACITORS" package="0603" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C7" library="PEDRO_CAPACITORS" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="PEDRO_CAPACITORS" package="0603" value="36pF">
<attribute name="NAME"/>
</element>
<element name="C9" library="PEDRO_CAPACITORS" package="0603" value="36pF">
<attribute name="NAME"/>
</element>
<element name="R1" library="PEDRO_RESISTORS" package="0603" value="8.2K">
<attribute name="NAME"/>
</element>
<element name="R2" library="PEDRO_RESISTORS" package="0603" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R3" library="PEDRO_RESISTORS" package="0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R4" library="PEDRO_RESISTORS" package="0603" value="4.7K">
<attribute name="NAME"/>
</element>
<element name="R5" library="PEDRO_RESISTORS" package="0603" value="100">
<attribute name="NAME"/>
</element>
<element name="R6" library="PEDRO_RESISTORS" package="0603" value="500">
<attribute name="NAME"/>
</element>
<element name="R7" library="PEDRO_RESISTORS" package="0603" value="100K">
<attribute name="NAME"/>
</element>
<element name="U$3" library="20MMBOARD" package="20MMBOARD" value=""/>
<element name="X1" library="ADC_VIN2" package="ADC_VIN2" value="">
<attribute name="VALUE"/>
</element>
<element name="X2" library="FPV_5V" package="FPV_5V" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SILVERWARE_LOGO_3" package="SILVERWARE_LOGO_3" value=""/>
</elements>
<signals>
<signal name="CSN">
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="CLK">
<contactref element="U2" pad="20"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="DATA">
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Y1" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U3" pad="9"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="11"/>
<contactref element="C16" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="U$4" pad="3"/>
<contactref element="ESC" pad="1"/>
<contactref element="U4" pad="5"/>
<contactref element="C18" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="PAD"/>
<contactref element="C17" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="ESC" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="C17" pad="1"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U3" pad="24"/>
<contactref element="U2" pad="18"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="23"/>
<contactref element="U2" pad="17"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U3" pad="20"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="10"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="4"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LED1" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U2" pad="11"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="ADC">
<contactref element="R1" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="DAT">
<contactref element="U2" pad="19"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="16"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="13"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="CLOCK">
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="B1">
<contactref element="U2" pad="14"/>
<contactref element="ESC" pad="6"/>
</signal>
<signal name="A7">
<contactref element="U2" pad="13"/>
<contactref element="ESC" pad="5"/>
</signal>
<signal name="A6">
<contactref element="U2" pad="12"/>
<contactref element="ESC" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U2" pad="10"/>
<contactref element="ESC" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="AE1" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="Q1" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="L1" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="7"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U4" pad="8"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
