(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 67)
    (no_connects 0)
    (area 111.684999 91.999999 180.415001 137.235001)
    (thickness 1.6)
    (drawings 77)
    (tracks 582)
    (zones 0)
    (modules 7)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 2.5)
    (trace_clearance 0.2)
    (zone_clearance 0.75)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.4)
    (user_via 1 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 146.05 137.16)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VMEM)
  (net 3 VCC)
  (net 4 /~CS1~_Bank0)
  (net 5 /A14)
  (net 6 /A13)
  (net 7 /A12)
  (net 8 /A11)
  (net 9 /A10)
  (net 10 /A9)
  (net 11 /A8)
  (net 12 /A7)
  (net 13 /A6)
  (net 14 /A5)
  (net 15 /A4)
  (net 16 /A3)
  (net 17 /A2)
  (net 18 /A1)
  (net 19 /A0)
  (net 20 /D7)
  (net 21 /D6)
  (net 22 /D5)
  (net 23 /D4)
  (net 24 /D3)
  (net 25 /D2)
  (net 26 /D1)
  (net 27 /D0)
  (net 28 /~OE)
  (net 29 /~WE)
  (net 30 /~CS1~_Bank2)
  (net 31 /~CS1~_Bank1)
  (net 32 /CS2)
  (net 33 /A15)
  (net 34 /A16)
  (net 35 /~OE~_Gated)
  (net 36 /CS1)
  (net 37 /~WE~_Gated)
  (net 38 /PU)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CS1)
    (add_net /CS2)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /PU)
    (add_net /~CS1~_Bank0)
    (add_net /~CS1~_Bank1)
    (add_net /~CS1~_Bank2)
    (add_net /~OE)
    (add_net /~OE~_Gated)
    (add_net /~WE)
    (add_net /~WE~_Gated)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
    (add_net VMEM)
  )
  (module 0Titanium:DIN41612-44-RightAngle (layer F.Cu) (tedit 58804885)
    (at 172.72 124.46)
    (fp_text reference P1 (at -58.42 -2.54) (layer F.SilkS))
    (fp_text value "DIN 41612" (at -26.67 5.08) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VMEM))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VMEM))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /~CS1~_Bank0))
    (pad 7 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 8 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 9 thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 10 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 12 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 13 thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 14 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 15 thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 17 thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 18 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 19 thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 20 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at -25.4 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 22 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 23 thru_hole circle (at -27.94 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 24 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 25 thru_hole circle (at -30.48 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /D7))
    (pad 27 thru_hole circle (at -33.02 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /D6))
    (pad 28 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /D5))
    (pad 29 thru_hole circle (at -35.56 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /D4))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at -38.1 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /D3))
    (pad 32 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /D2))
    (pad 33 thru_hole circle (at -40.64 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /D1))
    (pad 34 thru_hole circle (at -40.64 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /D0))
    (pad 35 thru_hole circle (at -43.18 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 36 thru_hole circle (at -43.18 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /~OE))
    (pad 37 thru_hole circle (at -45.72 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole circle (at -45.72 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /~WE))
    (pad 39 thru_hole circle (at -48.26 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /~CS1~_Bank2))
    (pad 40 thru_hole circle (at -48.26 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /~CS1~_Bank1))
    (pad 41 thru_hole circle (at -50.8 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at -50.8 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /CS2))
    (pad 43 thru_hole circle (at -53.34 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 44 thru_hole circle (at -53.34 -2.54) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 5.08 2.54) (size 2.8 2.8) (drill 2.8) (layers *.Cu))
    (pad "" np_thru_hole circle (at -58.42 2.54) (size 2.8 2.8) (drill 2.8) (layers *.Cu))
  )
  (module 0Titanium:SOP32-WIDE (layer F.Cu) (tedit 5881971C)
    (at 143.51 106.045)
    (fp_text reference U1 (at -6.858 -11.811) (layer F.SilkS))
    (fp_text value "128k x 8 SRAM" (at 1.016 -11.811) (layer F.SilkS))
    (pad 18 smd rect (at 6.6 8.255) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /D6))
    (pad 15 smd rect (at -6.6 8.255) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 25 /D2))
    (pad 16 smd rect (at -6.6 9.525) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 6.6 9.525) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /D7))
    (pad 19 smd rect (at 6.6 6.985) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /D5))
    (pad 14 smd rect (at -6.6 6.985) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 /D1))
    (pad 13 smd rect (at -6.6 5.715) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /D0))
    (pad 20 smd rect (at 6.6 5.715) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 /D4))
    (pad 24 smd rect (at 6.6 0.635) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 35 /~OE~_Gated))
    (pad 9 smd rect (at -6.6 0.635) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A2))
    (pad 10 smd rect (at -6.6 1.905) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A3))
    (pad 23 smd rect (at 6.6 1.905) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 34 /A16))
    (pad 21 smd rect (at 6.6 4.445) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /D3))
    (pad 12 smd rect (at -6.6 4.445) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /A1))
    (pad 11 smd rect (at -6.6 3.175) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /A0))
    (pad 22 smd rect (at 6.6 3.175) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 36 /CS1))
    (pad 30 smd rect (at 6.6 -6.985) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /CS2))
    (pad 3 smd rect (at -6.6 -6.985) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /A8))
    (pad 4 smd rect (at -6.6 -5.715) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /A9))
    (pad 29 smd rect (at 6.6 -5.715) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /~WE~_Gated))
    (pad 31 smd rect (at 6.6 -8.255) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /A10))
    (pad 2 smd rect (at -6.6 -8.255) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /A11))
    (pad 1 smd rect (at -6.6 -9.525) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 6.6 -9.525) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VMEM))
    (pad 28 smd rect (at 6.6 -4.445) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /A12))
    (pad 5 smd rect (at -6.6 -4.445) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /A7))
    (pad 6 smd rect (at -6.6 -3.175) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /A6))
    (pad 27 smd rect (at 6.6 -3.175) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 /A15))
    (pad 25 smd rect (at 6.6 -0.635) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /A13))
    (pad 8 smd rect (at -6.6 -0.635) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /A4))
    (pad 7 smd rect (at -6.6 -1.905) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A5))
    (pad 26 smd rect (at 6.6 -1.905) (size 1.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /A14))
    (model Housings_SSOP.3dshapes/TSSOP-32_6.1x11mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.75 1.954 1.75))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58805335)
    (at 165.735 100.965)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -3.175 -5.461) (layer F.SilkS))
    (fp_text value 74HC08 (at 1.397 -5.461) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /PU))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /~WE))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /~WE~_Gated))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /PU))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /~OE))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /~OE~_Gated))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 5880534F)
    (at 166.37 112.395)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -3.81 6.223) (layer F.SilkS))
    (fp_text value 74HC148 (at 1.27 6.223) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /~CS1~_Bank1))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /A16))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /A15))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /~CS1~_Bank2))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /~CS1~_Bank0))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /CS1))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58805881)
    (at 154.305 96.52 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.413 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 5.08 -0.381 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VMEM))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58805327)
    (at 172.72 99.695 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -4.064 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58805316)
    (at 159.385 98.425 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.191 0.127 360) (layer F.SilkS))
    (fp_text value 10K (at 4.191 0.127 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 /PU))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Component packages:\n\n- 128k x 8 SRAM: SOP\n- 74HC08 and 74HC148: SOIC\n- Capacitors and resistor: 1206 " (at 140.97 97.155) (layer B.SilkS))
  (gr_text ~WE (at 127 120.65 90) (layer B.SilkS))
  (gr_text "~CS1~ Bank 1" (at 124.46 120.65 90) (layer B.SilkS))
  (gr_text "GND (IN)" (at 119.38 120.65 90) (layer B.SilkS))
  (gr_text CS2 (at 121.92 120.65 90) (layer B.SilkS))
  (gr_text D0 (at 132.08 120.65 90) (layer B.SilkS))
  (gr_text ~OE (at 129.54 120.65 90) (layer B.SilkS))
  (gr_text A5 (at 152.4 120.65 90) (layer B.SilkS))
  (gr_text GND (at 149.86 120.65 90) (layer B.SilkS))
  (gr_text A0 (at 144.78 120.65 90) (layer B.SilkS))
  (gr_text A2 (at 147.32 120.65 90) (layer B.SilkS))
  (gr_text N/C (at 137.16 120.65 90) (layer B.SilkS))
  (gr_text D2 (at 134.62 120.65 90) (layer B.SilkS))
  (gr_text D5 (at 139.7 120.65 90) (layer B.SilkS))
  (gr_text D7 (at 142.24 120.65 90) (layer B.SilkS))
  (gr_text GND (at 162.56 120.65 90) (layer B.SilkS))
  (gr_text A10 (at 160.02 120.65 90) (layer B.SilkS))
  (gr_text A7 (at 154.94 120.65 90) (layer B.SilkS))
  (gr_text A8 (at 157.48 120.65 90) (layer B.SilkS))
  (gr_text "~CS1~ Bank 0" (at 167.64 120.65 90) (layer B.SilkS))
  (gr_text A13 (at 165.1 120.65 90) (layer B.SilkS))
  (gr_text "VCC Logic" (at 170.18 120.65 90) (layer B.SilkS))
  (gr_text "VCC SRAM" (at 172.72 120.65 90) (layer B.SilkS))
  (gr_text "GND (IN)" (at 119.38 125.73 90) (layer B.SilkS))
  (gr_text GND (at 129.54 125.73 90) (layer B.SilkS))
  (gr_text GND (at 127 125.73 90) (layer B.SilkS))
  (gr_text N/C (at 121.92 125.73 90) (layer B.SilkS))
  (gr_text "~CS1~ Bank 2" (at 124.46 125.73 90) (layer B.SilkS))
  (gr_text D1 (at 132.08 125.73 90) (layer B.SilkS))
  (gr_text A6 (at 152.4 125.73 90) (layer B.SilkS))
  (gr_text A4 (at 149.86 125.73 90) (layer B.SilkS))
  (gr_text A1 (at 144.78 125.73 90) (layer B.SilkS))
  (gr_text A3 (at 147.32 125.73 90) (layer B.SilkS))
  (gr_text D4 (at 137.16 125.73 90) (layer B.SilkS))
  (gr_text D3 (at 134.62 125.73 90) (layer B.SilkS))
  (gr_text D6 (at 139.7 125.73 90) (layer B.SilkS))
  (gr_text GND (at 142.24 125.73 90) (layer B.SilkS))
  (gr_text A12 (at 162.56 125.73 90) (layer B.SilkS))
  (gr_text A11 (at 160.02 125.73 90) (layer B.SilkS))
  (gr_text GND (at 154.94 125.73 90) (layer B.SilkS))
  (gr_text A9 (at 157.48 125.73 90) (layer B.SilkS))
  (gr_text GND (at 167.64 125.73 90) (layer B.SilkS))
  (gr_text A14 (at 165.1 125.73 90) (layer B.SilkS))
  (gr_text "VCC Logic" (at 170.18 125.73 90) (layer B.SilkS))
  (gr_text "VCC SRAM" (at 172.72 125.73 90) (layer B.SilkS))
  (gr_text "Screws are NOT required" (at 169.545 135.255) (layer B.SilkS))
  (gr_text "This design is \nhereby placed into \nthe public domain" (at 125.095 112.395) (layer F.SilkS))
  (gr_text "96K SRAM Module\nfor\nTandy Model 600" (at 125.095 102.235) (layer F.SilkS))
  (gr_text "ISSI IS62C1024AL\nor similar" (at 144.145 118.745) (layer F.SilkS))
  (gr_line (start 178.435 97.79) (end 179.07 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 112.395) (end 177.8 98.425) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.07 113.03) (end 178.435 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 178.435 112.395) (end 178.435 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 178.435 98.425) (end 177.8 98.425) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.665 112.395) (end 114.3 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 113.03) (end 113.665 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 98.425) (end 114.3 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 97.79) (end 113.665 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.665 98.425) (end 113.665 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 93.345) (end 180.34 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 93.345) (end 111.76 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 114.3) (end 180.34 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.07 114.3) (end 179.07 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.07 96.52) (end 180.34 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.76 114.3) (end 111.76 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 114.3) (end 111.76 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 96.52) (end 113.03 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Hirose Electric Co Ltd PCN10EA-44P-2.54DS(72) or similar" (at 146.05 132.08) (layer F.SilkS))
  (gr_line (start 179.07 137.16) (end 113.03 137.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 92.075) (end 179.07 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 135.89) (end 113.03 137.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.07 135.89) (end 180.34 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.07 93.345) (end 179.07 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 113.03 93.345) (end 111.76 93.345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 146.05 137.16) (xy 180.34 137.16) (xy 180.34 92.075) (xy 111.76 92.075) (xy 111.76 137.16)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.75))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 146.05 137.16) (xy 180.34 137.16) (xy 180.34 92.075) (xy 111.76 92.075) (xy 111.76 137.16)
      )
    )
  )
)
