(kicad_pcb (version 20171130) (host pcbnew 5.1.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 80)
    (zones 0)
    (modules 17)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 GND)
  (net 4 "Net-(J10-Pad4)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(J5-Pad2)")
  (net 8 "Net-(J5-Pad3)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(C1-Pad1)")
  (net 12 "Net-(Q1-Pad2)")
  (net 13 "Net-(J3-Pad7)")
  (net 14 "Net-(J3-Pad3)")
  (net 15 "Net-(Q3-Pad2)")
  (net 16 "Net-(J3-Pad4)")
  (net 17 "Net-(C1-Pad2)")
  (net 18 "Net-(J2-Pad3)")
  (net 19 "Net-(J6-Pad2)")
  (net 20 "Net-(J3-Pad1)")
  (net 21 "Net-(J3-Pad2)")
  (net 22 "Net-(J3-Pad6)")
  (net 23 "Net-(J3-Pad8)")
  (net 24 "Net-(J3-Pad9)")
  (net 25 "Net-(J10-Pad3)")
  (net 26 "Net-(Q2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 156 141 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1 -3.81 180) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 149 141 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 -2.06 90) (layer F.SilkS))
    (fp_text value 1N4148FSCT-ND (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 143 141 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.08 -2.06 90) (layer F.SilkS))
    (fp_text value 1N4148FSCT-ND (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:5747840-4 (layer F.Cu) (tedit 0)
    (at 107 148 180)
    (fp_text reference J3 (at -5.5372 -10.922 180) (layer F.SilkS))
    (fp_text value CONN_5747840-4 (at -5.5372 -10.922 180) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (fp_text user * (at 0 0 180) (layer F.SilkS))
    (fp_text user * (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at -2.7686 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at -5.5372 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at -8.3058 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -11.0744 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole circle (at -1.3843 -2.8448 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at -4.1529 -2.8448 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at -6.9215 -2.8448 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad8)"))
    (pad 9 thru_hole circle (at -9.6901 -2.8448 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad9)"))
    (pad 10 np_thru_hole circle (at -18.161 -1.4224 180) (size 3.302 3.302) (drill 3.302) (layers))
    (pad 11 np_thru_hole circle (at 7.0866 -1.4224 180) (size 3.302 3.302) (drill 3.302) (layers))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 137 131)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value PTT+MUTE (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 131 134 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CW/MUTE (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RCJ-013:CUI_RCJ-013 (layer F.Cu) (tedit 0)
    (at 104 120 270)
    (descr "<b>DC POWER JACK</b><p>Source: DCJ0202.pdf")
    (fp_text reference J6 (at -4.67394 -5.77221 270) (layer F.SilkS))
    (fp_text value RCJ-013 (at -3.75429 5.50865 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.95 0 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J6-Pad2)"))
    (pad 1A thru_hole circle (at 5.95 -5 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1B thru_hole circle (at 5.95 5 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1C thru_hole circle (at 1.45 0 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module RCJ-015:CUI_RCJ-015 (layer F.Cu) (tedit 0)
    (at 120 120 270)
    (descr "<b>DC POWER JACK</b><p>Source: DCJ0202.pdf")
    (fp_text reference J7 (at -4.66679 -5.76337 270) (layer F.SilkS))
    (fp_text value RCJ-015 (at -3.75294 5.50667 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.95 0 270) (size 2.55 2.55) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad3)"))
    (pad 1A thru_hole circle (at 5.95 -5 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1B thru_hole circle (at 5.95 5 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1C thru_hole circle (at 1.45 0 270) (size 3.616 3.616) (drill 2.6) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 154 123 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value ACC2 (at 0 17.57 270) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J10-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 132 142)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3904FS-ND (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 98 133)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3906FS-ND (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 "Net-(J6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 98 141)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N3904FS-ND (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 128 142 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 109 134)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 104 141)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Q3-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module SJ1-3523N:CUI_SJ1-3523N (layer F.Cu) (tedit 5B445FAB)
    (at 137 154.5 90)
    (fp_text reference J2 (at -0.9611 -7.94406 90) (layer F.SilkS))
    (fp_text value SJ1-3523N (at -0.325301 7.64198 90) (layer F.SilkS))
    (fp_line (start -4.5 -6) (end -4.5 -2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.5 -2) (end -3.3 -2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -3.3 -2) (end -3.3 2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -3.3 2) (end -4.5 2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.5 2) (end -4.5 6) (layer Edge.Cuts) (width 0.0001))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad4)"))
    (pad 2 thru_hole circle (at 5 5 270) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J10-Pad3)"))
    (pad 3 thru_hole circle (at 5 -5 270) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad3)"))
    (pad Hole np_thru_hole circle (at -2.5 -5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 0 -5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at -2.5 5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 0 5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module SJ1-3523N:CUI_SJ1-3523N (layer F.Cu) (tedit 5B445FAB)
    (at 152 154.5 90)
    (fp_text reference J1 (at -0.9611 -7.94406 90) (layer F.SilkS))
    (fp_text value SJ1-3523N (at -0.325301 7.64198 90) (layer F.SilkS))
    (fp_line (start -4.5 -6) (end -4.5 -2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.5 -2) (end -3.3 -2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -3.3 -2) (end -3.3 2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -3.3 2) (end -4.5 2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.5 2) (end -4.5 6) (layer Edge.Cuts) (width 0.0001))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5 5 270) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad2)"))
    (pad 3 thru_hole circle (at 5 -5 270) (size 2.616 2.616) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad Hole np_thru_hole circle (at -2.5 -5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 0 -5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 5 0 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at -2.5 5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 0 5 90) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 135 159) (end 90 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135 157.8) (end 135 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 157.8) (end 135 157.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 159) (end 139 157.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 159) (end 139 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 157.8) (end 150 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 157.8) (end 150 157.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 159) (end 154 157.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165 159) (end 154 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165 118) (end 165 159) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90 118) (end 165 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90 159) (end 90 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text WD1CKS/W8BSD (at 149 135.75) (layer B.SilkS))
  (gr_text "Ultimate TS-940S Interface v1.1" (at 110.75 156) (layer B.SilkS))
  (gr_text 8 (at 138.75 120.25 90) (layer F.SilkS))
  (gr_text 9 (at 141.25 120.25 90) (layer F.SilkS))
  (gr_text 13 (at 143.75 120.25 90) (layer F.SilkS))
  (gr_text 12 (at 146.5 120.25 90) (layer F.SilkS))
  (gr_text 11 (at 148.75 120.25 90) (layer F.SilkS))
  (gr_text 4 (at 151.5 120.25 90) (layer F.SilkS))
  (gr_text 3 (at 154 120.25 90) (layer F.SilkS))
  (gr_text "LINE OUT" (at 129.75 148.25 90) (layer F.SilkS))
  (gr_text "LINE IN" (at 144.5 149.25 90) (layer F.SilkS))
  (gr_text CW (at 112 122) (layer F.SilkS))
  (gr_text FSK (at 95 122) (layer F.SilkS))
  (gr_text PTT+MUTE (at 139 127) (layer F.SilkS))
  (gr_text MUTE (at 131 130 90) (layer F.SilkS))
  (gr_text CW (at 126 131 90) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165 159) (xy 90 159) (xy 90 118) (xy 165 118)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165 159) (xy 90 159) (xy 90 118) (xy 165 118)
      )
    )
  )
)
