<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="33.02" x2="20.32" y2="33.02" width="0.254" layer="20"/>
<wire x1="21.59" y1="31.75" x2="21.59" y2="25.4" width="0.254" layer="20"/>
<wire x1="5.08" y1="33.02" x2="3.81" y2="31.75" width="0.254" layer="20" curve="90"/>
<wire x1="3.81" y1="31.75" x2="3.81" y2="25.4" width="0.254" layer="20"/>
<wire x1="20.32" y1="0" x2="5.08" y2="0" width="0.254" layer="20"/>
<wire x1="3.81" y1="1.27" x2="3.81" y2="7.62" width="0.254" layer="20"/>
<text>L</text>
<text>U</text>
<text>C</text>
<text>D</text>
<text>R</text>
<text>G</text>
<text>KD0GLS 2017</text>
<text>L</text>
<text>U</text>
<text>C</text>
<text>D</text>
<text>R</text>
<text>G</text>
<wire x1="21.59" y1="1.27" x2="21.59" y2="7.62" width="0.254" layer="20"/>
<wire x1="3.81" y1="7.62" x2="3.81" y2="25.4" width="0.254" layer="20" curve="-90"/>
<wire x1="21.59" y1="25.4" x2="21.59" y2="7.62" width="0.254" layer="20" curve="-90"/>
<wire x1="3.81" y1="1.27" x2="5.08" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="20.32" y1="0" x2="21.59" y2="1.27" width="0.254" layer="20" curve="90"/>
<wire x1="21.59" y1="31.75" x2="20.32" y2="33.02" width="0.254" layer="20" curve="90"/>
<text>5-WAY NAV</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CONN_BREAKAWAY_1X6_100">
</package>
<package name="SWITCH_PANASONIC_EVQQ2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="kd0gls" package="CONN_BREAKAWAY_1X6_100" value="CONN_BREAKAWAY_1X6_100"/>
<element name="SW1" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="SW2" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="SW3" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="SW4" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="SW5" library="kd0gls" package="SWITCH_PANASONIC_EVQQ2" value="SWITCH_PANASONIC_EVQQ2"/>
<element name="J2" library="kd0gls" package="CONN_BREAKAWAY_1X6_100" value="CONN_BREAKAWAY_1X6_100"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SW5" pad="B"/>
<contactref element="SW5" pad="B'"/>
<contactref element="SW3" pad="B"/>
<contactref element="SW3" pad="B'"/>
<contactref element="SW2" pad="B"/>
<contactref element="SW2" pad="B'"/>
<contactref element="SW1" pad="B"/>
<contactref element="SW1" pad="B'"/>
<contactref element="SW4" pad="B"/>
<contactref element="SW4" pad="B'"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="UP">
<contactref element="J1" pad="2"/>
<contactref element="SW3" pad="A"/>
<contactref element="SW3" pad="A'"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="LEFT">
<contactref element="J1" pad="3"/>
<contactref element="SW2" pad="A"/>
<contactref element="SW2" pad="A'"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="CENTER">
<contactref element="J1" pad="4"/>
<contactref element="SW1" pad="A"/>
<contactref element="SW1" pad="A'"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="RIGHT">
<contactref element="J1" pad="5"/>
<contactref element="SW4" pad="A"/>
<contactref element="SW4" pad="A'"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="DOWN">
<contactref element="J1" pad="6"/>
<contactref element="SW5" pad="A"/>
<contactref element="SW5" pad="A'"/>
<contactref element="J2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
