(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "PT100OSHPark:4-40 Thru" (layer "F.Cu")
    (tedit 623D00AB)
    (at 140.5 72.41)
    (attr through_hole)
    (fp_text reference "e" (at 6.858 0) (layer "Dwgs.User"))
    (fp_text value "4-40 Thru" (at -8.128 -0.127) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.95 2.95) (drill 2.95) (layers *.Cu *.Mask))
  )
  (footprint "PT100OSHPark:SolderConn" (layer "F.Cu")
    (tedit 623CFEAF)
    (at 142.748 76.2508)
    (attr through_hole)
    (fp_text reference "REF**" (at 6.223 2.667) (layer "Dwgs.User"))
    (fp_text value "SolderConn" (at 6.858 -1.397) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "PT100OSHPark:SolderConn" (layer "F.Cu")
    (tedit 623CFEAF)
    (at 138.1506 76.3016)
    (attr through_hole)
    (fp_text reference "REF**" (at 11.176 4.445) (layer "Dwgs.User"))
    (fp_text value "SolderConn" (at -5.969 -0.635) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "PT100OSHPark:pt100 thru" (layer "F.Cu")
    (tedit 623CFC15)
    (at 140.5256 76.2146)
    (attr through_hole)
    (fp_text reference "REF**" (at 9.055 -0.421) (layer "Dwgs.User"))
    (fp_text value "pt100 thru" (at -8.598 -0.294) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -0.75 0) (size 0.397 0.397) (drill 0.397) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0) (size 0.397 0.397) (drill 0.397) (layers *.Cu *.Mask))
  )
  (footprint "PT100OSHPark:Amp_4pin" (layer "F.Cu")
    (tedit 623D6984)
    (at 140.5488 67.7746 180)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 3.25) (layer "Dwgs.User"))
    (fp_text value "Amp_4pin" (at 0 -2.75) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -1.125 180) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -0.5 -1.125 180) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 0.5 -1.125 180) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect (at 1.5 -1.125 180) (size 0.5 1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at -2.25 1.125 180) (size 1.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect (at 2.25 1.125 180) (size 1.2 1.7) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (gr_line (start 136.7156 80.4546) (end 144.3356 80.4546) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 144.3356 80.4546) (end 144.3356 65.2146) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 136.7156 80.4546) (end 136.7156 65.2146) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 136.7156 65.2146) (end 144.3356 65.2146) (layer "Edge.Cuts") (width 0.15))
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.272 65.2018)
        (xy 144.2974 80.4164)
        (xy 136.7282 80.391)
        (xy 136.7028 65.2018)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.4178 77.86)
        (xy 138.6078 77.851)
        (xy 138.6078 74.6506)
        (xy 142.4178 74.6506)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.4178 77.8764)
        (xy 138.6078 77.851)
        (xy 138.6078 74.6506)
        (xy 142.4178 74.6506)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.5768 80.772)
        (xy 136.398 80.772)
        (xy 136.398 65.024)
        (xy 144.5768 65.024)
      )
    )
  )
)
