(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 36)
    (zones 0)
    (modules 3)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /SCL)
  (net 4 /SDA)
  (net 5 /GPIO2)
  (net 6 /GPIO1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GPIO1)
    (add_net /GPIO2)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net VCC)
  )
  (module tom-connectors:PMOD_1X6_PTH_RA_PLUG (layer F.Cu) (tedit 5D668F7F)
    (at 33.55 41.25 270)
    (attr smd)
    (fp_text reference PMOD1 (at 0 3 90) (layer F.SilkS))
    (fp_text value PMOD-Device-x1-Type-1-GPIO (at -0.25 4.5 90) (layer F.SilkS) hide)
    (pad 6 thru_hole oval (at 6.35 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole oval (at 3.81 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 1.27 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 3 thru_hole oval (at -1.27 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 3 /SCL))
    (pad 2 thru_hole oval (at -3.81 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 5 /GPIO2))
    (pad 1 thru_hole oval (at -6.35 1.27 180) (size 2.54 1.7) (drill 1 (offset -0.4 0)) (layers *.Cu *.Mask)
      (net 6 /GPIO1))
  )
  (module badgelife-parts:Badgelife-SAOv169-BADGE-2x3 (layer F.Cu) (tedit 5C931861)
    (at 49.6 41.45 270)
    (descr "Through hole straight IDC box header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x03 2.54mm double row")
    (fp_text reference X1 (at -5.05 0 180) (layer F.SilkS))
    (fp_text value Badgelife_sao_connector_v169bis (at 0 -8.509 90) (layer F.Fab) hide)
    (fp_text user GPIO1 (at 3.937 -2.794 90) (layer B.SilkS))
    (fp_text user GPIO2 (at 3.937 3.048 90) (layer B.SilkS))
    (fp_text user SCL (at 0 3.048 90) (layer B.SilkS))
    (fp_text user SDA (at 0 -2.794 90) (layer B.SilkS))
    (fp_text user GND (at -2.54 3.048 90) (layer B.SilkS))
    (fp_text user VCC (at -2.54 -2.794 90) (layer B.SilkS))
    (fp_text user %R (at 0.06 0.02 180) (layer F.Fab))
    (pad 2 thru_hole rect (at -2.48 1.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at -2.48 -1.25 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0.06 1.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /SCL))
    (pad 3 thru_hole oval (at 0.06 -1.25 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /SDA))
    (pad 6 thru_hole circle (at 2.6 1.29 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /GPIO2))
    (pad 5 thru_hole circle (at 2.6 -1.25 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /GPIO1))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 38.85 46.65 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.75 -0.05 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Aug 2019" (at 38.6 41.6 90) (layer B.SilkS))
  (gr_text pmod-sao (at 35.7 41.3 90) (layer F.SilkS))
  (gr_text tom@tomk.in (at 42 41.5 90) (layer F.SilkS))
  (gr_line (start 55 34) (end 55 49) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 30 32) (end 53 32) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 28 49) (end 28 34) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53 51) (end 30 51) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 30 49) (end 28 49) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53 49) (end 53 51) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 53 34) (end 55 34) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 30 34) (end 30 32) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28 32) (xy 55 32) (xy 55 51) (xy 28 50.9)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 32) (xy 28 32) (xy 28 50.9) (xy 55 51)
      )
    )
  )
)
