(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 121.674999 83.624999 147.825001 114.775001)
    (thickness 1.6)
    (drawings 27)
    (tracks 62)
    (zones 0)
    (modules 7)
    (nets 10)
  )
  (page USLetter)
  (title_block
    (title "NE8FDV Breakout")
    (date 2017-09-06)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.6 2)
    (pad_drill 6.6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 190.5 107.95)
    (grid_origin 190.5 107.95)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J2-Pad2)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J4-Pad2)")
  (net 9 "Net-(J4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Audio ""
    (clearance 0.38608)
    (trace_width 0.64008)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59B0712A)
    (at 145.28 111.43 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.Fab))
    (fp_text value "CH 1" (at 3.05 7.41 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59B0713D)
    (at 145.28 92.38 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.Fab))
    (fp_text value CH2 (at 3.05 7.41 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59B07130)
    (at 123.69 111.43 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.Fab))
    (fp_text value "CH 3" (at -3.3 7.41 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59B07136)
    (at 123.69 92.38 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.Fab))
    (fp_text value "CH 4" (at -3.3 7.41 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NeutrikSnakeLib:NE8FDV-noHole (layer F.Cu) (tedit 59B0B669)
    (at 126.23 99.365)
    (fp_text reference J5 (at 5.84 1.365) (layer F.Fab))
    (fp_text value RJ45 (at 5.27 0.085) (layer F.Fab))
    (pad 1 thru_hole circle (at 12.865 -2.11) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad2)"))
    (pad 2 thru_hole circle (at 11.595 -4.65) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 3 thru_hole circle (at 10.325 -2.11) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 4 thru_hole circle (at 9.055 -4.65) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 7.785 -2.11) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 6 thru_hole circle (at 6.515 -4.65) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 7 thru_hole circle (at 5.245 -2.11) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad2)"))
    (pad 8 thru_hole circle (at 3.975 -4.65) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad3)"))
    (pad 9 thru_hole circle (at 15.025 10.55) (size 2.15 2.15) (drill 1.45) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at 2.625 -11.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 16.85 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 14.225 -11.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  )
  (module logo:TSC (layer F.Cu) (tedit 59B07D79)
    (at 134.62 104.648)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module logo:TSCMask (layer F.Cu) (tedit 59B07D79)
    (at 134.62 104.648)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (gr_arc (start 131.826 89.408) (end 131.826 90.932) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.414 89.408) (end 137.414 87.884) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_text "CUT OUT" (at 134.75 89.7) (layer F.SilkS))
  (gr_text 12.12.2017 (at 134.75 113.7) (layer F.SilkS))
  (gr_text NE8FDV (at 134.75 85.7) (layer F.SilkS))
  (gr_line (start 131.826 87.884) (end 137.414 87.884) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.414 90.932) (end 131.826 90.932) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.75 111.2) (end 121.75 87.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.25 114.7) (end 125.25 114.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.75 87.2) (end 147.75 111.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.25 83.7) (end 144.25 83.7) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.25 111.2) (end 125.25 114.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.25 111.2) (end 147.75 111.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.25 87.2) (end 144.25 83.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.25 87.2) (end 121.75 87.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 142.105 106.35) (layer F.SilkS))
  (gr_text + (at 142.105 108.89) (layer F.SilkS))
  (gr_text GND (at 141.47 111.43) (layer F.SilkS))
  (gr_text GND (at 141.47 92.38) (layer F.SilkS))
  (gr_text + (at 141.47 89.84) (layer F.SilkS))
  (gr_text - (at 141.47 87.3) (layer F.SilkS))
  (gr_text GND (at 127.5 111.43) (layer F.SilkS))
  (gr_text + (at 127.5 108.89) (layer F.SilkS))
  (gr_text - (at 127.5 106.35) (layer F.SilkS))
  (gr_text - (at 127.5 87.3) (layer F.SilkS))
  (gr_text + (at 127.5 89.84) (layer F.SilkS))
  (gr_text GND (at 127.5 92.38) (layer F.SilkS))
)
