(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 50)
    (no_connects 0)
    (area 13.919999 23.7998 77.7 85.25)
    (thickness 1.6)
    (drawings 14)
    (tracks 143)
    (zones 0)
    (modules 31)
    (nets 19)
  )
  (page A3)
  (title_block
    (rev 2)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gbr/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 +5V)
  (net 3 "/IR SIG")
  (net 4 /SIG3)
  (net 5 /SIG4)
  (net 6 GND)
  (net 7 "Net-(C1-Pad1)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(IC1-Pad1)")
  (net 11 "Net-(IC1-Pad7)")
  (net 12 "Net-(P2-Pad2)")
  (net 13 "Net-(Q1-Pad1)")
  (net 14 "Net-(Q1-Pad2)")
  (net 15 "Net-(Q2-Pad1)")
  (net 16 "Net-(Q2-Pad2)")
  (net 17 "Net-(Q3-Pad3)")
  (net 18 "Net-(Q5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net "/IR SIG")
    (add_net /SIG3)
    (add_net /SIG4)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q5-Pad2)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +12V)
    (add_net GND)
  )
  (module PIN_ARRAY_3X1 (layer F.Cu) (tedit 4C1130E0)
    (at 16.51 52.07 270)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference K1 (at 0.254 -2.159 270) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 -2.159 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "/IR SIG"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model pin_array/pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-3MM (layer F.Cu) (tedit 50ADE848)
    (at 26.67 59.69)
    (descr "LED 3mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 3mm 3MM 100mil 2,54mm")
    (fp_text reference D2 (at 1.778 -2.794) (layer F.SilkS))
    (fp_text value LED (at 0 2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.6764 1.6764) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D2-Pad2)"))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C2 (layer F.Cu) (tedit 200000)
    (at 31.75 38.1 90)
    (descr "Condensateur = 2 pas")
    (tags C)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module C2 (layer F.Cu) (tedit 200000)
    (at 21.59 38.1 90)
    (descr "Condensateur = 2 pas")
    (tags C)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 0.33uF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bornier2 (layer F.Cu) (tedit 59307027)
    (at 27.94 29.21)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P1 (at -6.35 -2.54) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model device/bornier_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bornier2 (layer F.Cu) (tedit 5930701F)
    (at 48.26 29.21)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P2 (at -7.62 0) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad2)"))
    (model device/bornier_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DIP-8__300 (layer F.Cu) (tedit 53D69865)
    (at 26.67 50.8 270)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference IC1 (at -6.35 -2.54 360) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG3))
    (pad 3 thru_hole circle (at 1.27 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG4))
    (pad 4 thru_hole circle (at 3.81 3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 5 thru_hole circle (at 3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D2-Pad1)"))
    (pad 6 thru_hole circle (at 1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 "/IR SIG"))
    (pad 7 thru_hole circle (at -1.27 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole circle (at -3.81 -3.81 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model dil/dil_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO92flat (layer F.Cu) (tedit 53D545CF)
    (at 33.02 69.85)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (fp_text reference Q1 (at -2.54 2.54) (layer F.SilkS))
    (fp_text value BC547 (at 0 -1.905) (layer F.SilkS))
    (pad 1 thru_hole rect (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO92flat (layer F.Cu) (tedit 53D52961)
    (at 50.8 67.31 180)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (fp_text reference Q2 (at 0 3.175 180) (layer F.SilkS))
    (fp_text value BC547 (at 0 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO92flat (layer F.Cu) (tedit 53D52961)
    (at 46.99 62.23 180)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (fp_text reference Q3 (at 0 3.175 180) (layer F.SilkS))
    (fp_text value BC337 (at 0 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(Q2-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(Q3-Pad3)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO92flat (layer F.Cu) (tedit 53D52961)
    (at 54.61 62.23)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (fp_text reference Q4 (at 0 3.175) (layer F.SilkS))
    (fp_text value BC327 (at 0 -1.905) (layer F.SilkS))
    (pad 1 thru_hole rect (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(Q2-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(Q3-Pad3)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO92_78L05 (layer F.Cu) (tedit 53D69871)
    (at 26.67 40.64)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (fp_text reference U1 (at -1.27 2.54) (layer F.SilkS))
    (fp_text value 78L05 (at 0 -1.905) (layer F.SilkS))
    (pad VO thru_hole rect (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad GND thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad VI thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C1-Pad1)"))
    (model discret/to98.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO220_IRF540N (layer F.Cu) (tedit 53D53A29)
    (at 54.61 54.61 90)
    (descr "Regulateur TO220 serie LM78xx")
    (tags "TR TO220")
    (fp_text reference Q5 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value IRF540N (at 0.635 -6.35 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(Q5-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P2-Pad2)"))
  )
  (module 1pin (layer F.Cu) (tedit 5434228D)
    (at 17.78 69.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module 1pin (layer F.Cu) (tedit 5434227F)
    (at 57.15 69.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module 1pin (layer F.Cu) (tedit 54342285)
    (at 57.15 27.94)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module 1pin (layer F.Cu) (tedit 54342289)
    (at 17.78 27.94)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference 1PIN (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module C2 (layer F.Cu) (tedit 200000)
    (at 44.45 54.61 90)
    (descr "Condensateur = 2 pas")
    (tags C)
    (fp_text reference C3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_3X1 (layer F.Cu) (tedit 4C1130E0)
    (at 16.51 60.96 270)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference K2 (at 0.254 -2.159 270) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 -2.159 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SIG3))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model pin_array/pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIN_ARRAY_3X1 (layer F.Cu) (tedit 4C1130E0)
    (at 20.32 60.96 270)
    (descr "Connecteur 3 pins")
    (tags "CONN DEV")
    (fp_text reference K3 (at 0.254 -2.159 270) (layer F.SilkS))
    (fp_text value CONN_3 (at 0 -2.159 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SIG4))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model pin_array/pins_array_3x1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5920C254)
    (at 34.29 45.72 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C4 (at 2.5 -2.01 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.01 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 34.29 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(IC1-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 593078E7)
    (at 36.83 45.72 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_5W_P10.16mm_Horizontal (layer F.Cu) (tedit 59307841)
    (at 16.51 43.18 90)
    (descr "D, 5W series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=8.9*3.7mm^2, , http://www.diodes.com/_files/packages/8686949.gif")
    (tags "D 5W series Axial Horizontal pin pitch 10.16mm  length 8.9mm diameter 3.7mm")
    (fp_text reference D1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 1N4001 (at 5.08 2.91 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_5W_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 593078A3)
    (at 39.37 45.72 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value 10R (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q3-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Q5-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59307886)
    (at 41.91 35.56 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 10K (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Q5-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59307865)
    (at 33.02 54.61 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 4K7 (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59340046)
    (at 38.735 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5930786F)
    (at 35.56 54.61 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 38.1 54.61 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 40.64 64.77 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.31 90) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 19.05 54.61) (layer B.SilkS))
  (gr_text SIG (at 19.05 52.07) (layer B.SilkS))
  (gr_text +5 (at 19.05 49.53) (layer B.SilkS))
  (gr_text -LED (at 50.8 26.67) (layer B.SilkS))
  (gr_text +LED (at 45.72 26.67) (layer B.SilkS))
  (gr_text GND (at 30.48 26.67) (layer B.SilkS))
  (gr_text +12 (at 25.4 26.67) (layer B.SilkS))
  (gr_text "rurLedDimmer\nv. 1.1\n2017/06" (at 52.07 39.37) (layer F.SilkS))
  (dimension 49.53 (width 0.3) (layer Dwgs.User)
    (gr_text "49,530 mm" (at 71.2 48.895 90) (layer Dwgs.User))
    (feature1 (pts (xy 64.77 24.13) (xy 72.55 24.13)))
    (feature2 (pts (xy 64.77 73.66) (xy 72.55 73.66)))
    (crossbar (pts (xy 69.85 73.66) (xy 69.85 24.13)))
    (arrow1a (pts (xy 69.85 24.13) (xy 70.43642 25.256503)))
    (arrow1b (pts (xy 69.85 24.13) (xy 69.26358 25.256503)))
    (arrow2a (pts (xy 69.85 73.66) (xy 70.43642 72.533497)))
    (arrow2b (pts (xy 69.85 73.66) (xy 69.26358 72.533497)))
  )
  (gr_line (start 60.96 24.13) (end 60.96 73.66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 13.97 24.13) (end 13.97 73.66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.96 73.66) (end 13.97 73.66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 13.97 24.13) (end 60.96 24.13) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 46.99 (width 0.3) (layer Dwgs.User)
    (gr_text "46,990 mm" (at 37.465 83.899999) (layer Dwgs.User))
    (feature1 (pts (xy 60.96 77.47) (xy 60.96 85.249999)))
    (feature2 (pts (xy 13.97 77.47) (xy 13.97 85.249999)))
    (crossbar (pts (xy 13.97 82.549999) (xy 60.96 82.549999)))
    (arrow1a (pts (xy 60.96 82.549999) (xy 59.833497 83.136419)))
    (arrow1b (pts (xy 60.96 82.549999) (xy 59.833497 81.963579)))
    (arrow2a (pts (xy 13.97 82.549999) (xy 15.096503 83.136419)))
    (arrow2b (pts (xy 13.97 82.549999) (xy 15.096503 81.963579)))
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.96 24.13) (xy 13.97 24.13) (xy 13.97 73.66) (xy 60.96 73.66)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.96 24.13) (xy 13.97 24.13) (xy 13.97 73.66) (xy 60.96 73.66)
      )
    )
  )
)
