<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<circle x="16.002" y="16.002" radius="15.494" width="0.0254" layer="20"/>
<text>4800 uF @ 25V</text>
<text>1200 uF X4</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>Barbouri 2020
Greg Christenson</text>
<text>+</text>
<text>Do Not Cut</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>Open Hardware</text>
<text>HP 3456A C5</text>
<text>Rev 1.1</text>
<text>Caps
UHW1E122MPD
Nichicon</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,17/1,3">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="E5-10,5" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="UHW1E122MPD"/>
</element>
<element name="GND" library="wirepad" package="3,17/1,3" value="GND">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="3,17/1,3" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="3,17/1,3" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="3,17/1,3" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="E5-10,5" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="UHW1E122MPD"/>
</element>
<element name="C3" library="adafruit" package="E5-10,5" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="UHW1E122MPD"/>
</element>
<element name="C4" library="adafruit" package="E5-10,5" value="1200uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="UHW1E122MPD"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="PAD4" pad="1"/>
<contactref element="PAD5" pad="1"/>
<contactref element="PAD3" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
</signal>
<signal name="+5">
<contactref element="C1" pad="+"/>
<contactref element="C4" pad="+"/>
<contactref element="C3" pad="+"/>
<contactref element="C2" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
