(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 135)
    (zones 0)
    (modules 21)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.8)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 3.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x0f030_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D2-Pad2)")
  (net 3 +3V3)
  (net 4 Z_PROBE_CONN)
  (net 5 -FAN0)
  (net 6 -FAN1)
  (net 7 +V_LED)
  (net 8 -V_LED)
  (net 9 +FAN0)
  (net 10 +FAN1)
  (net 11 -V_IN)
  (net 12 +V_IN)
  (net 13 -V_Probe)
  (net 14 -THERM)
  (net 15 +THERM)
  (net 16 "Net-(D3-Pad2)")
  (net 17 "Net-(D4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +FAN0)
    (add_net +FAN1)
    (add_net +THERM)
    (add_net +V_IN)
    (add_net +V_LED)
    (add_net -FAN0)
    (add_net -FAN1)
    (add_net -THERM)
    (add_net -V_IN)
    (add_net -V_LED)
    (add_net -V_Probe)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net Z_PROBE_CONN)
  )
  (module CArraigeFanBreakout:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical_DJP (layer F.Cu) (tedit 5FA8964D)
    (at 92.5 67.7)
    (descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J13 (at 1.25 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 -THERM))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 15 +THERM))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_JST_B2B-XH-A(LF)(SN)/eec.models/JST_-_B2B-XH-A(LF)(SN).step"
      (offset (xyz 1.25 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical_DJP (layer F.Cu) (tedit 5FA8964D)
    (at 109.22 62.23)
    (descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J11 (at -2.17 5.17 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 +V_LED))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 8 -V_LED))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_JST_B2B-XH-A(LF)(SN)/eec.models/JST_-_B2B-XH-A(LF)(SN).step"
      (offset (xyz 1.25 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical_DJP (layer F.Cu) (tedit 5FA8964D)
    (at 120.65 78.74 180)
    (descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J4 (at -4.05 -2.11 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 +FAN1))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 6 -FAN1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_JST_B2B-XH-A(LF)(SN)/eec.models/JST_-_B2B-XH-A(LF)(SN).step"
      (offset (xyz 1.25 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical_DJP (layer F.Cu) (tedit 5FA8964D)
    (at 111.76 78.74 180)
    (descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J3 (at 6.36 1.89 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 +FAN1))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 6 -FAN1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_JST_B2B-XH-A(LF)(SN)/eec.models/JST_-_B2B-XH-A(LF)(SN).step"
      (offset (xyz 1.25 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical_DJP (layer F.Cu) (tedit 5FA8964D)
    (at 118.11 62.23)
    (descr "JST XH series connector, B2B-XH-AM, with boss (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical boss")
    (fp_text reference J2 (at 6.29 -1.88 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.6 2) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 +FAN0))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 5 -FAN0))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-AM_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_JST_B2B-XH-A(LF)(SN)/eec.models/JST_-_B2B-XH-A(LF)(SN).step"
      (offset (xyz 1.25 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 127.4 64.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 -V_IN))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:Phoenix_Contact-1751248-0-0-0 (layer F.Cu) (tedit 5FA890B0)
    (at 102.05 70.200001)
    (fp_text reference J7 (at -3.35 4.799999 180) (layer F.SilkS))
    (fp_text value 1751248 (at 0 0) (layer Cmts.User))
    (pad 1 thru_hole rect (at -1.75 0.049999) (size 1.7 1.7) (drill 1.1) (layers *.Cu)
      (net 12 +V_IN))
    (pad 2 thru_hole circle (at 1.75 0.049999) (size 1.7 1.7) (drill 1.1) (layers *.Cu)
      (net 11 -V_IN))
    (model eec.models/Phoenix_Contact_-_1751248.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_Phoenix Contact_1751248/eec.models/pxc_1751248_04_MKDS-1-2-3-5_3D.stp"
      (offset (xyz -3.75 -3.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 127.525 61.9)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 17 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 12 +V_IN))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 115.45 72.6 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -1.565 -1.71 90) (layer F.SilkS))
    (fp_text value R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 -V_LED))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 114.95 68.7 270)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at -3.15 0 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 16 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 7 +V_LED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 109.22 68.58 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J11 (at -0.97 -2.97) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +V_LED))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 -V_LED))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 92.3 73.75 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at -2.85 2.85) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 -THERM))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 +THERM))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 127.245 78.74)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at -0.045 2.11) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 2 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 10 +FAN1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 104.09 79.75 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at -2.55 5.24) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 -V_Probe))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Z_PROBE_CONN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 120.65 72.39 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 0.11 -2.85 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +FAN1))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 -FAN1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 118.11 68.58 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0.08 5.39 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +FAN0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 -FAN0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CArraigeFanBreakout:Phoenix_Contact-1751248-0-0-0 (layer F.Cu) (tedit 5FA890B0)
    (at 102.08 62.23 180)
    (fp_text reference J6 (at 4.83 1.18 270) (layer F.SilkS))
    (fp_text value 1751248 (at -0.48 2.54) (layer Dwgs.User) hide)
    (pad 1 thru_hole rect (at -1.75 0.049999 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu)
      (net 11 -V_IN))
    (pad 2 thru_hole circle (at 1.75 0.049999 180) (size 1.7 1.7) (drill 1.1) (layers *.Cu)
      (net 12 +V_IN))
    (model eec.models/Phoenix_Contact_-_1751248.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "F:/kicad/Conn_Phoenix Contact_1751248/eec.models/pxc_1751248_04_MKDS-1-2-3-5_3D.stp"
      (offset (xyz -3.75 -3.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 127.15 76.35)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0.0925 -1.69) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 -FAN1))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 127.3075 71.63 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -3.3425 -0.02) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 -FAN0))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 112.9 72.7 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 2.25 7.85) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 -V_Probe))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Z_PROBE_CONN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF1)
    (at 127.3 69)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 3.45 0.15) (layer F.SilkS))
    (fp_text value LED (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 9 +FAN0))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text https://git.io/JkJs4 (at 118.7 66.05) (layer B.SilkS))
  (gr_arc (start 133.835 76.2) (end 133.835 77.47) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.93 77.47) (end 133.835 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.93 74.93) (end 133.835 74.93) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.93 76.2) (end 131.93 74.93) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.93 66.04) (end 133.835 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.93 63.5) (end 133.835 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 133.835 64.77) (end 133.835 66.04) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 131.93 64.77) (end 131.93 63.5) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.75 58.42) (end 135.74 58.42) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.57 78.74) (end 89.57 61.595) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.74 81.915) (end 92.745 81.915) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.01 59.69) (end 137.01 80.645) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 135.74 80.645) (end 135.74 81.915) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 135.74 59.69) (end 137.01 59.69) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.745 61.595) (end 92.745 58.42) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 92.745 78.74) (end 89.57 78.74) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 92.745 61.595) (end 92.745 63.195) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 92.745 78.74) (end 92.745 80.34) (layer Edge.Cuts) (width 0.05))
)
