(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (title_block
    (title "Raspberry PiDal Switcher Relay Board")
    (date "2025-02-12")
    (rev "v1.1")
    (company "Slow Brewed Effects")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user "plugins.config")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(K1A--)")
  (net 4 "Net-(K1A-+)")
  (net 5 "Net-(D2-C)")
  (net 6 "Net-(D2-PadA)")
  (net 7 "Net-(V0-PAD)")
  (net 8 "Net-(K2A--)")
  (net 9 "Net-(K2A-+)")
  (net 10 "Net-(D5-C)")
  (net 11 "Net-(D5-PadA)")
  (net 12 "Net-(K3A--)")
  (net 13 "Net-(K3A-+)")
  (net 14 "Net-(D7-C)")
  (net 15 "Net-(D7-PadA)")
  (net 16 "Net-(K4A--)")
  (net 17 "Net-(K4A-+)")
  (net 18 "Net-(D9-C)")
  (net 19 "Net-(D9-PadA)")
  (net 20 "Net-(K5A--)")
  (net 21 "Net-(K5A-+)")
  (net 22 "Net-(D11-C)")
  (net 23 "Net-(D11-PadA)")
  (net 24 "Net-(K6A--)")
  (net 25 "Net-(K6A-+)")
  (net 26 "Net-(D13-C)")
  (net 27 "Net-(D13-PadA)")
  (net 28 "Net-(K7A--)")
  (net 29 "Net-(K7A-+)")
  (net 30 "Net-(D15-C)")
  (net 31 "Net-(D15-PadA)")
  (net 32 "Net-(K8A--)")
  (net 33 "Net-(K8A-+)")
  (net 34 "Net-(D17-C)")
  (net 35 "Net-(D17-PadA)")
  (net 36 "Net-(ER1-PAD)")
  (net 37 "Net-(ER2-PAD)")
  (net 38 "Net-(ER3-PAD)")
  (net 39 "Net-(ER4-PAD)")
  (net 40 "Net-(ER5-PAD)")
  (net 41 "Net-(ER6-PAD)")
  (net 42 "Net-(ER7-PAD)")
  (net 43 "/N$5")
  (net 44 "Net-(ES3-PAD)")
  (net 45 "Net-(ES4-PAD)")
  (net 46 "Net-(ES5-PAD)")
  (net 47 "Net-(ES6-PAD)")
  (net 48 "Net-(ES7-PAD)")
  (net 49 "unconnected-(IC1-Pad4)")
  (net 50 "Net-(P1-PAD)")
  (net 51 "unconnected-(IC2-Pad4)")
  (net 52 "Net-(P2-PAD)")
  (net 53 "unconnected-(IC3-Pad4)")
  (net 54 "Net-(P3-PAD)")
  (net 55 "Net-(IC9-ANODE)")
  (net 56 "unconnected-(IC4-Pad4)")
  (net 57 "Net-(P4-PAD)")
  (net 58 "Net-(IC10-ANODE)")
  (net 59 "unconnected-(IC5-Pad4)")
  (net 60 "Net-(P5-PAD)")
  (net 61 "Net-(IC11-ANODE)")
  (net 62 "unconnected-(IC6-Pad4)")
  (net 63 "Net-(P6-PAD)")
  (net 64 "Net-(IC12-ANODE)")
  (net 65 "unconnected-(IC7-Pad4)")
  (net 66 "Net-(P7-PAD)")
  (net 67 "Net-(IC13-ANODE)")
  (net 68 "unconnected-(IC8-Pad4)")
  (net 69 "Net-(PI8-PAD)")
  (net 70 "Net-(IC14-ANODE)")
  (net 71 "/3")
  (net 72 "/2")
  (net 73 "/E")
  (net 74 "/4")
  (net 75 "/5")
  (net 76 "/SEND")
  (net 77 "/7")
  (net 78 "/6")
  (net 79 "/9")
  (net 80 "/8")
  (net 81 "/12")
  (net 82 "/11")
  (net 83 "/14")
  (net 84 "/13")
  (net 85 "/16")
  (net 86 "/15")
  (net 87 "Net-(IC15-ANODE)")
  (net 88 "Net-(IC16-ANODE)")
  (net 89 "Net-(ER8-PAD)")
  (net 90 "Net-(ER9-PAD)")
  (net 91 "Net-(ES1-PAD)")
  (net 92 "Net-(ES8-PAD)")
  (net 93 "Net-(ES9-PAD)")
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 185.062 77.5237)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R16" (at -1.27 0.635) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D17-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 136.8115 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S6" (at -3.072139 0) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 82 "/11") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 116.4915 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S5" (at -3.137035 0.017698) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 80 "/8") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 103.6958 77.4208)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R12" (at -1.27 0.635) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D9-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 185.0715 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D17" (at -5.719187 0.020924) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D17-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(D17-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 183.8015 60.4735 -90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES9" (at 1.387752 -0.718844 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(ES9-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO41-3" (layer "F.Cu")
    (at 25.0515 70.6335 90)
    (descr "<b>DO-41 0.3\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D3" (at -0.841785 0.011856 90) (layer "F.SilkS"))
    (fp_text value "1N5817" (at -3.81 2.54 90) (layer "F.Fab"))
    (pad "A" thru_hole circle (at 3.81 0 90) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(V0-PAD)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -3.81 0 90) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 52.9915 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K2" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(K2A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "/4") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(ER2-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "/E") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(ES3-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(ER2-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(K2A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 84.7415 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER4" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(ER4-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 164.6981 77.5599)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R15" (at -1.65393 0.026676) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D15-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 24.772917 79.397722)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 113.9515 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K5" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(K5A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "/8") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(ER5-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "/9") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(ES6-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(ER5-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(K5A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 113.9515 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D10" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(K5A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(K5A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 124.1115 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D11" (at -6.35 0) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D11-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D11-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 172.3715 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R8" (at -3.712714 0.64023) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 85 "/16") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 98.7115 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P4" (at 1.27 0 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(P4-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 103.7915 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC4" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(K4A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(K4A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(IC4-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 64 "Net-(IC12-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(P4-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D9-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 185.0715 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC8" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(K8A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(K8A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(IC8-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 88 "Net-(IC16-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(PI8-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D17-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 44.1015 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER2" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(ER2-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 42.8493 77.357)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R9" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at 207.5689 -2.7636 180) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 83.4715 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC3" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(K3A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(K3A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(IC3-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 61 "Net-(IC11-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(P3-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D7-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 32.6715 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K1" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(K1A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "/2") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(ER1-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "/3") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "/N$5") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(ER1-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(K1A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 174.9115 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D16" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(K8A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(K8A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 63.1233 77.4815)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R10" (at -1.27 0.635) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D5-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 157.1315 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S7" (at -3.30786 -0.007323) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 84 "/13") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 122.8415 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES6" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(ES6-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 124.1115 77.2071)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R13" (at -1.671715 0.062341) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D11-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 179.9915 80.7935)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "PI8" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 69 "Net-(PI8-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 131.7315 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R6" (at -3.256605 0.637161) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 81 "/12") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 23.7815 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER1" (at 0 5.08 -90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(ER1-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 152.0515 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R7" (at -3.304973 0.610613) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 83 "/14") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 91.0915 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R4" (at -3.167704 0.694987) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 77 "/7") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 102.5215 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES5" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(ES5-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 35.2115 60.4735 -90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S1" (at 0 1.27 -180) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 72 "/2") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 70.7715 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R3" (at -3.346676 0.66076) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 75 "/5") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 103.7915 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D9" (at -5.08 0) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D9-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D9-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 164.7515 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC7" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(K7A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(K7A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(IC7-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 87 "Net-(IC15-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(P7-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D15-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 21.2415 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES1" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(ES1-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 105.0615 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER5" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(ER5-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 63.1515 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D5" (at -5.08 0) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D5-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D5-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 93.6315 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K4" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(K4A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "/6") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(ER4-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "/7") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(ES5-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(ER4-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(K4A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 144.4315 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D13" (at -6.35 0) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D13-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(D13-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:063_025" (layer "F.Cu")
    (at 18.7015 71.9035 -90)
    (descr "<b>6.3mm diameter, 2.5 mm lead spacing, 0.1\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C1" (at -1.524 2.159 90) (layer "F.SilkS"))
    (fp_text value "063-EU" (at -1.47 4.556 90) (layer "F.Fab") hide)
    (pad "+" thru_hole rect (at -1.27 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "-" thru_hole circle (at 1.27 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 119.0315 80.7935)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P5" (at 0 -1.27 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(P5-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 75.8515 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S3" (at -3.127983 -0.013376) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 76 "/SEND") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 78.3915 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P3" (at 1.27 0 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(P3-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 190.1515 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "OUT0" (at -1.777893 4.187387 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(ER9-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 143.1615 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES7" (at 0 5.08 -90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(ES7-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 154.5915 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D14" (at -1.2954 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(K7A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(K7A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 177.4515 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S8" (at -3.31257 -0.047601) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 86 "/15") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 124.1115 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC5" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(K5A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(K5A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(IC5-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 67 "Net-(IC13-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(P5-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D11-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 17.4315 66.8235)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "V0" (at 1.27 0.635) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(V0-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 50.4515 60.4735 180)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R2" (at 1.061937 -0.672559) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 73 "/E") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 30.1315 60.4735 -90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R1" (at 0.668236 1.27) (layer "F.SilkS"))
    (fp_text value "PAD" (at -6.35 -1.27 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 71 "/3") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 159.6715 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P7" (at 1.27 0 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 66 "Net-(P7-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 83.4715 77.2071)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R11" (at -1.587327 -0.057615) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D7-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 52.9915 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D4" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(K2A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(K2A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 83.4715 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D7" (at -5.08 0 180) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D7-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D7-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 58.0715 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P2" (at 1.27 0 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(P2-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 42.8315 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC1" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(K1A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(K1A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(IC1-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(IC9-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(P1-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 73.3115 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D6" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(K3A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(K3A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 42.8315 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D2" (at -5.08 0 180) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D2-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 154.5915 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K7" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(K7A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "/13") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(ER7-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "/14") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(ES8-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(ER7-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(K7A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 111.4115 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R5" (at -3.318551 0.690258 180) (layer "F.SilkS"))
    (fp_text value "PAD" (at 123.7489 8.6664) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 79 "/9") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 82.2015 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES4" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(ES4-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 17.4315 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "I0" (at 0 3.175 -90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 91 "Net-(ES1-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 61.8815 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES3" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(ES3-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 96.1715 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S4" (at -3.244805 0.010628) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 78 "/6") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 73.3115 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K3" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(K3A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 76 "/SEND") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(ER3-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "/5") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(ES4-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(ER3-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(K3A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 139.3515 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P6" (at 1.27 0 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(P6-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 19.231598 63.669461)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 134.2715 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D12" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(K6A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(K6A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 17.4315 76.9835)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "G0" (at 1.27 0.635) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 134.2715 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K6" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(K6A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "/11") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(ER6-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "/12") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(ES7-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(ER6-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(K6A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 166.0215 60.4735 -90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER8" (at 1.766902 -0.701582 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(ER8-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:LED3MM" (layer "F.Cu")
    (at 164.7515 80.7935 180)
    (descr "<B>LED</B><p>\n3 mm, round")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D15" (at -6.35 0) (layer "F.SilkS"))
    (fp_text value "LED3MM" (at 1.905 1.651) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at -1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D15-PadA)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "K" thru_hole rect (at 1.27 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D15-C)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 144.4315 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC6" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(K6A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(K6A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(IC6-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 70 "Net-(IC14-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 63 "Net-(P6-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D13-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 37.7515 80.7935 90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "P1" (at 1.27 0 270) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(P1-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 186.3415 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER9" (at 0.714323 4.530899 -90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 90 "Net-(ER9-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 93.6315 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D8" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(K4A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(K4A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 163.4815 60.4735 -90)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES8" (at 1.831019 -0.657194 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 270) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 92 "Net-(ES8-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SOCKED-08" (layer "F.Cu")
    (at 63.1515 70.6335 -90)
    (descr "<b>Dual In Line Socket</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC2" (at -2.921 -0.381 90) (layer "F.SilkS"))
    (fp_text value "DIL8S" (at -3.302 2.032 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at -1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(K2A-+)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 1.27 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(K2A--)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 3.81 3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(IC2-Pad4)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(IC10-ANODE)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(P2-PAD)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at -1.27 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D5-PadA)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at -3.81 -3.81) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:NA" (layer "F.Cu")
    (at 174.9115 70.6335 90)
    (descr "<b>RELAY</b><p>\ndummy")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "K8" (at -6.35 0 90) (layer "F.SilkS"))
    (fp_text value "NA" (at -2.54 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -6.35 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(K8A-+)") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "3" thru_hole oval (at -1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "4" thru_hole oval (at 1.27 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "/15") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 3.81 2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(ER8-PAD)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "8" thru_hole oval (at 3.81 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "/16") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "9" thru_hole oval (at 1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "Net-(ES9-PAD)") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "10" thru_hole oval (at -1.27 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "Net-(ER8-PAD)") (pinfunction "O") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "12" thru_hole oval (at -6.35 -2.54 180) (size 2.616 1.308) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(K8A--)") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 55.5315 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "S2" (at -3.279641 0.026548) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 74 "/4") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 181.174717 62.874454)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "pidal-relay:R0207_3" (layer "F.Cu")
    (at 144.4284 77.2754)
    (descr "<b>RESISTOR</b><br>\n<br>\nlength: 6mm<br>\nformat: 0.1\" (perfboard)<br>\nspacing: 3 holes\n\n<p>This length resistor applies to 1/4 watt metal film.")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "R14" (at -1.27 0.635) (layer "F.SilkS"))
    (fp_text value "6MM-EU" (at -1.27 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(D13-C)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 3.81 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 64.4215 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER3" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(ER3-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 145.7015 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER7" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(ER7-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:DO35-2" (layer "F.Cu")
    (at 32.6715 79.5235 180)
    (descr "<b>DO-35 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D1" (at -1.27 0) (layer "F.SilkS"))
    (fp_text value "1N4148-2" (at -2.286 2.667) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(K1A--)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(K1A-+)") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 125.3815 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ER6" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(ER6-PAD)") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-relay:SQUARE" (layer "F.Cu")
    (at 41.5615 60.4735)
    (descr "<b>Square Pad</b>\n<ul><li>drill diameter 0.7 mm</li></ul>")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "ES2" (at 0 5.08 90) (layer "F.SilkS"))
    (fp_text value "PAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.208 1.208) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 43 "/N$5") (pinfunction "PAD") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 124.1115 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC13" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "Net-(IC13-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "Net-(ES6-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 164.7515 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC15" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "Net-(IC15-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "Net-(ES8-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 103.7915 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC12" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "Net-(IC12-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "Net-(ES5-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 42.8315 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC9" (at 0 0 270) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 270) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "Net-(IC9-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "/N$5") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 144.4315 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC14" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "Net-(IC14-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "Net-(ES7-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 63.1515 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC10" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "Net-(IC10-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(ES3-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 83.4715 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC11" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "Net-(IC11-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "Net-(ES4-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOP254P1000X425-4N" (layer "B.Cu")
    (at 185.0715 69.3635 90)
    (descr "TLP240 MODEL LF1")
    (tags "Integrated Circuit")
    (property "Height" "4.25")
    (property "Manufacturer_Name" "Toshiba")
    (property "Manufacturer_Part_Number" "TLP240A(TP1,F")
    (property "Mouser Part Number" "757-TLP240ATP1F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP240ATP1F?qs=u4fy%2FsgLU9P9ySxW9yuUkw%3D%3D")
    (property "Sheetfile" "pidal-relay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "MOSFET Output Optocouplers Photo IC 3mA 60V 5000Vrms")
    (attr smd)
    (fp_text reference "IC16" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "TLP240A_TP1,F" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "Net-(IC16-ANODE)") (pinfunction "ANODE") (pintype "passive"))
    (pad "2" smd rect (at -4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "CATHODE") (pintype "passive"))
    (pad "3" smd rect (at 4.5 -1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "DRAIN_1") (pintype "passive"))
    (pad "4" smd rect (at 4.5 1.27) (size 1.5 1.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "Net-(ES9-PAD)") (pinfunction "DRAIN_2") (pintype "passive"))
    (model "TLP240A_TP1,F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 191.4215 58.9495) (end 15.6026 58.9495)
    (layer "Edge.Cuts"))
  (gr_line (start 191.4215 83.3335) (end 191.4215 58.9495)
    (layer "Edge.Cuts"))
  (gr_line (start 15.6026 58.9495) (end 15.6026 83.3335)
    (layer "Edge.Cuts"))
  (gr_line (start 15.6026 83.3335) (end 191.4215 83.3335)
    (layer "Edge.Cuts"))
  (gr_text "Raspberry PiDal Switcher RB" (at 32.91722 82.82984) (layer "B.SilkS"))
  (gr_text "by Toni Wren" (at 23.954621 80.881449) (layer "B.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (name "stitch_zone_1") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15.9075 59.2035)
        (xy 191.1675 59.2035)
        (xy 191.1675 83.0795)
        (xy 15.9075 83.0795)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (name "stitch_zone_0") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 15.9075 59.2035)
        (xy 191.1675 59.2035)
        (xy 191.1675 83.0795)
        (xy 15.9075 83.0795)
      )
    )
  )
)
