<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="21.5" x2="0" y2="0.5" width="0" layer="20"/>
<wire x1="0" y1="0.5" x2="0.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.5" y1="0" x2="34.5" y2="0" width="0" layer="20"/>
<wire x1="34.5" y1="0" x2="35" y2="0.5" width="0" layer="20" curve="90"/>
<wire x1="35" y1="0.5" x2="35" y2="33.75" width="0" layer="20"/>
<wire x1="35" y1="33.75" x2="34" y2="35" width="0" layer="20" curve="90"/>
<wire x1="34" y1="35" x2="1" y2="35" width="0" layer="20"/>
<wire x1="1" y1="35" x2="0" y2="34" width="0" layer="20" curve="90"/>
<wire x1="0" y1="34" x2="0" y2="31" width="0" layer="20"/>
<wire x1="0" y1="31" x2="0.5" y2="30.5" width="0" layer="20" curve="90"/>
<wire x1="0.5" y1="30.5" x2="0.75" y2="30.5" width="0" layer="20"/>
<wire x1="0.75" y1="30.5" x2="1.25" y2="30" width="0" layer="20" curve="-90"/>
<wire x1="1.25" y1="30" x2="1.25" y2="22.5" width="0" layer="20"/>
<wire x1="1.25" y1="22.5" x2="0.75" y2="22" width="0" layer="20" curve="-90"/>
<wire x1="0.75" y1="22" x2="0.5" y2="22" width="0" layer="20"/>
<wire x1="0.5" y1="22" x2="0" y2="21.5" width="0" layer="20" curve="90"/>
<text>JAW 2018-07</text>
<text>www.amiketo.com</text>
<text>AMIKETO/3 Rev. 0</text>
<text>Pb</text>
<text>buttons:
BT0 RST</text>
<text>prog</text>
<text>JAW 2018-07</text>
<text>AMIKETO/3DPY</text>
<text>X</text>
<text>Y</text>
<text>L</text>
</plain>
<libraries>
<library name="jaw">
<packages>
<package name="SMD0603">
</package>
<package name="HEADER-5X2-PTH">
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="SMD0805D">
</package>
<package name="SMD1206">
</package>
<package name="SMD0603D">
</package>
<package name="SC-70-3">
</package>
<package name="PUI-0540">
</package>
<package name="KMR211">
</package>
<package name="ROBOTMAN-LOGO2">
</package>
<package name="UQPFN48">
</package>
<package name="SOT-23-3@1">
</package>
<package name="RESONATOR-CSTCE">
</package>
<package name="HEADER-3X2-POGO">
</package>
<package name="M05-1X30-FPC">
<description>&lt;b&gt;30-Pin 0.5mm FPC&lt;/b&gt; Top+Bottom - OMRON - XF2M-3015-1A</description>
</package>
<package name="LGA14A">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="Sparkfun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="CONN_USB_MICRO-B">
<description>USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3" library="adafruit" package="JST-PH-2-SMT-RA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONN1" library="jaw" package="HEADER-5X2-PTH" value="HEADER-5X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="jaw" package="SOD-323" value="any">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="jaw" package="SMD0805D" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="jaw" package="SMD1206" value="750mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="white">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="Sparkfun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="Q1" library="jaw" package="SC-70-3" value="IRLML6344TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="jaw" package="SMD0603" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="jaw" package="SMD0603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPKR1" library="jaw" package="PUI-0540" value="SPKR-PUI-0540">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="SW3" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$4" library="jaw" package="ROBOTMAN-LOGO2" value="ROBOTMAN-LOGO2"/>
<element name="U1" library="jaw" package="UQPFN48" value="STM32F411/48">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="dp_devices" package="CONN_USB_MICRO-B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="jaw" package="SOT-23-3@1" value="mcp1700 /3v3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="jaw" package="RESONATOR-CSTCE" value="12MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="jaw" package="HEADER-3X2-POGO" value="DO NOT PLACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="Sparkfun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="CONN2" library="jaw" package="M05-1X30-FPC" value="HEADER-30X1-XF2M">
<attribute name="NAME"/>
</element>
<element name="C3" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0603" value="600k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
</element>
<element name="D4" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
</element>
<element name="C6" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="microbuilder" package="SOT23-5" value="FAN5331SX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD0603" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
</element>
<element name="C12" library="jaw" package="SMD0603" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="jaw" package="LGA14A" value="LSM6DS3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jaw" package="SMD0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="C15" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="VR1" pad="1"/>
<contactref element="CN3" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C14" pad="2"/>
<contactref element="USB1" pad="P4"/>
<contactref element="USB1" pad="P5"/>
<contactref element="U1" pad="P23"/>
<contactref element="U1" pad="P35"/>
<contactref element="U1" pad="P47"/>
<contactref element="U1" pad="PAD"/>
<contactref element="U1" pad="P8"/>
<contactref element="U1" pad="P20"/>
<contactref element="CONN1" pad="8"/>
<contactref element="CN2" pad="2"/>
<contactref element="CONN2" pad="30"/>
<contactref element="CONN2" pad="28"/>
<contactref element="CONN2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="D4" pad="C"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="CONN2" pad="17"/>
<contactref element="CONN2" pad="18"/>
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U7" pad="7"/>
<contactref element="U7" pad="6"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R5" pad="2"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW3" pad="3"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="VR1" pad="2"/>
<contactref element="U1" pad="P24"/>
<contactref element="U1" pad="P36"/>
<contactref element="U1" pad="P48"/>
<contactref element="R3" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="U1" pad="P9"/>
<contactref element="U1" pad="P1"/>
<contactref element="C14" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="SPKR1" pad="P1"/>
<contactref element="CONN1" pad="1"/>
<contactref element="CONN2" pad="27"/>
<contactref element="CONN2" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="4"/>
<contactref element="L1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U7" pad="8"/>
<contactref element="U7" pad="5"/>
<contactref element="U7" pad="12"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="BOOT0">
<contactref element="SW3" pad="2"/>
<contactref element="SW3" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="P44"/>
<contactref element="U1" pad="P2"/>
<contactref element="CN2" pad="5"/>
</signal>
<signal name="NRST">
<contactref element="C15" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW2" pad="4"/>
<contactref element="U1" pad="P7"/>
<contactref element="CN2" pad="6"/>
</signal>
<signal name="VUSB">
<contactref element="USB1" pad="P1"/>
<contactref element="F1" pad="1"/>
<contactref element="CN2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="P5"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="P6"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="P22"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="USBDM">
<contactref element="U1" pad="P32"/>
<contactref element="USB1" pad="P2"/>
</signal>
<signal name="USBDP">
<contactref element="U1" pad="P33"/>
<contactref element="USB1" pad="P3"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="SPKR1" pad="P2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="IOB9">
<contactref element="U1" pad="P46"/>
<contactref element="Q1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="IOB8">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="P45"/>
</signal>
<signal name="SPISCK">
<contactref element="U1" pad="P26"/>
<contactref element="CONN1" pad="4"/>
</signal>
<signal name="SPIMISO">
<contactref element="U1" pad="P27"/>
<contactref element="CONN1" pad="3"/>
</signal>
<signal name="SPIMOSI">
<contactref element="U1" pad="P28"/>
<contactref element="CONN1" pad="5"/>
</signal>
<signal name="SDCS">
<contactref element="U1" pad="P29"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="VBAT">
<contactref element="CN3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="VR1" pad="3"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="I2CCL">
<contactref element="U1" pad="P42"/>
<contactref element="R3" pad="1"/>
<contactref element="CONN1" pad="9"/>
<contactref element="U7" pad="13"/>
</signal>
<signal name="I2CDA">
<contactref element="U1" pad="P43"/>
<contactref element="R9" pad="1"/>
<contactref element="CONN1" pad="10"/>
<contactref element="U7" pad="14"/>
</signal>
<signal name="DPYDC">
<contactref element="U1" pad="P21"/>
<contactref element="CONN1" pad="6"/>
</signal>
<signal name="DPYCS">
<contactref element="U1" pad="P25"/>
<contactref element="CONN1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="P30"/>
<contactref element="CN2" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="P31"/>
<contactref element="CN2" pad="3"/>
</signal>
<signal name="SWDIO">
<contactref element="U1" pad="P34"/>
</signal>
<signal name="SWDCK">
<contactref element="U1" pad="P37"/>
</signal>
<signal name="PWREN">
<contactref element="U1" pad="P41"/>
</signal>
<signal name="N$24">
<contactref element="F1" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="NRST2">
<contactref element="CONN1" pad="2"/>
<contactref element="U1" pad="P39"/>
</signal>
<signal name="SPI1SCK">
<contactref element="U1" pad="P15"/>
<contactref element="CONN2" pad="14"/>
</signal>
<signal name="SPI1MISO">
<contactref element="U1" pad="P16"/>
</signal>
<signal name="SPI1MOSI">
<contactref element="U1" pad="P17"/>
<contactref element="CONN2" pad="13"/>
</signal>
<signal name="V13">
<contactref element="CONN2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D5" pad="C"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="CONN2" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="CONN2" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="DPY1CS">
<contactref element="CONN2" pad="19"/>
<contactref element="U1" pad="P14"/>
</signal>
<signal name="DPY1DC">
<contactref element="CONN2" pad="20"/>
<contactref element="U1" pad="P13"/>
</signal>
<signal name="NRST3">
<contactref element="CONN2" pad="21"/>
<contactref element="U1" pad="P12"/>
</signal>
<signal name="N$26">
<contactref element="CONN2" pad="22"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="CONN2" pad="26"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="U3" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$1">
<contactref element="U1" pad="P19"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="P11"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="P18"/>
</signal>
<signal name="N$6">
</signal>
</signals>
</board>
</drawing>
</eagle>
