<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="104.1275" y2="0" width="0" layer="20"/>
<wire x1="104.1275" y1="0" x2="104.1275" y2="84.7625" width="0" layer="20"/>
<wire x1="104.1275" y1="84.7625" x2="0" y2="84.7625" width="0" layer="20"/>
<wire x1="0" y1="84.7625" x2="0" y2="0" width="0" layer="20"/>
<text>SR1</text>
<text>MCLK</text>
<text>CBLNK</text>
<text>VCC</text>
<text>GND</text>
<text>VID.
OUT</text>
<text>!W</text>
<text>D0</text>
<text>Inty Video
Overlay 1.4
17 JUL 2017</text>
<text>D1</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>CLK
OUT</text>
<text>X4</text>
<text>X2</text>
<text>X1</text>
<text>D8</text>
<text>PIXEL</text>
<text>ENABLED</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CAP-PTH-SMALL">
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory-idt">
<description>&lt;b&gt;IDT Memories&lt;/b&gt;&lt;p&gt;
Integrated Device Technology, Inc.&lt;p&gt;
http://www.idt.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PLCC-S32--SOCKET">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socket</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC8" library="maxim" package="DIL08" value="MAX913CPA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k"/>
<element name="R10" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="AXIAL-0.4" value="330k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="texas" package="DIL16" value="CD74HCT7046A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="5.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="100pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="AXIAL-0.4" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="470nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="68pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="40xx" package="DIL16" value="4040N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74xx-us" package="DIL14" value="74LS73N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="40xx" package="DIL16" value="4040N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC16" library="74xx-us" package="DIL14" value="74ALS11N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="memory-idt" package="PLCC-S32--SOCKET" value="IDT7205">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC5" library="74xx-us" package="DIL14" value="74S74N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="820">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="74xx-us" package="DIL16" value="74151N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="74xx-us" package="DIL16" value="74S133N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC12" library="74xx-us" package="DIL16" value="74S133N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC13" library="74xx-us" package="DIL14" value="7404N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC14" library="74xx-us" package="DIL14" value="7404N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC15" library="74xx-us" package="DIL16" value="74S133N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC17" library="74xx-us" package="DIL16" value="74S133N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC18" library="74xx-us" package="DIL14" value="7404N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="74xx-us" package="DIL14" value="74AS08N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-25V" value="470uF 25V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-25V" value="470uF 25V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-25V" value="470uF 25V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC1" library="74xx-us" package="DIL14" value="74LS32N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="330pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="470pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="330pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="TO92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="470nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="4.7pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="470nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.4" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.4" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="470nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="330pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="AXIAL-0.4" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="AXIAL-0.4" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="AXIAL-0.4" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="68pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="CBLNK">
<contactref element="IC3" pad="10"/>
<contactref element="IC9" pad="11"/>
<contactref element="IC14" pad="3"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="MCLK">
<contactref element="C1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="P$2"/>
<contactref element="R10" pad="P$2"/>
<contactref element="R13" pad="P$2"/>
<contactref element="U$4" pad="16"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC9" pad="16"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC11" pad="32"/>
<contactref element="IC11" pad="26"/>
<contactref element="IC5" pad="14"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC4" pad="14"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC7" pad="16"/>
<contactref element="IC12" pad="16"/>
<contactref element="IC13" pad="14"/>
<contactref element="IC14" pad="14"/>
<contactref element="IC12" pad="12"/>
<contactref element="IC15" pad="16"/>
<contactref element="IC17" pad="16"/>
<contactref element="IC18" pad="14"/>
<contactref element="IC16" pad="14"/>
<contactref element="IC17" pad="11"/>
<contactref element="IC15" pad="10"/>
<contactref element="IC15" pad="11"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC10" pad="14"/>
<contactref element="IC14" pad="13"/>
<contactref element="IC14" pad="11"/>
<contactref element="C6" pad="+"/>
<contactref element="IC17" pad="14"/>
<contactref element="IC17" pad="15"/>
<contactref element="IC17" pad="13"/>
<contactref element="IC12" pad="15"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC7" pad="13"/>
<contactref element="IC12" pad="14"/>
<contactref element="IC15" pad="2"/>
<contactref element="IC15" pad="3"/>
<contactref element="IC15" pad="5"/>
<contactref element="C7" pad="+"/>
<contactref element="C8" pad="+"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC5" pad="13"/>
<contactref element="IC1" pad="14"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="IC8" pad="3"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R10" pad="P$1"/>
<contactref element="R11" pad="P$2"/>
<contactref element="IC8" pad="2"/>
<contactref element="R14" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U$4" pad="11"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="C1A">
<contactref element="U$4" pad="6"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="C1B">
<contactref element="C2" pad="1"/>
<contactref element="U$4" pad="7"/>
</signal>
<signal name="PC2_OUT">
<contactref element="U$4" pad="13"/>
<contactref element="R15" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="R15" pad="P$2"/>
<contactref element="C4" pad="1"/>
<contactref element="U$4" pad="9"/>
</signal>
<signal name="CLD">
<contactref element="U$4" pad="15"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="MCLK_X4">
<contactref element="IC5" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="R27" pad="P$2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="MCLK_X1">
<contactref element="U$4" pad="3"/>
<contactref element="IC5" pad="9"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="MCLK_SQ3V3">
<contactref element="R13" pad="P$1"/>
<contactref element="R14" pad="P$2"/>
<contactref element="IC8" pad="7"/>
<contactref element="U$4" pad="14"/>
</signal>
<signal name="GND">
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="6"/>
<contactref element="U$4" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="U$4" pad="5"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R11" pad="P$1"/>
<contactref element="IC8" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC4" pad="11"/>
<contactref element="IC9" pad="8"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC11" pad="16"/>
<contactref element="IC11" pad="8"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC4" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC13" pad="7"/>
<contactref element="IC14" pad="7"/>
<contactref element="IC15" pad="8"/>
<contactref element="IC17" pad="8"/>
<contactref element="IC18" pad="7"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC16" pad="7"/>
<contactref element="IC10" pad="7"/>
<contactref element="C6" pad="-"/>
<contactref element="C7" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC1" pad="13"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="R7" pad="P$1"/>
<contactref element="R16" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R28" pad="P$1"/>
</signal>
<signal name="HENABL">
<contactref element="IC4" pad="12"/>
<contactref element="IC16" pad="9"/>
</signal>
<signal name="VENABL">
<contactref element="IC4" pad="9"/>
<contactref element="IC16" pad="11"/>
</signal>
<signal name="D0">
<contactref element="IC11" pad="7"/>
<contactref element="R18" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="!SR1">
<contactref element="IC3" pad="11"/>
<contactref element="IC14" pad="6"/>
</signal>
<signal name="SR1">
<contactref element="IC16" pad="10"/>
<contactref element="IC11" pad="25"/>
<contactref element="IC14" pad="5"/>
<contactref element="JP3" pad="3"/>
<contactref element="IC10" pad="12"/>
</signal>
<signal name="N$16">
<contactref element="R1" pad="P$2"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="!W">
<contactref element="IC11" pad="2"/>
<contactref element="R17" pad="P$2"/>
</signal>
<signal name="D1">
<contactref element="IC11" pad="6"/>
<contactref element="R19" pad="P$2"/>
</signal>
<signal name="D2">
<contactref element="IC11" pad="5"/>
<contactref element="R20" pad="P$2"/>
</signal>
<signal name="D3">
<contactref element="IC11" pad="4"/>
<contactref element="R21" pad="P$2"/>
</signal>
<signal name="!H_OFF">
<contactref element="IC12" pad="9"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="HCNT0">
<contactref element="IC9" pad="9"/>
<contactref element="IC13" pad="9"/>
<contactref element="IC2" pad="11"/>
<contactref element="IC16" pad="1"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="HCNT5">
<contactref element="IC9" pad="2"/>
<contactref element="IC7" pad="7"/>
<contactref element="IC12" pad="7"/>
</signal>
<signal name="HCNT1">
<contactref element="IC9" pad="7"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC16" pad="2"/>
<contactref element="IC12" pad="1"/>
<contactref element="IC7" pad="15"/>
</signal>
<signal name="HCNT2">
<contactref element="IC9" pad="6"/>
<contactref element="IC13" pad="3"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="HCNT3">
<contactref element="IC9" pad="5"/>
<contactref element="IC13" pad="5"/>
</signal>
<signal name="HCNT4">
<contactref element="IC9" pad="3"/>
<contactref element="IC13" pad="13"/>
</signal>
<signal name="!HCNT2">
<contactref element="IC13" pad="4"/>
<contactref element="IC16" pad="13"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC12" pad="5"/>
</signal>
<signal name="!HCNT3">
<contactref element="IC13" pad="6"/>
<contactref element="IC12" pad="2"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="!HCNT4">
<contactref element="IC13" pad="12"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC12" pad="6"/>
</signal>
<signal name="HCNT6">
<contactref element="IC9" pad="4"/>
<contactref element="IC13" pad="11"/>
<contactref element="IC12" pad="4"/>
</signal>
<signal name="!HCNT6">
<contactref element="IC13" pad="10"/>
<contactref element="IC7" pad="14"/>
</signal>
<signal name="HCNT7">
<contactref element="IC9" pad="13"/>
<contactref element="IC13" pad="1"/>
</signal>
<signal name="!HCNT7">
<contactref element="IC13" pad="2"/>
<contactref element="IC7" pad="11"/>
<contactref element="IC12" pad="11"/>
<contactref element="IC7" pad="12"/>
</signal>
<signal name="HCNT8">
<contactref element="IC9" pad="12"/>
<contactref element="IC14" pad="1"/>
<contactref element="IC12" pad="13"/>
</signal>
<signal name="!HCNT8">
<contactref element="IC14" pad="2"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="!V_OFF">
<contactref element="IC17" pad="9"/>
<contactref element="IC10" pad="13"/>
</signal>
<signal name="VCNT1">
<contactref element="IC3" pad="7"/>
<contactref element="IC17" pad="2"/>
<contactref element="IC15" pad="15"/>
</signal>
<signal name="VCNT4">
<contactref element="IC3" pad="3"/>
<contactref element="IC17" pad="5"/>
<contactref element="IC15" pad="12"/>
</signal>
<signal name="VCNT5">
<contactref element="IC3" pad="2"/>
<contactref element="IC15" pad="7"/>
<contactref element="IC17" pad="10"/>
</signal>
<signal name="VCNT0">
<contactref element="IC3" pad="9"/>
<contactref element="IC18" pad="9"/>
</signal>
<signal name="!VCNT0">
<contactref element="IC18" pad="8"/>
<contactref element="IC15" pad="1"/>
<contactref element="IC17" pad="1"/>
</signal>
<signal name="VCNT2">
<contactref element="IC3" pad="6"/>
<contactref element="IC18" pad="11"/>
</signal>
<signal name="!VCNT2">
<contactref element="IC18" pad="10"/>
<contactref element="IC17" pad="3"/>
<contactref element="IC15" pad="14"/>
</signal>
<signal name="VCNT3">
<contactref element="IC3" pad="5"/>
<contactref element="IC18" pad="5"/>
</signal>
<signal name="!VCNT3">
<contactref element="IC18" pad="6"/>
<contactref element="IC17" pad="4"/>
<contactref element="IC15" pad="13"/>
</signal>
<signal name="VCNT6">
<contactref element="IC3" pad="4"/>
<contactref element="IC18" pad="1"/>
<contactref element="IC17" pad="7"/>
</signal>
<signal name="!VCNT6">
<contactref element="IC18" pad="2"/>
<contactref element="IC15" pad="6"/>
</signal>
<signal name="VCNT7">
<contactref element="IC3" pad="13"/>
<contactref element="IC18" pad="3"/>
<contactref element="IC17" pad="12"/>
</signal>
<signal name="!VCNT7">
<contactref element="IC18" pad="4"/>
<contactref element="IC15" pad="4"/>
</signal>
<signal name="V_ON">
<contactref element="IC4" pad="5"/>
<contactref element="IC15" pad="9"/>
</signal>
<signal name="VIDENABL">
<contactref element="IC16" pad="8"/>
<contactref element="IC10" pad="9"/>
<contactref element="IC10" pad="5"/>
<contactref element="JP5" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="D4">
<contactref element="IC11" pad="31"/>
<contactref element="R22" pad="P$2"/>
</signal>
<signal name="D5">
<contactref element="IC11" pad="30"/>
<contactref element="R23" pad="P$2"/>
</signal>
<signal name="D6">
<contactref element="IC11" pad="29"/>
<contactref element="R24" pad="P$2"/>
</signal>
<signal name="D7">
<contactref element="IC11" pad="28"/>
<contactref element="R25" pad="P$2"/>
</signal>
<signal name="!CBLNK">
<contactref element="IC14" pad="4"/>
<contactref element="IC10" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="IC10" pad="3"/>
<contactref element="IC9" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="IC16" pad="12"/>
<contactref element="IC10" pad="10"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="H_ON">
<contactref element="IC7" pad="9"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="!VCNT8">
<contactref element="IC18" pad="12"/>
<contactref element="IC17" pad="6"/>
</signal>
<signal name="VCNT8">
<contactref element="IC3" pad="12"/>
<contactref element="IC18" pad="13"/>
</signal>
<signal name="R">
<contactref element="IC10" pad="8"/>
<contactref element="IC14" pad="9"/>
</signal>
<signal name="!R">
<contactref element="IC14" pad="8"/>
<contactref element="IC11" pad="18"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="RD3">
<contactref element="IC11" pad="14"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="RD2">
<contactref element="IC11" pad="13"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="RD1">
<contactref element="IC11" pad="11"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="RD0">
<contactref element="IC11" pad="10"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="RD7">
<contactref element="IC11" pad="22"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="RD6">
<contactref element="IC11" pad="21"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="RD5">
<contactref element="IC11" pad="20"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="RD4">
<contactref element="IC11" pad="19"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="PIXEL">
<contactref element="IC2" pad="5"/>
<contactref element="IC10" pad="4"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="V_OFF">
<contactref element="IC4" pad="6"/>
<contactref element="IC10" pad="11"/>
</signal>
<signal name="!HCNT0">
<contactref element="IC13" pad="8"/>
<contactref element="IC12" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="MCLK_X2">
<contactref element="JP4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="R8" pad="P$1"/>
<contactref element="IC10" pad="1"/>
</signal>
<signal name="RD8">
<contactref element="IC11" pad="15"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC16" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC16" pad="4"/>
</signal>
<signal name="VIDEO_OUT">
<contactref element="JP1" pad="3"/>
<contactref element="IC16" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="IC16" pad="5"/>
<contactref element="IC10" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="IC11" pad="3"/>
<contactref element="R26" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="T1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="P$1"/>
<contactref element="T1" pad="1"/>
<contactref element="R6" pad="P$2"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="N$17">
<contactref element="R12" pad="P$2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="C16" pad="2"/>
<contactref element="R16" pad="P$2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="JP2" pad="1"/>
<contactref element="R17" pad="P$1"/>
</signal>
<signal name="N$21">
<contactref element="JP2" pad="2"/>
<contactref element="R18" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="JP2" pad="3"/>
<contactref element="R19" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="JP2" pad="4"/>
<contactref element="R20" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="JP2" pad="7"/>
<contactref element="R23" pad="P$1"/>
</signal>
<signal name="N$25">
<contactref element="JP2" pad="10"/>
<contactref element="R26" pad="P$1"/>
</signal>
<signal name="N$26">
<contactref element="JP2" pad="5"/>
<contactref element="R21" pad="P$1"/>
</signal>
<signal name="N$27">
<contactref element="JP2" pad="6"/>
<contactref element="R22" pad="P$1"/>
</signal>
<signal name="N$28">
<contactref element="JP2" pad="8"/>
<contactref element="R24" pad="P$1"/>
</signal>
<signal name="N$29">
<contactref element="JP2" pad="9"/>
<contactref element="R25" pad="P$1"/>
</signal>
<signal name="N$30">
<contactref element="U$4" pad="4"/>
<contactref element="R27" pad="P$1"/>
</signal>
<signal name="N$31">
<contactref element="C5" pad="1"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="11"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="C17" pad="2"/>
<contactref element="R28" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
