(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 330)
    (zones 0)
    (modules 23)
    (nets 43)
  )
  (page USLetter)
  (title_block
    (title "Didj-Fi NAND")
    (date 2020-05-25)
    (rev v1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.889 9.525)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Didj-Fi_NAND/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /DAT1)
  (net 4 /DAT0)
  (net 5 /CLK)
  (net 6 /CMD)
  (net 7 /DAT3)
  (net 8 /DAT2)
  (net 9 /~RST)
  (net 10 "Net-(U2-Pad7)")
  (net 11 /EN)
  (net 12 /D5)
  (net 13 /D6)
  (net 14 /CLE)
  (net 15 /~WE)
  (net 16 /ALE)
  (net 17 /D3)
  (net 18 /~WP)
  (net 19 /D1)
  (net 20 /D2)
  (net 21 /D0)
  (net 22 /D7)
  (net 23 /R_~B)
  (net 24 /~CE)
  (net 25 /D4)
  (net 26 /~RE)
  (net 27 "Net-(JP2-Pad2)")
  (net 28 "Net-(JP1-Pad2)")
  (net 29 /GPIO15)
  (net 30 "Net-(JP3-Pad2)")
  (net 31 "Net-(U2-Pad2)")
  (net 32 "Net-(U2-Pad4)")
  (net 33 "Net-(U2-Pad5)")
  (net 34 "Net-(U2-Pad6)")
  (net 35 "Net-(U2-Pad19)")
  (net 36 "Net-(U2-Pad20)")
  (net 37 "Net-(U2-Pad21)")
  (net 38 "Net-(U2-Pad22)")
  (net 39 /TX)
  (net 40 /RX)
  (net 41 /GPIO2)
  (net 42 /GPIO0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ALE)
    (add_net /CLE)
    (add_net /CLK)
    (add_net /CMD)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DAT0)
    (add_net /DAT1)
    (add_net /DAT2)
    (add_net /DAT3)
    (add_net /EN)
    (add_net /GPIO0)
    (add_net /GPIO15)
    (add_net /GPIO2)
    (add_net /RX)
    (add_net /R_~B)
    (add_net /TX)
    (add_net /~CE)
    (add_net /~RE)
    (add_net /~RST)
    (add_net /~WE)
    (add_net /~WP)
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.05 101.399998 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /GPIO0))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.015 103.399998 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /GPIO2))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:ESP-12E locked (layer F.Cu) (tedit 5ECC6840)
    (at 128.75 96.899998)
    (descr "Wi-Fi Module, http://wiki.ai-thinker.com/_media/esp8266/docs/aithinker_esp_12f_datasheet_en.pdf")
    (tags "Wi-Fi Module")
    (attr smd)
    (fp_text reference U2 (at -10.56 -5.26) (layer F.SilkS) hide)
    (fp_text value ESP-12F (at -0.06 -12.78) (layer F.Fab) hide)
    (fp_text user %R (at 0.49 -0.8) (layer F.Fab))
    (fp_text user "KEEP-OUT ZONE" (at 0.03 -9.55 180) (layer Cmts.User))
    (fp_text user Antenna (at -0.06 -7 180) (layer Cmts.User))
    (pad 22 smd rect (at 7.6 -3.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad22)"))
    (pad 21 smd rect (at 7.6 -1.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad21)"))
    (pad 20 smd rect (at 7.6 0.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad20)"))
    (pad 19 smd rect (at 7.6 2.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad19)"))
    (pad 18 smd rect (at 7.6 4.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 42 /GPIO0))
    (pad 17 smd rect (at 7.6 6.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 41 /GPIO2))
    (pad 16 smd rect (at 7.6 8.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /GPIO15))
    (pad 15 smd rect (at 7.6 10.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 5 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /CLK))
    (pad 13 smd rect (at 3 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /DAT1))
    (pad 12 smd rect (at 1 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /DAT3))
    (pad 11 smd rect (at -1 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAT2))
    (pad 10 smd rect (at -3 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /DAT0))
    (pad 9 smd rect (at -5 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /CMD))
    (pad 8 smd rect (at -7.6 10.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -7.6 8.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -7.6 6.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -7.6 4.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -7.6 2.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -7.6 0.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /EN))
    (pad 2 smd rect (at -7.6 -1.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -7.6 -3.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /~RST))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP-12E.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 157.5 95.149998 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value SD[6] (at 0 1.9 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 27 "Net-(JP2-Pad2)"))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 +3V3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal locked (layer F.Cu) (tedit 5ECC685F)
    (at 141.25 93.899998 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0.5 0 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 4.385 9.89 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.77 3.81 180) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /TX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 121.25 111.899998 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 22u (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.235 98.399998 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 4.7k (at 0 1.17 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(JP3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /D5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.5 105.899998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /GPIO15))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 127.75 112.399998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /DAT2))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module project:didj_cart (layer F.Cu) (tedit 5ECC671E)
    (at 118.1865 115.064498)
    (attr smd)
    (fp_text reference J1 (at 2.032 -12.446) (layer F.SilkS) hide)
    (fp_text value didj_cart (at 3.048 -14.224) (layer F.Fab) hide)
    (fp_text user 30 (at 42.926 4.958) (layer F.SilkS) hide)
    (fp_text user 1 (at 2.032 4.958) (layer F.SilkS) hide)
    (pad 25 connect rect (at 34.58 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 26 /~RE))
    (pad 27 connect rect (at 37.12 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 25 /D4))
    (pad 24 connect rect (at 33.31 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 24 /~CE))
    (pad 26 connect rect (at 35.85 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 23 /R_~B))
    (pad 29 connect rect (at 39.66 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 13 /D6))
    (pad 23 connect rect (at 32.04 5.085) (size 0.889 9.525) (drill (offset 0 0.3125)) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 28 connect rect (at 38.39 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 12 /D5))
    (pad 30 connect rect (at 40.93 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 22 /D7))
    (pad 22 connect rect (at 30.77 5.085) (size 0.889 9.525) (drill (offset 0 0.3125)) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 14 connect rect (at 20.61 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 21 /D0))
    (pad 16 connect rect (at 23.15 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 20 /D2))
    (pad 13 connect rect (at 19.34 5.085) (size 0.889 9.525) (drill (offset 0 0.3125)) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 15 connect rect (at 21.88 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 19 /D1))
    (pad 18 connect rect (at 25.69 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 18 /~WP))
    (pad 12 connect rect (at 18.07 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 39 /TX))
    (pad 17 connect rect (at 24.42 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 17 /D3))
    (pad 20 connect rect (at 28.23 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 16 /ALE))
    (pad 19 connect rect (at 26.96 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 15 /~WE))
    (pad 21 connect rect (at 29.5 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 14 /CLE))
    (pad 11 connect rect (at 16.8 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 40 /RX))
    (pad 10 connect rect (at 15.53 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 3 /DAT1))
    (pad 9 connect rect (at 14.26 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 4 /DAT0))
    (pad 8 connect rect (at 12.99 5.085) (size 0.889 9.525) (drill (offset 0 0.3125)) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 7 connect rect (at 11.72 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 5 /CLK))
    (pad 6 connect rect (at 10.45 5.085) (size 0.889 9.525) (drill (offset 0 0.3125)) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 5 connect rect (at 9.18 5.085) (size 0.889 9.525) (drill (offset 0 0.3175)) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 4 connect rect (at 7.91 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 6 /CMD))
    (pad 3 connect rect (at 6.64 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 7 /DAT3))
    (pad 2 connect rect (at 5.37 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 8 /DAT2))
    (pad 1 connect rect (at 4.1 5.085) (size 0.889 8.89) (layers F.Cu F.Mask)
      (net 11 /EN))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 139.5 105.899998 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.75 112.399998 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 161.25 95.149998 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value SD[7] (at 0 1.9 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 28 "Net-(JP1-Pad2)"))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 +3V3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391EB7)
    (at 153.75 95.149998 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value SD[5] (at 0 1.9 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 30 "Net-(JP3-Pad2)"))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 +3V3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (module project:TSOP48 locked (layer F.Cu) (tedit 5ECC6225)
    (at 151 105.899998 90)
    (attr smd)
    (fp_text reference U1 (at -7.545 -7.022 90) (layer F.SilkS) hide)
    (fp_text value NAND-8BIT (at 0.71 7.022 90) (layer F.Fab) hide)
    (pad 48 smd rect (at -5.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at -5.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at -4.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 45 smd rect (at -4.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at -3.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 22 /D7))
    (pad 43 smd rect (at -3.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 /D6))
    (pad 42 smd rect (at -2.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 /D5))
    (pad 41 smd rect (at -2.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 25 /D4))
    (pad 40 smd rect (at -1.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at -1.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at -0.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at -0.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 36 smd rect (at 0.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 35 smd rect (at 0.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 1.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 1.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 2.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 17 /D3))
    (pad 31 smd rect (at 2.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 20 /D2))
    (pad 30 smd rect (at 3.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 19 /D1))
    (pad 29 smd rect (at 3.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 21 /D0))
    (pad 28 smd rect (at 4.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 5.25 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 5.75 -9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 5.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 5.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 4.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 4.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 3.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 3.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 18 /~WP))
    (pad 18 smd rect (at 2.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 15 /~WE))
    (pad 17 smd rect (at 2.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 16 /ALE))
    (pad 16 smd rect (at 1.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 14 /CLE))
    (pad 15 smd rect (at 1.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -0.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 11 smd rect (at -0.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -1.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -1.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 24 /~CE))
    (pad 8 smd rect (at -2.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 26 /~RE))
    (pad 7 smd rect (at -2.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask)
      (net 23 /R_~B))
    (pad 6 smd rect (at -3.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -3.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.25 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -5.75 9.74 180) (size 1.48 0.28) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.25 105.914998 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0.1u (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 159.75 98.399998 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 4.7k (at 0 1.17 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(JP1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /D7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.985 98.399998 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 4.7k (at 0 1.17 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(JP2-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /D6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.75 112.399998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /DAT0))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.5 112.384998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /~RST))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 123.75 112.414998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 3k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /CMD))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.75 112.399998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /DAT1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.75 112.414998 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /DAT3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 148.9 95.5 90) (layer F.SilkS))
  (gr_text 3.3v (at 146.25 95.5 90) (layer F.SilkS))
  (gr_text TX (at 143.75 95.5 90) (layer F.SilkS))
  (gr_text RX (at 141.25 95.5 90) (layer F.SilkS))
  (gr_text 1 (at 159.25 96.5) (layer F.SilkS))
  (gr_text 0 (at 159.25 94) (layer F.SilkS))
  (gr_text 0 (at 155.5 94) (layer F.SilkS))
  (gr_text 1 (at 155.5 96.5) (layer F.SilkS))
  (gr_text 1 (at 151.75 96.5) (layer F.SilkS))
  (gr_text 0 (at 151.75 94) (layer F.SilkS))
  (gr_text "7 6 5 | Boot mode\n---------------\nX X X | Device default\nX 0 0 | UART\n0 0 1 | Internal NAND\n1 0 1 | Cartridge NAND\nX 1 1 | None (RAM)" (at 162 120.5) (layer B.SilkS))
  (gr_text "Didj-Fi NAND v1.0" (at 140 94.5) (layer B.SilkS))
  (gr_text SD5 (at 153.75 98.25 90) (layer F.SilkS))
  (gr_text SD6 (at 157.5 98.25 90) (layer F.SilkS))
  (gr_text SD7 (at 161.25 98.25 90) (layer F.SilkS))
  (gr_text JLCJLCJLCJLC (at 128.156 99.765998 90) (layer F.SilkS))
  (gr_text jkent.net/w/didjfi (at 136.25 97.25) (layer B.SilkS))
  (gr_text "Didj-Fi NAND v1.0" (at 135 113.5) (layer F.SilkS))
  (gr_line (start 118.25 92.399998) (end 118.25 125.899998) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.15 92.399998) (end 118.25 92.399998) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.15 125.899998) (end 163.15 92.399998) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.25 125.899998) (end 163.15 125.899998) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.25 115.005998) (xy 163.208 115.005998) (xy 163.208 125.927998) (xy 118.25 125.927998)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.1445 92.399998) (xy 163.1445 125.927998) (xy 118.25 125.927998) (xy 118.25 92.399998)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.25 92.399998) (xy 163.1445 92.399998) (xy 163.1445 125.927998) (xy 118.25 125.927998)
      )
    )
  )
)
