<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="13.1" y2="0" width="0" layer="20"/>
<wire x1="13.1" y1="0" x2="13.1" y2="10.4" width="0" layer="20"/>
<wire x1="13.1" y1="10.4" x2="0" y2="10.4" width="0" layer="20"/>
<wire x1="0" y1="10.4" x2="0" y2="0" width="0" layer="20"/>
<text>1</text>
<text>SOIC .150"</text>
<text>SOIC .208"</text>
</plain>
<libraries>
<library name="_hhn_attiny25_45_85">
<description>&lt;h3&gt;ATMEL ATtiny 25 / 45 /48&lt;/h3&gt;
&lt;p&gt;&lt;br /&gt;&lt;b&gt;&lt;u&gt;Supplied Packages:&lt;/u&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;P&lt;/b&gt; &amp;nbsp; = PDIP 08 30mil&lt;br /&gt;
&lt;b&gt;S&lt;/b&gt; &amp;nbsp; = SOIC 08 EIAJ 208mil&lt;br /&gt;
&lt;b&gt;SS&lt;/b&gt; = SOIC 08 JEDEC 150mil&lt;br /&gt;
&lt;b&gt;X&lt;/b&gt;&gt; &amp;nbsp; = TSSOP 08 4.4mm&lt;/p&gt;

&lt;p&gt;&lt;u&gt;&lt;b&gt;Revisions / Changelog&lt;/b&gt;&lt;/u&gt;&lt;br /&gt;
&amp;bull; &amp;nbsp;5.0.0 [EAGLE 5]&lt;br /&gt;
&lt;/p&gt;

&lt;hr /&gt;

&lt;author&gt;
&lt;p&gt;&lt;u&gt;Author:&lt;/u&gt;&lt;br /&gt;
Dipl.-Ing. FH Rainer Bayer&lt;br /&gt;
HHN Hochschule Heilbronn (Heilbronn University), &lt;i&gt;rainer.bayer@hs-heilbronn.de&lt;/i&gt;&lt;br /&gt;
Ingenieurbüro ing-rb, &lt;i&gt;mail@ing-rb.de&lt;/i&gt;&lt;/p&gt;&lt;/author&gt;</description>
<packages>
<package name="SOIC8_EIAJ_208MIL">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
208-mil body</description>
</package>
<package name="SOIC08_JEDEC_150MIL">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="_hhn_attiny25_45_85" package="SOIC8_EIAJ_208MIL" value="ATTINY85V-10S"/>
<element name="U2" library="_hhn_attiny25_45_85" package="SOIC08_JEDEC_150MIL" value="ATTINY25V-10SS"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="8">
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="8"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="4">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="1">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="3">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="2">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="7">
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="7"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="6">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="5">
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="5"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
