(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "BATT+")
  (net 3 "RESET")
  (net 4 "RX")
  (net 5 "TX")
  (net 6 "SDA")
  (net 7 "SCL")
  (net 8 "SWDIO")
  (net 9 "SWDCLK")
  (net 10 "BT1")
  (net 11 "BT2")
  (net 12 "BT3")
  (net 13 "Data5")
  (net 14 "Data4")
  (net 15 "Data3")
  (net 16 "Data2")
  (net 17 "Data1")
  (net 18 "Net-(J1-Pad39)")
  (net 19 "Net-(J1-Pad40)")
  (net 20 "5V")
  (net 21 "unconnected-(D26-Pad1)")
  (net 22 "unconnected-(J1-Pad14)")
  (net 23 "unconnected-(J1-Pad16)")
  (net 24 "unconnected-(J1-Pad18)")
  (net 25 "unconnected-(J1-Pad19)")
  (net 26 "unconnected-(J1-Pad20)")
  (net 27 "unconnected-(J1-Pad21)")
  (net 28 "unconnected-(J1-Pad22)")
  (net 29 "3.3V")
  (net 30 "3.3v_periph")
  (net 31 "Net-(BATT1-Pad1)")
  (net 32 "Net-(BATT2-Pad1)")
  (net 33 "Net-(D1-Pad1)")
  (net 34 "Net-(D1-Pad2)")
  (net 35 "Net-(D6-Pad1)")
  (net 36 "Net-(D6-Pad2)")
  (net 37 "Net-(D7-Pad1)")
  (net 38 "Net-(D7-Pad2)")
  (net 39 "Net-(D8-Pad2)")
  (net 40 "Net-(D8-Pad1)")
  (net 41 "Net-(D9-Pad1)")
  (net 42 "Net-(D9-Pad2)")
  (net 43 "Net-(D10-Pad2)")
  (net 44 "Net-(D10-Pad1)")
  (net 45 "Net-(D11-Pad1)")
  (net 46 "Net-(D11-Pad2)")
  (net 47 "Net-(D12-Pad2)")
  (net 48 "Net-(D12-Pad1)")
  (net 49 "Net-(D13-Pad1)")
  (net 50 "Net-(D13-Pad2)")
  (net 51 "Net-(D14-Pad2)")
  (net 52 "Net-(D14-Pad1)")
  (net 53 "Net-(D15-Pad1)")
  (net 54 "Net-(D15-Pad2)")
  (net 55 "Net-(D16-Pad1)")
  (net 56 "Net-(D16-Pad2)")
  (net 57 "Net-(D17-Pad2)")
  (net 58 "Net-(D17-Pad1)")
  (net 59 "Net-(D18-Pad1)")
  (net 60 "Net-(D18-Pad2)")
  (net 61 "Net-(D19-Pad2)")
  (net 62 "Net-(D19-Pad1)")
  (net 63 "Net-(D20-Pad2)")
  (net 64 "Net-(D20-Pad1)")
  (net 65 "Net-(D21-Pad2)")
  (net 66 "Net-(D21-Pad1)")
  (net 67 "Net-(D1_selector1-Pad1)")
  (net 68 "Net-(D1_selector1-Pad3)")
  (net 69 "DIN")
  (net 70 "unconnected-(J1-Pad24)")
  (net 71 "unconnected-(J1-Pad26)")
  (net 72 "unconnected-(STLINK1-Pad3)")
  (net 73 "unconnected-(STLINK1-Pad5)")
  (net 74 "unconnected-(STLINK1-Pad7)")
  (net 75 "unconnected-(STLINK1-Pad8)")
  (net 76 "unconnected-(STLINK1-Pad9)")
  (net 77 "Net-(J1-Pad28)")
  (net 78 "Net-(J1-Pad30)")
  (net 79 "Net-(J1-Pad32)")
  (net 80 "Net-(J1-Pad34)")
  (net 81 "Net-(J1-Pad36)")
  (net 82 "LED1")
  (net 83 "Net-(D1-Pad3)")
  (net 84 "Net-(D2-Pad1)")
  (net 85 "Net-(D3-Pad1)")
  (net 86 "Net-(D4-Pad1)")
  (net 87 "Net-(D22-Pad3)")
  (net 88 "Net-(D22-Pad1)")
  (net 89 "Net-(D23-Pad1)")
  (net 90 "Net-(D24-Pad1)")
  (net 91 "Net-(D25-Pad1)")
  (net 92 "unconnected-(STLINK1-Pad10)")
  (net 93 "Net-(D27-Pad1)")
  (net 94 "Net-(D27-Pad2)")
  (net 95 "Net-(D28-Pad2)")
  (net 96 "Net-(D28-Pad1)")
  (net 97 "Net-(D29-Pad1)")
  (net 98 "Net-(D29-Pad2)")
  (net 99 "Free3")
  (net 100 "Free2")
  (net 101 "Free1")
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 124.46 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(D22-Pad3)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D4-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 101.6 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 104.14 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 106.68 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 109.22 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D10" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D10-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(D10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 121.92 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(D11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 124.46 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D12" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(D12-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(D12-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 127 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D13-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(D13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 129.54 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D14" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(D14-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(D14-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 132.08 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D15" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(D15-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 137.16)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D16" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(D16-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(D16-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 139.7)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D17" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(D17-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(D17-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 142.24)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D18" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(D18-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(D18-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 144.78)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D19" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(D19-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(D19-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 149.86)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D21" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(D21-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(D21-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 134.62 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D23" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(D23-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D22-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 93.98 99.06)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 12.49) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(D6-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(D7-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "SDA") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(D8-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "TX") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(D9-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "RX") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(D10-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 93.98 137.16)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x06_Odd_Even" (at 1.27 15.03) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad28)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(D16-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad30)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(D17-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad32)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(D18-Pad1)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad34)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(D19-Pad1)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad36)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(D20-Pad1)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "LED1") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(D21-Pad1)") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 99.06 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(D6-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 101.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "3.3k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(D7-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 104.14 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(D8-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 109.22 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(D10-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 121.92 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(D11-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 124.46 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(D12-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 127 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(D13-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 129.54 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(D14-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 132.08 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(D15-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 139.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(D17-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 142.24 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(D18-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 144.78 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(D19-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 147.32 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(D20-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 149.86 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(D21-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 87.63 161.29 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SPKR1" (at 9.398 -2.794 -90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad40)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad39)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_PTS645" (layer "F.Cu")
    (tedit 5A02FC95)
    (at 113.03 158.75 90)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at 0 -4.05 90) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 4.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.05 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "BT2") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "BT2") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at -3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at 3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_PTS645" (layer "F.Cu")
    (tedit 5A02FC95)
    (at 104.14 158.75 90)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at 0 -4.05 90) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 4.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.05 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "BT3") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "BT3") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 147.32)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D20" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(D20-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(D20-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 137.16 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "BATT+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(D16-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 139.7 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D24" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(D24-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(D23-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 114.3 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(D3-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(D2-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 99.06 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 106.68 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(D9-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 133.35 90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BATT1" (at 0 8.89 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 6.985 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.635 5.08 270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(BATT1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 104.14)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "I2C1" (at 6.35 2.54) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "SDA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "SCL") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "3.3v_periph") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 149.86 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D26" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(D26-Pad1)") (pinfunction "DOUT") (pintype "output+no_connect"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(D25-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 104.14 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(D1-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(D1-Pad3)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 144.78 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D25" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(D25-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(D24-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 104.775 95.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.27 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(D1_selector1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 138.43)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 5.08 3.175) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at 6.985 4.445) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(BATT1-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "BATT+") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(BATT2-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 85.09 104.14)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "TestBoardConnector" (at 1.27 50.59) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "BATT+") (pinfunction "BATT+") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "BATT-") (pintype "input"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "5V") (pinfunction "5V") (pintype "input"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "RESET") (pinfunction "RESET") (pintype "input"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "3.3V") (pinfunction "3.3V") (pintype "input"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "RX") (pinfunction "RX1") (pintype "input"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "TX") (pinfunction "TX1") (pintype "input"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "SDA") (pinfunction "SDA") (pintype "input"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "SCL") (pinfunction "SCL") (pintype "input"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "SWDIO") (pinfunction "SWDIO") (pintype "input"))
    (pad "12" thru_hole oval locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "SWDCLK") (pinfunction "SWDCLK") (pintype "input"))
    (pad "13" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "BT1") (pinfunction "BT1") (pintype "input"))
    (pad "14" thru_hole oval locked (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad14)") (pinfunction "U1") (pintype "input+no_connect"))
    (pad "15" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "BT2") (pinfunction "BT2") (pintype "input"))
    (pad "16" thru_hole oval locked (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad16)") (pinfunction "U2") (pintype "input+no_connect"))
    (pad "17" thru_hole oval locked (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "BT3") (pinfunction "BT3") (pintype "input"))
    (pad "18" thru_hole oval locked (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-Pad18)") (pinfunction "U3") (pintype "input+no_connect"))
    (pad "19" thru_hole oval locked (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad19)") (pinfunction "BT4") (pintype "input+no_connect"))
    (pad "20" thru_hole oval locked (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J1-Pad20)") (pinfunction "LED10") (pintype "input+no_connect"))
    (pad "21" thru_hole oval locked (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J1-Pad21)") (pinfunction "BT5") (pintype "input+no_connect"))
    (pad "22" thru_hole oval locked (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J1-Pad22)") (pinfunction "LED9") (pintype "input+no_connect"))
    (pad "23" thru_hole oval locked (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Free3") (pinfunction "BT6") (pintype "input"))
    (pad "24" thru_hole oval locked (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "unconnected-(J1-Pad24)") (pinfunction "LED8") (pintype "input+no_connect"))
    (pad "25" thru_hole oval locked (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Free2") (pinfunction "BT7") (pintype "input"))
    (pad "26" thru_hole oval locked (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "unconnected-(J1-Pad26)") (pinfunction "LED7") (pintype "input+no_connect"))
    (pad "27" thru_hole oval locked (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Free1") (pinfunction "Data6") (pintype "input"))
    (pad "28" thru_hole oval locked (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad28)") (pinfunction "LED6") (pintype "input"))
    (pad "29" thru_hole oval locked (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Data5") (pinfunction "Data5") (pintype "input"))
    (pad "30" thru_hole oval locked (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad30)") (pinfunction "LED5") (pintype "input"))
    (pad "31" thru_hole oval locked (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Data4") (pinfunction "Data4") (pintype "input"))
    (pad "32" thru_hole oval locked (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad32)") (pinfunction "LED4") (pintype "input"))
    (pad "33" thru_hole oval locked (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Data3") (pinfunction "Data3") (pintype "input"))
    (pad "34" thru_hole oval locked (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad34)") (pinfunction "LED3") (pintype "input"))
    (pad "35" thru_hole oval locked (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Data2") (pinfunction "Data2") (pintype "input"))
    (pad "36" thru_hole oval locked (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad36)") (pinfunction "LED2") (pintype "input"))
    (pad "37" thru_hole oval locked (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Data1") (pinfunction "Data1") (pintype "input"))
    (pad "38" thru_hole oval locked (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "LED1") (pinfunction "LED1") (pintype "input"))
    (pad "39" thru_hole oval locked (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad39)") (pinfunction "SP+") (pintype "input"))
    (pad "40" thru_hole oval locked (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad40)") (pinfunction "SP-") (pintype "input"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 88.9)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "3.3v_selector1" (at 5.08 0 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "3.3v_periph") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Data5") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 109.22 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(D2-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(D1-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 119.38 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(D4-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(D3-Pad1)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm" (layer "F.Cu")
    (tedit 5AA4B1EE)
    (at 110.49 129.54 180)
    (descr "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf")
    (tags "LED RGB NeoPixel Nano")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D22" (at 0 -2.2 180) (layer "F.SilkS"))
    (fp_text value "SK6812" (at 0 2.7 180) (layer "F.Fab"))
    (fp_text user "1" (at -2.15 -0.65 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D22-Pad1)") (pinfunction "DOUT") (pintype "output"))
    (pad "2" smd rect locked (at -1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(D1-Pad2)") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at 1 0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(D22-Pad3)") (pinfunction "DIN") (pintype "input"))
    (pad "4" smd rect locked (at 1 -0.65 180) (size 1 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "BATT+") (pinfunction "VDD") (pintype "power_in"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 148.59 -90)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BATT2" (at 1.905 -6.35 -90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 1.27 2.33 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -12.7) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(BATT2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 101.6 152.4 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "LED_SELECT1" (at -18.288 -3.048 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "LED1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(D1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 116.84)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Serial1" (at 6.35 0) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "3.3v_periph") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "TX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_PTS645" (layer "F.Cu")
    (tedit 5A02FC95)
    (at 95.25 158.75 90)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 -4.05 90) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 4.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -4.05 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "BT1") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect locked (at 3.98 -2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "BT1") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect locked (at -3.98 2.25 90) (size 1.55 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 114.3 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D27" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(D27-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(D27-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 116.84 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D28" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(D28-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(D28-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 101.6 119.38 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D29" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(D29-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(D29-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 114.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(D27-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 116.84 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(D28-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 105.41 119.38 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43 180) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 0 1.43 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 180) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(D29-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 93.98 114.3)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Free3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(D27-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Free2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(D28-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Free1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(D29-Pad2)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Data5") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(D11-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Data4") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(D12-Pad2)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Data3") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(D13-Pad2)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Data2") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(D14-Pad2)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Data1") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(D15-Pad2)") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 113.03 92.71 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at -3.175 0 -90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 270) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(D1_selector1-Pad3)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 107.95 100.33 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.54 0 90) (layer "F.SilkS"))
    (fp_text value "330" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(D1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 90) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "DIN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59DE0611)
    (at 96.52 90.17 -90)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "STLINK1" (at 1.27 -3.175 -90) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 16.764 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "RESET") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "SWDCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "unconnected-(STLINK1-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "SWDIO") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "unconnected-(STLINK1-Pad5)") (pinfunction "Pin_5") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "unconnected-(STLINK1-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "unconnected-(STLINK1-Pad8)") (pinfunction "Pin_8") (pintype "passive+no_connect"))
    (pad "9" thru_hole oval locked (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "unconnected-(STLINK1-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" thru_hole oval locked (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 "unconnected-(STLINK1-Pad10)") (pinfunction "Pin_10") (pintype "passive+no_connect"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 105.41 91.44 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1_selector2" (at 6.985 1.27 180) (layer "F.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "BT1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "BT2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "BT3") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 115.57 97.79 -90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/v6_test_rig/v4_autotest2.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1_selector1" (at 1.27 -4.064 -90) (layer "F.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(D1_selector1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Data1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(D1_selector1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Data1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "DIN") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Data1") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 81.28 86.36) (end 118.745 86.36) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 118.745 165.1) (end 118.745 86.36) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.28 86.36) (end 81.28 165.1) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 81.28 165.1) (end 118.11 165.1) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 118.745 165.1) (end 118.11 165.1) (layer "Edge.Cuts") (width 0.15))
  (gr_text "Proffieboard V3 modular breakout board.\nDesigned by Fredrik Hubinette.\nhttps://fredrik.hubbe.net/lightsaber/" (at 104.648 124.6505 90) (layer "B.SilkS"))
  (gr_text "3.3v-P-SD\n" (at 117.856 91.44 90) (layer "F.SilkS"))
  (gr_text "-  +" (at 117.856 149.86 90) (layer "F.SilkS"))
  (gr_text "GND TX RX 3.3v" (at 117.856 120.904 90) (layer "F.SilkS"))
  (gr_text "B1 B2 B3\n" (at 107.95 93.345) (layer "F.SilkS"))
  (gr_text "Data 1-4" (at 99.06 128.905 90) (layer "F.SilkS"))
  (gr_text "SD" (at 99.06 121.92 90) (layer "F.SilkS"))
  (gr_text "GND 3.3v SCL SDA" (at 117.856 108.204 90) (layer "F.SilkS"))
  (gr_text "I2C" (at 113.284 108.204 90) (layer "F.SilkS"))
  (gr_text "PXL PU PD" (at 113.03 95.885) (layer "F.SilkS"))
  (gr_text "LED 1-6" (at 99.06 143.764 90) (layer "F.SilkS"))
  (gr_text "RX TX SDA SCL 5v" (at 99.06 104.14 90) (layer "F.SilkS"))
  (gr_text "FR 1-3\n" (at 99.06 116.84 90) (layer "F.SilkS"))
  (gr_text "D1 select" (at 121.92 98.425 90) (layer "F.SilkS"))
  (gr_text "Serial\n" (at 113.284 120.904 90) (layer "F.SilkS"))
  (gr_text "Speaker" (at 85.852 159.004) (layer "F.SilkS"))
  (gr_text "+ -" (at 86.36 163.576) (layer "F.SilkS"))
  (gr_text "LED1-PXL>" (at 96.012 152.5905) (layer "F.SilkS"))
  (gr_text "+  -" (at 117.856 132.08 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.2 81.28)
        (xy 120.65 81.28)
        (xy 119.38 167.64)
        (xy 76.2 167.64)
      )
    )
  )
)
