(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 60)
    (zones 0)
    (modules 6)
    (nets 13)
  )
  (page USLetter)
  (title_block
    (title NS73M-Breakout)
    (date 2017-05-03)
    (rev 1)
    (company "Conor Peterson")
    (comment 1 conor.p.peterson@gmail.com)
    (comment 2 CC-BY-4.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Gerbers/1.0/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P2-Pad1)")
  (net 3 "Net-(U1-Pad4)")
  (net 4 "Net-(U1-Pad10)")
  (net 5 /VCC)
  (net 6 /TEB)
  (net 7 /CK)
  (net 8 /DA)
  (net 9 /LA)
  (net 10 /I2C)
  (net 11 /RIN)
  (net 12 /LIN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Data ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CK)
    (add_net /DA)
    (add_net /I2C)
    (add_net /LA)
    (add_net /LIN)
    (add_net /RIN)
    (add_net /TEB)
    (add_net "Net-(U1-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.55)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VCC)
    (add_net GND)
  )
  (net_class RF ""
    (clearance 0.25)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P2-Pad1)")
  )
  (net_class Xtal ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad10)")
  )
  (module NS73M-Breakout:NS73M-DFN (layer F.Cu) (tedit 590A0C5F)
    (at 131 95 180)
    (fp_text reference U1 (at 2.65 -4.8 180) (layer F.SilkS))
    (fp_text value NS73M (at 0.15 -4.85 180) (layer F.Fab) hide)
    (pad 1 smd oval (at 3.5 2.8 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd oval (at 3.5 2 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 3 smd oval (at 3.5 1.2 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /TEB))
    (pad 4 smd oval (at 3.5 0.4 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad4)"))
    (pad 5 smd oval (at 3.5 -0.4 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /CK))
    (pad 6 smd oval (at 3.5 -1.2 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /DA))
    (pad 7 smd oval (at 3.5 -2 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /LA))
    (pad 8 smd oval (at 3.5 -2.8 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /I2C))
    (pad 9 smd oval (at -3.5 -2.4 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 10 smd oval (at -3.5 -1.6 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad10)"))
    (pad 11 smd oval (at -3.5 -0.8 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd oval (at -3.5 0 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /LIN))
    (pad 13 smd oval (at -3.5 0.8 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /RIN))
    (pad 14 smd oval (at -3.5 1.6 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd oval (at -3.5 2.5 180) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module Capacitors_SMD:CP_Elec_4x4.5 (layer F.Cu) (tedit 590A0C3C)
    (at 129 87)
    (descr "SMT capacitor, aluminium electrolytic, 4x4.5")
    (attr smd)
    (fp_text reference C1 (at -3.3 -2.45 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 -3.45) (layer F.Fab) hide)
    (fp_text user + (at -1.24 -0.08) (layer F.Fab))
    (fp_text user + (at -2.78 1.99 180) (layer F.SilkS))
    (fp_text user %R (at 3.45 2.15) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /VCC))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Crystals:Crystal_C26-LF_d2.1mm_l6.5mm_Horizontal_1EP_style1 (layer F.Cu) (tedit 590A0C06)
    (at 134.75 103.05 270)
    (descr "Crystal THT C26-LF 6.5mm length 2.06mm diameter")
    (tags ['C26-LF'])
    (fp_text reference Y1 (at -1.2 2.55) (layer F.SilkS))
    (fp_text value "32.768 kHz" (at 3.57 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 1 5.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad10)"))
    (pad 2 thru_hole circle (at 1.9 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.95 5.75 270) (size 2.2 6.5) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_C26-LF_d2.1mm_l6.5mm_Horizontal_1EP_style1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module NS73M-Breakout:pinheader-9x (layer F.Cu) (tedit 590A0C23)
    (at 122 85)
    (fp_text reference P1 (at 2.2 21) (layer F.SilkS) hide)
    (fp_text value HEADER (at -2.54 10.16 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /VCC))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /TEB))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /CK))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DA))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /LA))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /I2C))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /RIN))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /LIN))
  )
  (module NS73M-Breakout:rf_hole (layer F.Cu) (tedit 590A0C44)
    (at 135 85)
    (fp_text reference P2 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value RF_OUT (at 0 -2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.25 96.95)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (gr_text "FM MODULE 1.1" (at 128.35 106.5) (layer F.SilkS))
  (gr_text "CP 17" (at 132.25 93.1 180) (layer B.SilkS))
  (gr_text "RF\n50Ω" (at 134.15 88.7 180) (layer B.SilkS))
  (gr_text "LIN\nRIN\nI2C\nLA\nDA\nCK\nTEB\n+3V\nGND" (at 123.3 95.1 180) (layer B.SilkS))
  (gr_text NS73M (at 132 99.75) (layer F.SilkS))
  (gr_line (start 119.95 107.7) (end 119.95 82.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.95 107.7) (end 119.95 107.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.95 82.7) (end 136.95 107.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.95 82.7) (end 136.95 82.7) (layer Edge.Cuts) (width 0.15))
)
